lloc: s10176 r8192 d14400 u32768 alloc=8*4096

<7>[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 

<4>[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 411136

<5>[    0.000000] Kernel command line: console=ttyS0,115200 rw init=/init loglevel=4 ion_reserve=256M boot_type=0 partitions=bootloader@nanda:env@nandb:boot@nandc:system@nandd:data@nande:misc@nandf:recovery@nandg:cache@nandh:databk@nandi:UDISK@nandj

<6>[    0.000000] PID hash table entries: 2048 (order: 1, 8192 bytes)

<6>[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)

<6>[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)

<6>[    0.000000] Memory: 49MB 1575MB = 1624MB total

<5>[    0.000000] Memory: 1633448k/1633448k available, 463704k reserved, 1318912K highmem

<5>[    0.000000] Virtual kernel memory layout:

<5>[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)

<5>[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)

<5>[    0.000000]     vmalloc : 0xf0000000 - 0xff000000   ( 240 MB)

<5>[    0.000000]     lowmem  : 0xc0000000 - 0xef800000   ( 760 MB)

<5>[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)

<5>[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)

<5>[    0.000000]       .text : 0xc0008000 - 0xc0784000   (7664 kB)

<5>[    0.000000]       .init : 0xc0784000 - 0xc07cb7c0   ( 286 kB)

<5>[    0.000000]       .data : 0xc07cc000 - 0xc0821f70   ( 344 kB)

<5>[    0.000000]        .bss : 0xc0821f94 - 0xc099dbd0   (1520 kB)

<6>[    0.000000] Preemptible hierarchical RCU implementation.

<6>[    0.000000] NR_IRQS:160

<4>[    0.000000] [aw_delay]: It is use use_time_delay function!

<6>[    0.000000] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 178956ms

<6>[    0.000000] Architected local timer running at 24.00MHz.

<6>[    0.000000] Console: colour dummy device 80x30

<6>[    0.000433] Calibrating delay loop... 2013.59 BogoMIPS (lpj=10067968)

<6>[    0.059952] pid_max: default: 32768 minimum: 301

<6>[    0.060304] Mount-cache hash table entries: 512

<6>[    0.061027] CPU: Testing write buffer coherency: ok

<6>[    0.061074] ftrace: allocating 20628 entries in 61 pages

<6>[    0.097493] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000

<6>[    0.097571] Setting up static identity map for 0x4058cb18 - 0x4058cb70

<4>[    0.224706] CPU1: Booted secondary processor

<6>[    0.277842] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001

<4>[    0.344836] CPU2: Booted secondary processor

<6>[    0.398011] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002

<4>[    0.465029] CPU3: Booted secondary processor

<6>[    0.518177] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003

<6>[    0.518270] Brought up 4 CPUs

<6>[    0.518285] SMP: Total of 4 processors activated (8054.37 BogoMIPS).

<6>[    0.519345] devtmpfs: initialized

<4>[    0.524769] script_init enter!

<4>[    0.525505] script_init exit!

<6>[    0.527155] print_constraints: dummy: 

<6>[    0.527642] NET: Registered protocol family 16

<7>[    0.527848] sunxi_dump_init success

<6>[    0.528125] script_sysfs_init success

<6>[    0.532834] gpiochip_add: registered GPIOs 0 to 27 on device: GPA

<6>[    0.533046] gpiochip_add: registered GPIOs 30 to 37 on device: GPB

<6>[    0.533247] gpiochip_add: registered GPIOs 40 to 67 on device: GPC

<6>[    0.533456] gpiochip_add: registered GPIOs 70 to 97 on device: GPD

<6>[    0.533671] gpiochip_add: registered GPIOs 100 to 116 on device: GPE

<6>[    0.533874] gpiochip_add: registered GPIOs 119 to 124 on device: GPF

<6>[    0.534082] gpiochip_add: registered GPIOs 127 to 145 on device: GPG

<6>[    0.534279] gpiochip_add: registered GPIOs 148 to 178 on device: GPH

<6>[    0.534478] gpiochip_add: registered GPIOs 181 to 189 on device: GPL

<6>[    0.534695] gpiochip_add: registered GPIOs 192 to 199 on device: GPM

<4>[    0.535139] sun6i ar100 driver v1.00

<4>[    0.543890] move ar100 binary data [addr = c00359d8, len = 13000] to sram_a2 finished

<3>[    0.954402] AR100 ERROR :ar100 ir power key code config type err!

<3>[    0.954413] AR100 WARING :parse ir power key code fail

<6>[    0.993436] bio: create slab <bio-0> at 0

<5>[    0.995331] SCSI subsystem initialized

<6>[    0.996129] usbcore: registered new interface driver usbfs

<6>[    0.996429] usbcore: registered new interface driver hub

<6>[    0.996651] usbcore: registered new device driver usb

<6>[    0.999839] axp_mfd 1-0034: AXP (CHIP ID: 0x17) detected

<4>[    1.004341] pmu fake power off config type err!

<6>[    1.004824] print_constraints: axp22_ldo1: 3000 mV 

<4>[    1.005225] suspend_set_state: axp22_ldo2: No configuration

<6>[    1.005284] print_constraints: axp22_ldo2: 700 <--> 3300 mV at 3300 mV 

<6>[    1.005809] print_constraints: axp22_ldo3: 700 <--> 3300 mV at 1800 mV 

<6>[    1.006320] print_constraints: axp22_ldo4: 700 <--> 3300 mV at 3000 mV 

<4>[    1.006737] suspend_set_state: axp22_ldo5: No configuration

<6>[    1.006794] print_constraints: axp22_ldo5: 700 <--> 3300 mV at 700 mV 

<4>[    1.007174] suspend_set_state: axp22_ldo6: No configuration

<6>[    1.007232] print_constraints: axp22_ldo6: 700 <--> 3300 mV at 700 mV 

<4>[    1.007608] suspend_set_state: axp22_ldo7: No configuration

<6>[    1.007665] print_constraints: axp22_ldo7: 700 <--> 3300 mV at 2800 mV 

<4>[    1.008058] suspend_set_state: axp22_ldo8: No configuration

<6>[    1.008115] print_constraints: axp22_ldo8: 700 <--> 3300 mV at 700 mV 

<4>[    1.008517] suspend_set_state: axp22_ldo9: No configuration

<6>[    1.008582] print_constraints: axp22_ldo9: 700 <--> 3300 mV at 1500 mV 

<4>[    1.008975] suspend_set_state: axp22_ldo10: No configuration

<6>[    1.009034] print_constraints: axp22_ldo10: 700 <--> 3300 mV at 1800 mV 

<4>[    1.009418] suspend_set_state: axp22_ldo11: No configuration

<6>[    1.009476] print_constraints: axp22_ldo11: 700 <--> 3300 mV at 1800 mV 

<6>[    1.010014] print_constraints: axp22_ldo12: 700 <--> 1400 mV at 1100 mV 

<6>[    1.010522] print_constraints: axp22_DCDC1: 1600 <--> 3400 mV at 3000 mV 

<6>[    1.011057] print_constraints: axp22_DCDC2: 600 <--> 1540 mV at 1200 mV 

<6>[    1.011616] print_constraints: axp22_DCDC3: 600 <--> 1860 mV at 1260 mV 

<6>[    1.012127] print_constraints: axp22_DCDC4: 600 <--> 1540 mV at 1200 mV 

<6>[    1.012643] print_constraints: axp22_DCDC5: 1000 <--> 2550 mV at 1500 mV 

<6>[    1.013078] print_constraints: axp22_ldoio0: 700 <--> 3300 mV at 2800 mV 

<6>[    1.013508] print_constraints: axp22_ldoio1: 700 <--> 3300 mV at 3800 mV 

<6>[    1.014201] input: axp22-supplyer as /devices/platform/sun6i-i2c.1/i2c-1/1-0034/axp22-supplyer.19/input/input0

<4>[    1.014215] axp charger not limit now

<4>[    1.017785] now_rest_vol = 100

<6>[    1.018590] gpiochip_add: registered GPIOs 202 to 206 on device: axp_pin

<6>[    1.019568] Advanced Linux Sound Architecture Driver Version 1.0.24.

<6>[    1.020682] Bluetooth: Core ver 2.16

<6>[    1.020840] NET: Registered protocol family 31

<6>[    1.020851] Bluetooth: HCI device and connection manager initialized

<6>[    1.020868] Bluetooth: HCI socket layer initialized

<6>[    1.020879] Bluetooth: L2CAP socket layer initialized

<6>[    1.020915] Bluetooth: SCO socket layer initialized

<6>[    1.021394] cfg80211: Calling CRDA to update world regulatory domain

<6>[    1.021987] Switching to clocksource arch_sys_counter

<5>[    1.040029] FS-Cache: Loaded

<6>[    1.040533] CacheFiles: Loaded

<6>[    1.060960] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.061177] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver

<4>[    1.061356] [usb_manager]: CONFIG_USB_SW_SUN6I_USB0_OTG

<4>[    1.061932] [sw_udc]: udc_init: version 20080411

<6>[    1.062955] NET: Registered protocol family 2

<6>[    1.063235] IP route cache hash table entries: 16384 (order: 4, 65536 bytes)

<6>[    1.063996] TCP established hash table entries: 65536 (order: 7, 524288 bytes)

<6>[    1.064984] TCP bind hash table entries: 65536 (order: 7, 786432 bytes)

<6>[    1.065910] TCP: Hash tables configured (established 65536 bind 65536)

<6>[    1.065922] TCP reno registered

<6>[    1.065937] UDP hash table entries: 256 (order: 1, 8192 bytes)

<6>[    1.065963] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)

<6>[    1.066328] NET: Registered protocol family 1

<6>[    1.066898] RPC: Registered named UNIX socket transport module.

<6>[    1.066908] RPC: Registered udp transport module.

<6>[    1.066918] RPC: Registered tcp transport module.

<6>[    1.066927] RPC: Registered tcp NFSv4.1 backchannel transport module.

<6>[    1.067182] Unpacking initramfs...

<6>[    1.214875] Freeing initrd memory: 564K

<6>[    1.214894] sunxi_reg_init enter

<4>[    1.215712] [pm]aw_pm_init!

<6>[    1.215725] standby_mode = 1. 

<6>[    1.215735] cpu0_en = 0.

<6>[    1.215743] dram_selfresh_en = 1.

<6>[    1.215753] wakeup src cnt is : 2. 

<4>[    1.215766] [exstandby]leave extended_standby_enable_wakeup_src : event 0x2000

<4>[    1.215777] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_map 0x20

<4>[    1.215789] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_group 0x0

<4>[    1.215801] [exstandby]leave extended_standby_enable_wakeup_src : event 0x2000

<4>[    1.215812] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_map 0x1020

<4>[    1.215823] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_group 0x0

<6>[    1.215835] cpus need care gpio: mem_para_info.cpus_gpio_wakeup = 0x0. 

<4>[    1.215854] [wifi]: select wifi: rtl8723au !!

<4>[    1.216232] [rtl8723au]: exec rtl8723au_wifi_gpio_init

<4>[    1.216248] [sw_hci_sun6i]: ERR: sw_ehci is null

<4>[    1.216258] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[    1.217260] [rtl8723au]: rtl8723au module power set by axp.

<4>[    1.217369] [rtl8723au]: first time

<4>[    1.217710] [wifi_pm]: wifi gpio init is OK !!

<4>[    1.219499] highmem bounce pool size: 64 pages

<6>[    1.223235] NTFS driver 2.1.30 [Flags: R/W].

<6>[    1.223700] fuse init (API version 7.18)

<6>[    1.224808] msgmni has been set to 615

<6>[    1.225839] io scheduler noop registered

<6>[    1.225851] io scheduler deadline registered (default)

<4>[    1.234763] [uart]: driver initializied

<6>[    1.235721] sw_serial.0: ttyS0 at MMIO 0x1c28000 (irq = 32) is a SW

<4>[    1.235749] [uart]: console setup baud 115200 parity n bits 8, flow n

<6>[    1.248478] console [ttyS0] enabled

<6>[    1.248970] sw_serial.2: ttyS2 at MMIO 0x1c28800 (irq = 34) is a SW

<6>[    1.249401] sw_serial.3: ttyS3 at MMIO 0x1c28c00 (irq = 35) is a SW

<6>[    1.257765] loop: module loaded

<3>[    1.257803] sun6i_vibrator_init motor is not used in config

<6>[    1.264058] sunxi_hw_init: sunxi debug register driver init

<6>[    1.264961] tun: Universal TUN/TAP device driver, 1.6

<6>[    1.264975] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>

<6>[    1.265279] PPP generic driver version 2.4.2

<6>[    1.265697] PPP BSD Compression module registered

<6>[    1.265712] PPP Deflate Compression module registered

<6>[    1.266308] PPP MPPE Compression module registered

<6>[    1.266328] NET: Registered protocol family 24

<6>[    1.266388] PPTP driver version 0.8.5

<6>[    1.266906] usbcore: registered new interface driver cdc_ether

<6>[    1.267076] usbcore: registered new interface driver cdc_eem

<6>[    1.267241] usbcore: registered new interface driver cdc_subset

<4>[    1.267324] [sw_hci_sun6i]: ERR: sw-ehci1(restrict_gpio) is invalid

<4>[    1.267339] [sw_hci_sun6i]: ERR: sw-ehci1(drv vbus) is invalid

<4>[    1.267355] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.267409] [sw_hci_sun6i]: ERR: sw-ohci1(restrict_gpio) is invalid

<4>[    1.267423] [sw_hci_sun6i]: ERR: sw-ohci1(drv vbus) is invalid

<4>[    1.267438] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.267481] [sw_hci_sun6i]: ERR: sw-ehci2(restrict_gpio) is invalid

<4>[    1.267497] [sw_hci_sun6i]: ERR: sw-ehci2(drv vbus) is invalid

<4>[    1.267512] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.267551] [sw_hci_sun6i]: ERR: sw-ohci2(restrict_gpio) is invalid

<4>[    1.267566] [sw_hci_sun6i]: ERR: sw-ohci2(drv vbus) is invalid

<4>[    1.267581] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.267872] [sw_hci_sun6i]: [sw-ehci1]: probe, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<4>[    1.267901] [sw_hci_sun6i]: [sw-ehci1]: open clock

<4>[    1.268131] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power ON

<6>[    1.268149] sw-ehci sw-ehci.1: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.268186] sw-ehci sw-ehci.1: new USB bus registered, assigned bus number 1

<6>[    1.268303] sw-ehci sw-ehci.1: irq 104, io mem 0xf1c1a000

<6>[    1.282070] sw-ehci sw-ehci.1: USB 0.0 started, EHCI 1.00

<4>[    1.282090] ehci_irq: highspeed device connect

<6>[    1.283067] hub 1-0:1.0: USB hub found

<6>[    1.283100] hub 1-0:1.0: 1 port detected

<4>[    1.283665] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_disable_ehci

<4>[    1.283684] [sw_hci_sun6i]: [sw-ehci1]: remove, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<6>[    1.283710] sw-ehci sw-ehci.1: remove, state 1

<6>[    1.283732] usb usb1: USB disconnect, device number 1

<6>[    1.285377] sw-ehci sw-ehci.1: USB bus 1 deregistered

<4>[    1.285400] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power OFF

<4>[    1.285415] [sw_hci_sun6i]: [sw-ehci1]: close clock

<4>[    1.285442] [sw_hci_sun6i]: ERR: usb1 sw-ohci1 is not enable

<4>[    1.285680] [sw_hci_sun6i]: [sw-ehci2]: probe, pdev->name: sw-ehci, pdev->id: 2, sw_ehci: 0xc08926bc

<4>[    1.285699] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[    1.285922] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<6>[    1.285937] sw-ehci sw-ehci.2: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.285969] sw-ehci sw-ehci.2: new USB bus registered, assigned bus number 1

<6>[    1.286048] sw-ehci sw-ehci.2: irq 106, io mem 0xf1c1b000

<6>[    1.302063] sw-ehci sw-ehci.2: USB 0.0 started, EHCI 1.00

<6>[    1.302944] hub 1-0:1.0: USB hub found

<6>[    1.302987] hub 1-0:1.0: 1 port detected

<4>[    1.303527] [sw_hci_sun6i]: ERR: usb2 sw-ohci2 is not enable

<4>[    1.303541] [sw_hci_sun6i]: ERR: usb0  is not enable

<6>[    1.303748] usbcore: registered new interface driver cdc_acm

<6>[    1.303762] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters

<6>[    1.303777] Initializing USB Mass Storage driver...

<6>[    1.303987] usbcore: registered new interface driver usb-storage

<6>[    1.304000] USB Mass Storage support registered.

<6>[    1.304171] usbcore: registered new interface driver ums-alauda

<6>[    1.304344] usbcore: registered new interface driver ums-cypress

<6>[    1.304513] usbcore: registered new interface driver ums-datafab

<6>[    1.304688] usbcore: registered new interface driver ums_eneub6250

<6>[    1.304855] usbcore: registered new interface driver ums-freecom

<6>[    1.305025] usbcore: registered new interface driver ums-isd200

<6>[    1.305194] usbcore: registered new interface driver ums-jumpshot

<6>[    1.305363] usbcore: registered new interface driver ums-karma

<6>[    1.305530] usbcore: registered new interface driver ums-onetouch

<6>[    1.305715] usbcore: registered new interface driver ums-realtek

<6>[    1.305884] usbcore: registered new interface driver ums-sddr09

<6>[    1.306062] usbcore: registered new interface driver ums-sddr55

<6>[    1.306231] usbcore: registered new interface driver ums-usbat

<6>[    1.306605] usbcore: registered new interface driver usbserial

<6>[    1.306619] usbserial: USB Serial Driver core

<6>[    1.306774] USB Serial support registered for GSM modem (1-port)

<6>[    1.307000] usbcore: registered new interface driver option

<6>[    1.307014] option: v0.7.2:USB Driver for GSM modems

<4>[    1.307505] [sw_udc]: [sw_usb_udc]: binding gadget driver 'android_usb'

<4>[    1.307527] [sw_udc]: alloc request: ep(0xc07fdf18, ep0, 64), req(0xeeaef0c0)

<4>[    1.307543] [sun6i_usb]: ERR: usb device is not active

<4>[    1.307559] [sw_udc]: sw_udc_pullup, is_on = 0

<4>[    1.307571] [sun6i_usb]: usb device is not active

<6>[    1.310755] android_usb gadget: Mass Storage Function, version: 2009/09/11

<6>[    1.310772] android_usb gadget: Number of LUNs=2

<6>[    1.310787]  lun0: LUN: removable file: (no medium)

<6>[    1.310801]  lun1: LUN: removable file: (no medium)

<4>[    1.311332] [sun6i_usb]: ERR: usb device is not active

<6>[    1.311356] android_usb gadget: android_usb ready

<4>[    1.311487] [sw_hcd0]: usb host driver initialize........

<4>[    1.311619] [sw_hcd0]: open_usb_clock

<4>[    1.311866] [sun6i_usb]: [sw_hcd0]: host_init_state = 0

<4>[    1.311880] [sw_hcd0]: platform is usb host

<4>[    1.311945] [sw_hcd0]: sw_hcd_init_controller: sw_hcd_host0: USB Host mode controller at f1c19000 using PIO, IRQ 103

<6>[    1.311964] sw_hcd_host0 sw_hcd_host0: sw_hcd host driver

<6>[    1.311982] sw_hcd_host0 sw_hcd_host0: new USB bus registered, assigned bus number 2

<6>[    1.312903] hub 2-0:1.0: USB hub found

<6>[    1.312934] hub 2-0:1.0: 1 port detected

<4>[    1.313458] [sw_hcd0]: sw_usb_host0_disable start

<4>[    1.313473] [sw_hcd0]: sw_hcd_wait_for_disconnect cnt=0

<4>[    1.313487] [sun6i_usb]: [sw_hcd_host0]: Set USB Power OFF

<4>[    1.313506] [sun6i_usb]: -------sw_hcd0_soft_disconnect---------

<4>[    1.313519] [sun6i_usb]: wrn: hcd is not enable, need not stop hcd

<4>[    1.313549] [sw_hcd0]: close_usb_clock

<4>[    1.313567] [sw_hcd0]: sw_usb_host0_disable end

<6>[    1.314263] mousedev: PS/2 mouse device common for all mice

<6>[    1.314991] =====ctp_fetch_sysconfig_para=====. 

<6>[    1.315785] sun6i-rtc sun6i-rtc: sun6i_rtc_probe tmp_data = 380239881

<6>[    1.315870] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[    1.315887] sun6i-rtc sun6i-rtc: read time 2014-1-14 4:11:43

<6>[    1.316439] using rtc device, rtc, for alarms

<6>[    1.316486] sun6i-rtc sun6i-rtc: rtc core: registered rtc as rtc0

<6>[    1.316653] Linux video capture interface: v2.00

<4>[    1.316794] [cedar]: install start!!!

<4>[    1.317718] [cedar]: install end!!!

<6>[    1.327811] device-mapper: ioctl: 4.22.0-ioctl (2011-10-19) initialised: dm-devel@redhat.com

<6>[    1.328377] Bluetooth: HCI UART driver ver 2.2

<6>[    1.328394] Bluetooth: HCI H4 protocol initialized

<6>[    1.328407] Bluetooth: HCI BCSP protocol initialized

<4>[    1.328895] [mmc]: sw_mci_init

<4>[    1.328950] [mmc]: MMC host used card: 0x3, boot card: 0x0, io_card 2

<4>[    1.330203] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[    1.331292] [mmc]: sdc0 Probe: base:0xf0038000 irq:92 sg_cpu:ffdfc000(42c00000) ret 0.

<4>[    1.331813] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[    1.332878] [mmc]: sdc1 Probe: base:0xf003a000 irq:93 sg_cpu:ffdfb000(42c01000) ret 0.

<6>[    1.335700] usbcore: registered new interface driver usbhid

<6>[    1.335714] usbhid: USB HID core driver

<6>[    1.336649] ashmem: initialized

<6>[    1.336910] logger: created 256K log 'log_main'

<6>[    1.337160] logger: created 256K log 'log_events'

<6>[    1.337413] logger: created 256K log 'log_radio'

<6>[    1.337673] logger: created 256K log 'log_system'

<6>[    1.338834] input: headset as /devices/virtual/input/input1

<4>[    1.341208] enter sun6i Audio codec!!!

<6>[    1.342717] sun6i audio support initialized

<4>[    1.342829] sun6i Audio codec init end

<6>[    1.345168] asoc: sndhdmi <-> sun6i-hdmiaudio.0 mapping ok

<6>[    1.346239] ALSA device list:

<6>[    1.346252]   #0: sun6i-CODEC  Audio Codec

<6>[    1.346264]   #1: sndhdmi

<6>[    1.346526] Netfilter messages via NETLINK v0.30.

<6>[    1.346635] nf_conntrack version 0.5.0 (16384 buckets, 65536 max)

<6>[    1.347141] ctnetlink v0.93: registering with nfnetlink.

<6>[    1.347174] NF_TPROXY: Transparent proxy support initialized, version 4.1.0

<6>[    1.347187] NF_TPROXY: Copyright (c) 2006-2007 BalaBit IT Ltd.

<6>[    1.348092] xt_time: kernel timezone is -0000

<6>[    1.348139] IPv4 over IPv4 tunneling driver

<6>[    1.349009] GRE over IPv4 demultiplexor driver

<6>[    1.349023] GRE over IPv4 tunneling driver

<6>[    1.350012] ip_tables: (C) 2000-2006 Netfilter Core Team

<6>[    1.350228] TCP cubic registered

<6>[    1.350239] Initializing XFRM netlink socket

<6>[    1.350933] NET: Registered protocol family 10

<6>[    1.352209] ip6_tables: (C) 2000-2006 Netfilter Core Team

<6>[    1.352409] IPv6 over IPv4 tunneling driver

<6>[    1.354315] NET: Registered protocol family 17

<6>[    1.354357] NET: Registered protocol family 15

<6>[    1.354490] Bluetooth: RFCOMM TTY layer initialized

<6>[    1.354528] Bluetooth: RFCOMM socket layer initialized

<6>[    1.354542] Bluetooth: RFCOMM ver 1.11

<6>[    1.354556] Bluetooth: BNEP (Ethernet Emulation) ver 1.3

<6>[    1.354569] Bluetooth: BNEP filters: protocol multicast

<6>[    1.354584] Bluetooth: HIDP (Human Interface Emulation) ver 1.2

<6>[    1.354811] L2TP core driver, V2.0

<6>[    1.354840] PPPoL2TP kernel driver, V2.0

<6>[    1.354852] L2TP IP encapsulation support (L2TPv3)

<6>[    1.355002] L2TP netlink interface

<6>[    1.355041] L2TP ethernet pseudowire support (L2TPv3)

<6>[    1.355055] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 3

<6>[    1.355089] ThumbEE CPU extension supported.

<5>[    1.355115] Registering SWP/SWPB emulation handler

<4>[    1.355953] [rfkill]: rfkill set power 0

<4>[    1.355970] [rtl8723au]: rtl8723au is powered up by bt

<4>[    1.355985] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_enable_ehci

<4>[    1.356004] [sw_hci_sun6i]: [sw-ehci1]: probe, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<4>[    1.356026] [sw_hci_sun6i]: [sw-ehci1]: open clock

<4>[    1.356256] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power ON

<6>[    1.356274] sw-ehci sw-ehci.1: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.356312] sw-ehci sw-ehci.1: new USB bus registered, assigned bus number 3

<6>[    1.356418] sw-ehci sw-ehci.1: irq 104, io mem 0xf1c1a000

<4>[    1.357560] regulator_init_complete: axp22_ldoio0: incomplete constraints, leaving on

<4>[    1.357620] regulator_init_complete: axp22_DCDC5: incomplete constraints, leaving on

<4>[    1.357677] regulator_init_complete: axp22_DCDC4: incomplete constraints, leaving on

<4>[    1.357734] regulator_init_complete: axp22_DCDC3: incomplete constraints, leaving on

<4>[    1.357791] regulator_init_complete: axp22_DCDC2: incomplete constraints, leaving on

<4>[    1.357849] regulator_init_complete: axp22_DCDC1: incomplete constraints, leaving on

<4>[    1.357906] regulator_init_complete: axp22_ldo12: incomplete constraints, leaving on

<4>[    1.357963] regulator_init_complete: axp22_ldo11: incomplete constraints, leaving on

<4>[    1.358263] regulator_init_complete: axp22_ldo4: incomplete constraints, leaving on

<4>[    1.358320] regulator_init_complete: axp22_ldo3: incomplete constraints, leaving on

<4>[    1.358450] [sw_module]: sw_module_init 1.0

<4>[    1.358853] [sw_module]: usimt6276ma modem support

<4>[    1.358876] [sw_module]: ERR: get dldo_name failed

<4>[    1.358932] [sw_module]: gpio_request bb_wake failed

<4>[    1.358955] [sw_module]: usi6276 modem init

<4>[    1.359242] [sw_module]: usi6276 modem probe

<4>[    1.359558] [sw_module]: usi6276_start: start ======

<3>[    1.359572] otg_wakelock_init: No OTG transceiver found

<4>[    1.359666] [sw_module]: before power on ======

<4>[    1.359676] [sw_module]: set usi6276 modem power on

<4>[    1.359690] [sw_module]: err: dldo parameter is invalid. dldo_name=, dldo_min_uV=2800000, dldo_max_uV=2800000.

<6>[    1.365458] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[    1.365477] sun6i-rtc sun6i-rtc: read time 2014-1-14 4:11:43

<6>[    1.365518] sun6i-rtc sun6i-rtc: setting system clock to 2014-01-14 04:11:43 UTC (1389672703)

<6>[    1.366240] Freeing init memory: 284K

<6>[    1.366255] Write protecting the kernel text section c0008000 - c0784000

<6>[    1.366439] rodata_test: attempting to write to read-only section:

<6>[    1.366458] write to read-only section trapped, success

<3>[    1.371337] init: /init.sun6i.rc: 150: invalid service name 'ttyusb-compatible'

<6>[    1.379575] sw-ehci sw-ehci.1: USB 0.0 started, EHCI 1.00

<4>[    1.379596] ehci_irq: highspeed device connect

<6>[    1.380674] hub 3-0:1.0: USB hub found

<6>[    1.380708] hub 3-0:1.0: 1 port detected

<4>[    1.381276] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[    1.381292] [rtl8723au]: rtl8723au power state change: wifi 0, bt 1 !!

<4>[    1.381577] init (1): /proc/1/oom_adj is deprecated, please use /proc/1/oom_score_adj instead.

<6>[    1.503415] init: command 'loglevel' r=0

<6>[    1.503504] init: command 'export' r=0

<6>[    1.503527] init: command 'export' r=0

<6>[    1.503547] init: command 'export' r=0

<6>[    1.503568] init: command 'export' r=0

<6>[    1.503587] init: command 'export' r=0

<6>[    1.503607] init: command 'export' r=0

<6>[    1.503626] init: command 'export' r=0

<6>[    1.503646] init: command 'export' r=0

<6>[    1.503665] init: command 'export' r=0

<6>[    1.503687] init: command 'export' r=0

<4>[    1.513121] hello:init_nand_libmodule,21

<4>[    1.513140] hello:init_nand_libmodule,22

<4>[    1.513160] [NAND]nand init start, nand0_used_flag is 1

<4>[    1.513175] [NAND] nand IO Merge: 0x2 

<4>[    1.513185] [NAND] turn off log release thread

<4>[    1.513200] [NAND] nand driver version: 0x2, 0x12 0x20130607 14:00

<4>[    1.515563] [NAND]nand get good block ratio  896

<4>[    1.515576] nand good block ratio value is valid 

<4>[    1.515613] Request memory for lsb page table 

<4>[    1.515627] page type: 0

<4>[    1.522990] PHY_PageReadSpare: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[    1.525268] PHY_PageReadSpare: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[    1.528321] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[    1.537010] [NAND]nandlogrelease_thread init 

<6>[    1.538891]  nanda:

<6>[    1.540842]  nandb: unknown partition table

<6>[    1.542678]  nandc: unknown partition table

<6>[    1.545395]  nandd: unknown partition table

<6>[    1.548083]  nande: unknown partition table

<6>[    1.550731]  nandf: unknown partition table

<6>[    1.552551]  nandg: unknown partition table

<6>[    1.560512]  nandh: unknown partition table

<6>[    1.562393]  nandi: unknown partition table

<6>[    1.565108]  nandj:

<4>[    1.565844] [NAND]nand init end.

<6>[    1.566215] init: command 'insmod' r=0

<6>[    1.566304] init: command 'symlink' r=0

<6>[    1.566356] init: command 'symlink' r=0

<6>[    1.566407] init: command 'symlink' r=0

<6>[    1.566448] init: command 'mkdir' r=0

<6>[    1.566604] init: command 'mount' r=-1

<6>[    1.566645] init: command 'mkdir' r=0

<6>[    1.566722] init: command 'mkdir' r=0

<6>[    1.566807] init: command 'mkdir' r=0

<6>[    1.566874] init: command 'mkdir' r=0

<6>[    1.566937] init: command 'mkdir' r=0

<6>[    1.567006] init: command 'mkdir' r=0

<6>[    1.567070] init: command 'mkdir' r=0

<6>[    1.567137] init: command 'mkdir' r=0

<6>[    1.567219] init: command 'mkdir' r=0

<6>[    1.567376] init: command 'mount' r=0

<6>[    1.567450] init: command 'mkdir' r=0

<6>[    1.567518] init: command 'mkdir' r=0

<6>[    1.567583] init: command 'mkdir' r=0

<6>[    1.567721] init: command 'mount' r=0

<6>[    1.567790] init: command 'mkdir' r=0

<6>[    1.567918] init: command 'mount' r=0

<6>[    1.568073] init: command 'write' r=0

<6>[    1.568203] init: command 'write' r=-2

<6>[    1.568310] init: command 'write' r=0

<6>[    1.568417] init: command 'write' r=-2

<6>[    1.568524] init: command 'write' r=-2

<6>[    1.568626] init: command 'write' r=-2

<6>[    1.568694] init: command 'write' r=0

<6>[    1.568767] init: command 'write' r=0

<6>[    1.568841] init: command 'write' r=0

<6>[    1.568913] init: command 'write' r=0

<6>[    1.569013] init: command 'write' r=0

<6>[    1.569090] init: command 'write' r=0

<6>[    1.569168] init: command 'write' r=0

<6>[    1.569240] init: command 'write' r=0

<6>[    1.569282] init: command 'mkdir' r=0

<6>[    1.622221] init: command 'mount' r=0

<6>[    1.622290] init: command 'chown' r=0

<6>[    1.622461] init: command 'chown' r=0

<6>[    1.622537] init: command 'chmod' r=0

<6>[    1.622591] init: command 'write' r=-22

<6>[    1.622646] init: command 'write' r=0

<6>[    1.622695] init: command 'write' r=0

<6>[    1.622851] init: command 'mkdir' r=0

<6>[    1.622908] init: command 'chown' r=0

<6>[    1.622958] init: command 'chmod' r=0

<6>[    1.623005] init: command 'write' r=0

<6>[    1.623055] init: command 'write' r=0

<6>[    1.623105] init: command 'write' r=0

<6>[    1.623263] init: command 'mkdir' r=0

<6>[    1.623320] init: command 'chown' r=0

<6>[    1.623371] init: command 'chmod' r=0

<6>[    1.623425] init: command 'write' r=0

<6>[    1.623478] init: command 'write' r=0

<6>[    1.623530] init: command 'write' r=0

<6>[    1.623599] init: command 'chmod' r=0

<6>[    1.623621] init: processing action 0x348f8 (init)

<6>[    1.623646] init: command 'export' r=0

<6>[    1.623713] init: command 'mkdir' r=0

<6>[    1.623775] init: command 'symlink' r=0

<6>[    1.623843] init: command 'symlink' r=0

<6>[    1.623913] init: command 'mkdir' r=0

<6>[    1.623977] init: command 'mkdir' r=0

<6>[    1.624099] init: command 'mount' r=0

<6>[    1.624166] init: command 'mkdir' r=0

<6>[    1.624186] init: processing action 0x34a88 (early-fs)

<6>[    1.633712] EXT4-fs (nandd): mounted filesystem with ordered data mode. Opts: (null)

<6>[    1.661913] EXT4-fs (nandh): recovery complete

<6>[    1.664241] EXT4-fs (nandh): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,errors=remount-ro

<6>[    1.692096] usb 3-1: new high-speed USB device number 2 using sw-ehci

<6>[    1.742104] fs_mgr: Running /system/bin/e2fsck on /dev/block/nandh

<6>[    1.827383] EXT4-fs (nandh): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,barrier=1

<6>[    1.831523] EXT4-fs (nandi): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,errors=remount-ro

<6>[    1.892093] fs_mgr: Running /system/bin/e2fsck on /dev/block/nandi

<6>[    1.907364] EXT4-fs (nandi): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,barrier=1

<6>[    1.919106] EXT4-fs (nande): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,errors=remount-ro

<4>[    2.002063] ====codec_resume_events===

<6>[    2.002104] fs_mgr: Running /system/bin/e2fsck on /dev/block/nande

<6>[    2.056813] EXT4-fs (nande): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,barrier=1

<6>[    2.057232] init: command 'mount_all' r=0

<6>[    2.057291] init: command 'setprop' r=0

<6>[    2.234748] [DISP]==disp_module_init==

<6>[    2.235921] [DISP]==disp_probe call==

<6>[    2.235939] [DISP]==disp_probe finish==

<6>[    2.236345] [DISP]capture_module_init

<6>[    2.237210] [DISP]capture_probe

<6>[    2.237396] [DISP]==capture finish==

<6>[    2.237409] [DISP]==disp_module_init finish==

<6>[    2.239073] init: command 'insmod' r=0

<6>[    2.259796] [LCD]==lcd_module_init==

<4>[    2.261699] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/iep/deu/iep_deu.c,line:458:    deu_mode1 not exist.

<4>[    2.261836] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/iep/drc/iep_drc.c,line:565:    lcdgamma4iep for lcd1 not exist.

<6>[    2.282062] [DISP]==Fb_Init==

<6>[    2.299231] [LCD]==lcd_module_init finish==

<6>[    2.299535] init: command 'insmod' r=0

<6>[    2.318012] [HDMI]==hdmi_module_init==

<6>[    2.319085] [HDMI]==hdmi_probe call==

<6>[    2.322367] [DISP]==Fb_Init==

<6>[    2.322381] [HDMI]==hdmi_probe finish==

<6>[    2.322587] [HDMI]==hdmi_module_init finish==

<6>[    2.322818] init: command 'insmod' r=0

<6>[    2.330346] init: command 'insmod' r=0

<6>[    2.337623] init: command 'insmod' r=0

<6>[    2.344807] init: command 'insmod' r=0

<6>[    2.351960] asoc: sndi2s <-> sun6i-i2s.0 mapping ok

<6>[    2.353616] init: command 'insmod' r=0

<6>[    2.360565] init: command 'insmod' r=0

<4>[    2.364350] [LCD] ANX9804 Chip found

<4>[    2.366907] [LCD] ANX9804 clock is stable.

<6>[    2.367831] init: command 'insmod' r=0

<6>[    2.375151] init: command 'insmod' r=0

<6>[    2.382442] asoc: sndpcm <-> sun6i-pcm.0 mapping ok

<6>[    2.384050] init: command 'insmod' r=0

<6>[    2.384106] init: processing action 0x37e30 (console_init)

<3>[    2.385058] init: width = 2048

<3>[    2.388484] init: height = 1536

<3>[    2.391995] init: s.st_size = 12582912

<6>[    2.448804] init: command 'console_init' r=0

<6>[    2.448877] init: processing action 0x2dbc0 (fs)

<6>[    2.448990] init: command 'mount' r=-1

<6>[    2.449014] init: command 'mount' r=-1

<6>[    2.449035] init: command 'mount' r=-1

<6>[    2.449054] init: command 'mount' r=-1

<6>[    2.449072] init: processing action 0x34c90 (fs)

<3>[    2.450467] init: dont need format /dev/block/by-name/UDISK

<6>[    2.456539] init: command 'format_userdata' r=1

<6>[    2.465260] init: command 'mkdir' r=0

<6>[    2.466322] init: command 'chmod' r=-30

<6>[    2.466384] init: command 'chmod' r=-2

<6>[    2.467423] init: command 'chmod' r=-30

<6>[    2.467495] init: command 'chmod' r=-30

<6>[    2.467541] init: command 'chown' r=-30

<6>[    2.467578] init: command 'chown' r=-2

<6>[    2.467620] init: command 'chown' r=-30

<6>[    2.467662] init: command 'chown' r=-30

<4>[    2.572571] create_regulator: axp22_DCDC2: Failed to create debugfs directory

<7>[    2.573180] gpu:open gpu power!

<6>[    2.594384] init: command 'insmod' r=0

<4>[    2.602321] #####: Device 0: Framebuffer physical address: 0x43100000

<6>[    2.602396] init: command 'insmod' r=0

<6>[    2.602613] init: command 'chmod' r=0

<6>[    2.602625] PVR_K:(Error): ############ !psDevInfo->psKernelSGXHostCtlMemInfo [0, ]

<6>[    2.602708] init: command 'chmod' r=0

<6>[    2.610339] init: command 'insmod' r=0

<6>[    2.615845] init: command 'insmod' r=0

<4>[    2.627421] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    2.627453] create_regulator: axp22_ldoio0: Failed to create debugfs directory

<4>[    2.627496] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    2.627522] create_regulator: axp22_ldo10: Failed to create debugfs directory

<4>[    2.802267] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x3c)

<4>[    2.962248] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x21)

<4>[    3.322243] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x21)

<4>[    3.482242] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x3c)

<6>[    3.823918] init: command 'insmod' r=0

<6>[    3.828220] init: command 'insmod' r=0

<6>[    3.832354] init: command 'insmod' r=0

<6>[    3.839853] init: command 'insmod' r=0

<6>[    3.846126] init: command 'insmod' r=0

<6>[    3.852706] init: command 'insmod' r=0

<6>[    3.860653] init: command 'insmod' r=0

<6>[    3.868304] init: command 'insmod' r=0

<4>[    3.882205] ehci_irq: highspeed device connect

<5>[    3.907154] [VFE]Welcome to Video Front End driver

<5>[    3.907813] [VFE]pdev->id = 1

<5>[    3.907825] [VFE]dev->mipi_sel = 1

<5>[    3.907836] [VFE]dev->vip_sel = 1

<5>[    3.907847] [VFE]dev->isp_sel = 0

<4>[    3.924091] [VFE_WARN]fetch front_camera from camera.ini failed,apply default value!

<4>[    3.924132] [VFE_WARN]fetch flicker_type from camera.ini failed,apply default value!

<4>[    3.924148] [VFE_WARN]fetch adaptive_frame_rate from camera.ini failed,apply default value!

<4>[    3.924167] [VFE_WARN]fetch color_denoise_level from camera.ini failed,apply default value!

<4>[    3.924183] [VFE_WARN]fetch defog_value from camera.ini failed,apply default value!

<4>[    3.924199] [VFE_WARN]fetch brightness_tune from camera.ini failed,apply default value!

<4>[    3.924214] [VFE_WARN]fetch gain_delay_frame from camera.ini failed,apply default value!

<4>[    3.924831] [VFE_WARN]fetch csc_coeff_0 from camera.ini failed,apply default value!

<4>[    3.924849] [VFE_WARN]fetch csc_coeff_1 from camera.ini failed,apply default value!

<4>[    3.924865] [VFE_WARN]fetch csc_coeff_2 from camera.ini failed,apply default value!

<4>[    3.924881] [VFE_WARN]fetch csc_coeff_3 from camera.ini failed,apply default value!

<4>[    3.924896] [VFE_WARN]fetch csc_coeff_4 from camera.ini failed,apply default value!

<4>[    3.924912] [VFE_WARN]fetch csc_coeff_5 from camera.ini failed,apply default value!

<5>[    3.934876] [VFE]vip_pin_list addr = 0 

<5>[    3.934893] [VFE]request gpio cnt=18, i=18

<5>[    3.935479] [VFE]vfe_init end

<6>[    3.935962] init: command 'insmod' r=0

<5>[    3.942090] [VFE]probe_work_handle start!

<5>[    3.942815] [VFE]registered sub device,input_num = 0

<5>[    3.943326] [VFE]registered act sub device,input_num = 0

<4>[    3.943386] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    3.943411] create_regulator: axp22_ldoio0: Failed to create debugfs directory

<4>[    3.943438] create_regulator: axp22_ldo9: Failed to create debugfs directory

<5>[    3.943921] [VFE]registered sub device,input_num = 1

<4>[    3.943951] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    3.943974] create_regulator: axp22_ldoio0: Failed to create debugfs directory

<4>[    3.944001] create_regulator: axp22_ldo10: Failed to create debugfs directory

<5>[    3.944018] [VFE]power on and standy on camera 0!

<5>[    3.945380] [VFE]mclk on

<7>[    3.951221] G2D: drv_g2d_init

<6>[    3.951431] G2D: Module initialized.major:245

<6>[    3.951628] init: command 'insmod' r=0

<4>[    3.957439] [VFE_WARN]invalid gpio

<6>[    3.961199] usbcore: registered new interface driver asix

<6>[    3.961256] init: command 'insmod' r=0

<6>[    3.970220] usbcore: registered new interface driver qf9700

<6>[    3.970278] init: command 'insmod' r=0

<6>[    3.978333] usbcore: registered new interface driver MOSCHIP usb-ethernet driver

<6>[    3.978389] init: command 'insmod' r=0

<6>[    3.987460] usbcore: registered new interface driver rtl8150

<6>[    3.987515] init: command 'insmod' r=0

<6>[    3.994161] init: command 'insmod' r=0

<6>[    3.999655] input: sw-keyboard as /devices/virtual/input/input2

<6>[    4.000064] init: command 'insmod' r=0

<6>[    4.000610] init: command 'chmod' r=0

<6>[    4.000882] init: command 'chown' r=0

<4>[    4.001037] [OV5647]disalbe oe!

<6>[    4.001224] init: command 'chmod' r=0

<6>[    4.001294] init: command 'chmod' r=-2

<6>[    4.001508] init: command 'chown' r=0

<6>[    4.001611] init: command 'chown' r=0

<4>[    4.001703] [rfkill]: rfkill set power 1

<4>[    4.001847] [rtl8723au]: rtl8723au is powered down by bt

<4>[    4.001863] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_disable_ehci

<4>[    4.001883] [sw_hci_sun6i]: [sw-ehci1]: remove, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<6>[    4.001914] sw-ehci sw-ehci.1: remove, state 1

<6>[    4.001945] usb usb3: USB disconnect, device number 1

<6>[    4.001961] usb 3-1: USB disconnect, device number 2

<6>[    4.006493] sw-ehci sw-ehci.1: USB bus 3 deregistered

<4>[    4.006520] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power OFF

<4>[    4.006536] [sw_hci_sun6i]: [sw-ehci1]: close clock

<4>[    4.006559] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[    4.006573] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<5>[    4.014858] [VFE]power on and standy on camera 1!

<5>[    4.016116] [VFE]mclk on

<6>[    4.022336] init: command 'write' r=0

<6>[    4.022406] init: command 'chown' r=-2

<6>[    4.022540] init: command 'chown' r=-30

<6>[    4.022610] init: command 'chown' r=-2

<6>[    4.022674] init: command 'setprop' r=0

<4>[    4.028170] [VFE_WARN]invalid gpio

<6>[    4.032852] rtk_btusb: Realtek Bluetooth USB driver ver 1.0.20130524

<4>[    4.032868] Registering file operations for btfcd driver

<4>[    4.033423] Class driver initialized successfully

<6>[    4.033672] usbcore: registered new interface driver rtk_btusb

<6>[    4.033726] init: command 'insmod' r=0

<6>[    4.033782] rtk_btusb: btfcd open

<6>[    4.033788] 

<3>[    4.033798] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.038790] rtk_btusb: btfcd open

<6>[    4.038795] 

<3>[    4.038804] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.043817] init: command 'chmod' r=-1

<6>[    4.043856] rtk_btusb: btfcd open

<6>[    4.043861] 

<3>[    4.043871] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.048857] rtk_btusb: btfcd open

<6>[    4.048862] 

<3>[    4.048871] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.053861] init: command 'chown' r=-1

<6>[    4.053884] init: processing action 0x2dca8 (post-fs)

<6>[    4.053987] init: command 'mount' r=0

<6>[    4.054027] init: command 'mount' r=0

<6>[    4.054176] init: command 'chown' r=0

<6>[    4.054238] init: command 'chmod' r=0

<6>[    4.054258] init: command 'restorecon' r=0

<6>[    4.067111] init: command 'chown' r=0

<6>[    4.067177] init: command 'chmod' r=0

<6>[    4.067196] init: command 'restorecon' r=0

<6>[    4.067314] init: command 'chown' r=0

<6>[    4.067388] init: command 'chmod' r=0

<6>[    4.067463] init: command 'chown' r=0

<6>[    4.067534] init: command 'chmod' r=0

<6>[    4.067608] init: command 'chown' r=0

<6>[    4.067678] init: command 'chmod' r=0

<6>[    4.067750] init: command 'chown' r=0

<6>[    4.067819] init: command 'chmod' r=0

<6>[    4.067893] init: command 'chown' r=-2

<6>[    4.067950] init: command 'chmod' r=-2

<6>[    4.068077] init: command 'mkdir' r=0

<6>[    4.068121] init: processing action 0x2dfd8 (post-fs-data)

<6>[    4.068193] init: command 'chown' r=0

<6>[    4.068248] init: command 'chmod' r=0

<6>[    4.068267] init: command 'restorecon' r=0

<6>[    4.068404] init: command 'mkdir' r=0

<6>[    4.068445] init: command 'copy' r=-1

<6>[    4.069449] init: command 'chown' r=-2

<6>[    4.069490] init: command 'chmod' r=-2

<6>[    4.069527] init: command 'copy' r=-1

<6>[    4.069583] init: command 'chown' r=-2

<6>[    4.069620] init: command 'chmod' r=-2

<6>[    4.069659] init: command 'write' r=-2

<6>[    4.069776] init: command 'mkdir' r=0

<6>[    4.069934] init: command 'mkdir' r=0

<6>[    4.070074] init: command 'mkdir' r=0

<6>[    4.070199] init: command 'mkdir' r=0

<6>[    4.070319] init: command 'mkdir' r=0

<6>[    4.070446] init: command 'mkdir' r=0

<6>[    4.070568] init: command 'mkdir' r=0

<6>[    4.070688] init: command 'mkdir' r=0

<6>[    4.070823] init: command 'mkdir' r=0

<4>[    4.071543] [CSI][GC2035]disalbe oe!

<6>[    4.071794] init: command 'chmod' r=0

<6>[    4.071860] init: command 'chown' r=0

<6>[    4.071986] init: command 'mkdir' r=0

<6>[    4.072136] init: command 'mkdir' r=0

<6>[    4.072195] init: command 'chown' r=0

<6>[    4.073192] init: command 'mkdir' r=0

<6>[    4.073313] init: command 'mkdir' r=0

<6>[    4.074330] init: command 'mkdir' r=0

<6>[    4.075316] init: command 'mkdir' r=0

<6>[    4.075438] init: command 'mkdir' r=0

<6>[    4.077281] init: command 'mkdir' r=0

<6>[    4.077398] init: command 'mkdir' r=0

<6>[    4.078425] init: command 'mkdir' r=0

<6>[    4.078556] init: command 'mkdir' r=0

<6>[    4.079568] init: command 'mkdir' r=0

<6>[    4.080556] init: command 'mkdir' r=0

<6>[    4.080678] init: command 'mkdir' r=0

<6>[    4.081692] init: command 'mkdir' r=0

<6>[    4.081748] init: command 'chown' r=0

<6>[    4.081802] init: command 'chmod' r=0

<6>[    4.081920] init: command 'mkdir' r=0

<6>[    4.082074] init: command 'mkdir' r=0

<6>[    4.082096] init: processing action 0x32288 (post-fs-data)

<6>[    4.082317] init: command 'chown' r=0

<6>[    4.082431] init: command 'chmod' r=0

<6>[    4.082535] init: command 'chown' r=0

<6>[    4.082621] init: command 'chmod' r=0

<6>[    4.082641] init: processing action 0x34c60 (post-fs-data)

<6>[    4.082661] init: processing action 0x37e78 (property_service_init)

<5>[    4.083584] [VFE]mclk off

<5>[    4.084102] [VFE]V4L2 device registered as video1

<5>[    4.084142] [VFE]register_early_suspend @ probe handle!

<5>[    4.084157] [VFE]probe_work_handle end!

<6>[    4.096920] init: Created socket '/dev/socket/property_service' with mode '666', user '0', group '0'

<6>[    4.096961] init: command 'property_service_init' r=0

<6>[    4.096991] init: processing action 0x37ec0 (signal_init)

<6>[    4.097073] init: command 'signal_init' r=0

<6>[    4.097110] init: processing action 0x37f08 (check_startup)

<6>[    4.097171] init: command 'check_startup' r=0

<6>[    4.097192] init: processing action 0x2e768 (boot)

<6>[    4.098108] init: command 'ifup' r=0

<6>[    4.098241] init: command 'hostname' r=0

<6>[    4.098325] init: command 'domainname' r=0

<6>[    4.098354] init: command 'setrlimit' r=0

<6>[    4.098436] init: command 'write' r=0

<6>[    4.098511] init: command 'write' r=0

<6>[    4.098638] init: command 'chown' r=0

<6>[    4.098701] init: command 'chmod' r=0

<6>[    4.098773] init: command 'chown' r=0

<6>[    4.098833] init: command 'chmod' r=0

<6>[    4.098908] init: command 'write' r=0

<6>[    4.098995] init: command 'write' r=0

<6>[    4.099056] init: command 'chown' r=-2

<6>[    4.099110] init: command 'chown' r=-2

<6>[    4.099163] init: command 'chown' r=-2

<6>[    4.099217] init: command 'chown' r=-2

<6>[    4.099270] init: command 'chown' r=-2

<6>[    4.099345] init: command 'chown' r=-2

<6>[    4.099411] init: command 'chown' r=0

<6>[    4.099477] init: command 'chown' r=0

<6>[    4.099543] init: command 'chown' r=0

<6>[    4.099626] init: command 'chown' r=0

<6>[    4.099683] init: command 'chmod' r=0

<6>[    4.099737] init: command 'chmod' r=0

<6>[    4.099791] init: command 'chmod' r=0

<6>[    4.099875] init: command 'chown' r=-2

<6>[    4.099947] init: command 'chmod' r=-2

<6>[    4.100019] init: command 'chown' r=-2

<6>[    4.100091] init: command 'chmod' r=-2

<6>[    4.100164] init: command 'chown' r=-2

<6>[    4.100237] init: command 'chmod' r=-2

<6>[    4.100310] init: command 'chown' r=-2

<6>[    4.100383] init: command 'chmod' r=-2

<6>[    4.100458] init: command 'chown' r=-2

<6>[    4.100528] init: command 'chmod' r=-2

<6>[    4.100601] init: command 'chown' r=-2

<6>[    4.100675] init: command 'chmod' r=-2

<6>[    4.100750] init: command 'chown' r=-2

<6>[    4.100823] init: command 'chown' r=-2

<6>[    4.100894] init: command 'chmod' r=-2

<6>[    4.100967] init: command 'chown' r=-2

<6>[    4.101040] init: command 'chmod' r=-2

<6>[    4.101122] init: command 'chown' r=0

<6>[    4.101186] init: command 'chmod' r=0

<6>[    4.101260] init: command 'chown' r=0

<6>[    4.101323] init: command 'chmod' r=0

<6>[    4.101399] init: command 'chown' r=0

<6>[    4.101462] init: command 'chmod' r=0

<6>[    4.101541] init: command 'chown' r=0

<6>[    4.101606] init: command 'chmod' r=0

<6>[    4.101682] init: command 'chown' r=0

<6>[    4.101744] init: command 'chmod' r=0

<6>[    4.101822] init: command 'chown' r=-2

<6>[    4.101887] init: command 'chown' r=-2

<6>[    4.101948] init: command 'chown' r=-2

<6>[    4.102008] init: command 'chown' r=-2

<6>[    4.102103] init: command 'chown' r=-2

<6>[    4.102166] init: command 'chown' r=-2

<6>[    4.102226] init: command 'chown' r=-2

<6>[    4.102285] init: command 'chown' r=-2

<6>[    4.102343] init: command 'chown' r=-2

<6>[    4.102403] init: command 'chown' r=-2

<6>[    4.102463] init: command 'chown' r=-2

<6>[    4.102523] init: command 'chown' r=-2

<6>[    4.102581] init: command 'chown' r=-2

<6>[    4.102640] init: command 'chown' r=-2

<6>[    4.102698] init: command 'chown' r=-2

<6>[    4.102758] init: command 'chown' r=-2

<6>[    4.102816] init: command 'chown' r=-2

<6>[    4.102879] init: command 'chown' r=-2

<6>[    4.102943] init: command 'chown' r=-2

<6>[    4.103028] init: command 'chown' r=0

<6>[    4.103097] init: command 'chown' r=0

<6>[    4.103164] init: command 'chown' r=0

<6>[    4.103232] init: command 'chown' r=0

<6>[    4.103326] init: command 'chown' r=0

<6>[    4.103395] init: command 'chown' r=0

<6>[    4.103490] init: command 'chown' r=0

<6>[    4.103608] init: command 'chmod' r=-30

<6>[    4.103688] init: command 'setprop' r=0

<6>[    4.103757] init: command 'setprop' r=0

<6>[    4.103825] init: command 'setprop' r=0

<6>[    4.103892] init: command 'setprop' r=0

<6>[    4.103960] init: command 'setprop' r=0

<6>[    4.104028] init: command 'setprop' r=0

<6>[    4.104097] init: command 'setprop' r=0

<6>[    4.104164] init: command 'setprop' r=0

<6>[    4.104232] init: command 'setprop' r=0

<6>[    4.104300] init: command 'setprop' r=0

<6>[    4.104369] init: command 'setprop' r=0

<6>[    4.104408] init: command 'setprop' r=0

<5>[    4.104484] init: starting 'servicemanager'

<5>[    4.104957] init: starting 'vold'

<6>[    4.105624] init: Created socket '/dev/socket/vold' with mode '660', user '0', group '1009'

<5>[    4.106400] init: starting 'pvrsrvctl'

<6>[    4.106719] init: command 'class_start' r=0

<5>[    4.106824] init: starting 'netd'

<5>[    4.107207] init: starting 'debuggerd'

<6>[    4.107499] init: Created socket '/dev/socket/mdns' with mode '660', user '0', group '1000'

<5>[    4.107534] init: starting 'updatesoftwinner'

<6>[    4.107631] init: Created socket '/dev/socket/dnsproxyd' with mode '660', user '0', group '3003'

<6>[    4.107764] init: Created socket '/dev/socket/netd' with mode '660', user '0', group '1000'

<5>[    4.107918] init: starting 'surfaceflinger'

<5>[    4.108355] init: starting 'zygote'

<5>[    4.108749] init: starting 'drm'

<6>[    4.109066] init: Created socket '/dev/socket/zygote' with mode '660', user '0', group '1000'

<5>[    4.109138] init: starting 'media'

<5>[    4.109521] init: starting 'installd'

<3>[    4.109906] init: cannot find '/system/etc/install-recovery.sh', disabling 'flash_recovery'

<6>[    4.110206] init: Created socket '/dev/socket/installd' with mode '600', user '1000', group '1000'

<5>[    4.119369] init: starting 'keystore'

<5>[    4.119844] init: starting 'ril-daemon'

<6>[    4.120176] init: Created socket '/dev/socket/keystore' with mode '666', user '0', group '0'

<5>[    4.120243] init: starting 'u3gmonitor'

<6>[    4.120515] init: Created socket '/dev/socket/rild-debug' with mode '660', user '1001', group '1000'

<5>[    4.120643] init: starting 'ttyusb-scan'

<6>[    4.120654] init: Created socket '/dev/socket/rild' with mode '660', user '0', group '1001'

<6>[    4.121007] init: command 'class_start' r=0

<6>[    4.121079] init: processing action 0x379d8 (boot)

<6>[    4.121178] init: command 'chmod' r=0

<6>[    4.121266] init: command 'chown' r=0

<6>[    4.121339] init: command 'chown' r=0

<6>[    4.121406] init: command 'chown' r=0

<6>[    4.121483] init: command 'chown' r=0

<6>[    4.121552] init: command 'chown' r=0

<6>[    4.121623] init: command 'chown' r=0

<6>[    4.121694] init: command 'chown' r=0

<6>[    4.121762] init: command 'chown' r=0

<6>[    4.121850] init: command 'chown' r=-2

<6>[    4.121914] init: command 'chown' r=0

<6>[    4.121975] init: command 'chmod' r=0

<6>[    4.122071] init: command 'chmod' r=0

<6>[    4.122138] init: command 'chmod' r=0

<6>[    4.122224] init: command 'chmod' r=0

<6>[    4.122318] init: command 'chmod' r=0

<6>[    4.122387] init: command 'chmod' r=0

<6>[    4.122457] init: command 'chmod' r=0

<6>[    4.122526] init: command 'chmod' r=0

<6>[    4.122629] init: command 'chmod' r=-2

<6>[    4.122699] init: command 'chmod' r=0

<4>[    4.153064] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6a)

<6>[    4.162156] usb 1-1: new high-speed USB device number 2 using sw-ehci

<4>[    4.172281] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6a)

<6>[    4.172301] init: command 'chown' r=0

<4>[    4.192292] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6b)

<4>[    4.212297] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6b)

<6>[    4.242291] init: command 'chmod' r=0

<6>[    4.242357] init: processing action 0x37f50 (queue_property_triggers)

<6>[    4.242467] init: command 'queue_property_triggers' r=0

<6>[    4.242491] init: processing action 0x2f5f8 (nonencrypted)

<6>[    4.242519] init: command 'class_start' r=0

<6>[    4.242540] init: processing action 0x2fa98 (property:ro.debuggable=1)

<5>[    4.242694] init: starting 'console'

<6>[    4.243204] init: command 'start' r=0

<6>[    4.243238] init: processing action 0x32c80 (property:persist.sys.usb.config=*)

<6>[    4.243335] init: command 'setprop' r=0

<6>[    4.243452] init: command 'setprop' r=0

<6>[    4.243477] init: processing action 0x32358 (property:sys.usb.config=none)

<6>[    4.243534] init: command 'stop' r=0

<6>[    4.243696] init: command 'write' r=0

<6>[    4.243835] init: command 'write' r=0

<6>[    4.243899] init: command 'setprop' r=0

<6>[    4.243923] init: processing action 0x368f8 (property:sys.usb.config=mass_storage,adb)

<6>[    4.244024] init: command 'write' r=0

<6>[    4.244136] init: command 'write' r=0

<6>[    4.244269] init: command 'write' r=0

<6>[    4.244395] init: command 'write' r=0

<6>[    4.244498] init: command 'write' r=0

<5>[    4.244535] init: starting 'adbd'

<6>[    4.244905] init: command 'start' r=0

<6>[    4.244989] init: command 'setprop' r=0

<6>[    4.245684] init: Created socket '/dev/socket/adbd' with mode '660', user '1000', group '1000'

<6>[    4.247348] adb_open

<4>[    4.247387] ep_matches, wrn: endpoint already claimed, ep(0xc07fdf64, 0xeeafd480, ep1-bulk)

<6>[    4.247406] adb_bind_config

<4>[    4.247423] ep_matches, wrn: endpoint already claimed, ep(0xc07fdf64, 0xeeafd480, ep1-bulk)

<4>[    4.247440] ep_matches, wrn: endpoint already claimed, ep(0xc07fdfb0, 0xeeafd480, ep2-bulk)

<4>[    4.247459] ep_matches, wrn: endpoint already claimed, ep(0xc07fdf64, 0xeeafd480, ep1-bulk)

<4>[    4.247476] ep_matches, wrn: endpoint already claimed, ep(0xc07fdfb0, 0xeeafd480, ep2-bulk)

<4>[    4.247493] ep_matches, wrn: endpoint already claimed, ep(0xc07fdffc, 0xeeaebe00, ep3-bulk)

<4>[    4.247514] [sw_udc]: alloc request: ep(0xc07fe048, ep4-bulk, 512), req(0xee55a4c0)

<4>[    4.247539] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xee55a440)

<4>[    4.247563] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xee55a3c0)

<4>[    4.247585] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xee55a340)

<4>[    4.247607] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xee55a2c0)

<4>[    4.247647] [sw_udc]: sw_udc_pullup, is_on = 1

<4>[    4.247672] [sun6i_usb]: usb device is not active

<6>[    4.303981] init: waitpid returned pid 1295, status = 00000000

<5>[    4.304011] init: process 'pvrsrvctl', pid 1295 exited

<6>[    4.315999] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<5>[    4.810718] init: starting 'bootanim'

<4>[    4.810758] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[    5.072640] [sun6i_usb]: set ctrl gpio off

<6>[    9.086221] warning: `zygote' uses 32-bit capabilities (legacy support in use)

<6>[    9.212891] gsensor_detect: addr= 1c

<4>[    9.213316] gsensor_detect: mma8452 equipment is detected!

<6>[    9.215262] mma8452 2-001d: build time Nov  4 2013 19:17:35

<6>[    9.215809] input: mma8452 as /devices/virtual/input/input3

<4>[    9.282561] i2c-core: driver [gslX680] using legacy suspend method

<4>[    9.282582] i2c-core: driver [gslX680] using legacy resume method

<6>[    9.283864] input: gslX680 as /devices/platform/sun6i-i2c.1/i2c-1/1-0040/input/input4

<6>[    9.285047] init: processing action 0x2fcd0 (property:sys.sensors=1)

<5>[    9.285181] init: starting 'sensors'

<6>[    9.285608] init: command 'start' r=0

<6>[    9.348107] init: waitpid returned pid 2050, status = 00000a00

<5>[    9.348137] init: process 'sensors', pid 2050 exited

<4>[   11.132565] [sun6i_usb]: set ctrl gpio on

<6>[   16.581078] request_suspend_state: wakeup (3->0) at 16569025176 (2014-01-14 04:11:58.707681632 UTC)

<6>[   18.839760] EXT4-fs (dm-0): mounted filesystem without journal. Opts: (null)

<6>[   18.929394] EXT4-fs (dm-0): re-mounted. Opts: (null)

<6>[   18.934897] EXT4-fs (dm-0): re-mounted. Opts: (null)

<6>[   20.077146] acc_open

<6>[   20.077178] acc_release

<4>[   20.554737] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[   21.085148] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<6>[   22.291475] EXT4-fs (dm-1): mounted filesystem without journal. Opts: (null)

<6>[   22.567131] EXT4-fs (dm-1): re-mounted. Opts: (null)

<6>[   22.574601] EXT4-fs (dm-1): re-mounted. Opts: (null)

<6>[   22.764679] EXT4-fs (dm-2): mounted filesystem without journal. Opts: (null)

<4>[   22.878061] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[   22.887943] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[   22.894899] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<6>[   23.072505] EXT4-fs (dm-2): re-mounted. Opts: (null)

<6>[   23.090841] EXT4-fs (dm-2): re-mounted. Opts: (null)

<4>[   23.753032] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[   24.417114] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<4>[   24.475804] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<4>[   24.629636] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[   24.686801] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[   25.662997] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[   26.137383] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[   27.873637] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<4>[   27.956864] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<6>[   28.072840] init: processing action 0x312c0 (property:sys.boot_completed=1)

<5>[   28.073177] init: starting 'preinstall'

<6>[   28.075001] init: command 'start' r=0

<6>[   28.450994] init: waitpid returned pid 3005, status = 00000000

<5>[   28.451043] init: process 'preinstall', pid 3005 exited

<4>[   28.489816] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<3>[   28.601183] init: sys_prop: permission denied uid:1003  name:service.bootanim.exit

<6>[   28.734066] init: waitpid returned pid 1827, status = 00000000

<5>[   28.734102] init: process 'bootanim', pid 1827 exited

<4>[   29.389122] [rfkill]: rfkill set power 1

<4>[   29.389151] [rtl8723au]: rtl8723au is powered down by bt

<4>[   29.389168] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[   29.404948] [rfkill]: rfkill set power 0

<4>[   29.404972] [rtl8723au]: rtl8723au is powered up by bt

<4>[   29.404989] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_enable_ehci

<4>[   29.405012] [sw_hci_sun6i]: [sw-ehci1]: probe, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<4>[   29.405037] [sw_hci_sun6i]: [sw-ehci1]: open clock

<4>[   29.405269] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power ON

<6>[   29.405287] sw-ehci sw-ehci.1: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[   29.405350] sw-ehci sw-ehci.1: new USB bus registered, assigned bus number 3

<6>[   29.405499] sw-ehci sw-ehci.1: irq 104, io mem 0xf1c1a000

<6>[   29.422102] sw-ehci sw-ehci.1: USB 0.0 started, EHCI 1.00

<4>[   29.422126] ehci_irq: highspeed device connect

<6>[   29.423703] hub 3-0:1.0: USB hub found

<6>[   29.423742] hub 3-0:1.0: 1 port detected

<4>[   29.424559] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[   29.424579] [rtl8723au]: rtl8723au power state change: wifi 0, bt 1 !!

<6>[   29.642814] rtk_btusb: btfcd open

<6>[   29.642825] 

<3>[   29.642841] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[   29.742134] usb 3-1: new high-speed USB device number 2 using sw-ehci

<6>[   29.847968] rtk_btusb: btfcd open

<6>[   29.847983] 

<3>[   29.847998] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[   29.894781] rtk_btusb: btusb_probe 1==========can_wakeup=1	 flag2=0

<6>[   29.894798] rtk_btusb: patch_add

<6>[   29.894830] rtk_btusb: hci_register_dev eca4b000 name  bus 1

<6>[   29.894843] rtk_btusb: id=0 

<6>[   29.894854] rtk_btusb: hdev->name=hci0 

<3>[   29.894863] rtk_btusb:  ===================hci_register_dev success

<6>[   30.053161] rtk_btusb: btfcd open

<6>[   30.053174] 

<6>[   30.053202] rtk_btusb: btusb_open start pm_usage_cnt(0x0)

<6>[   30.053215] rtk_btusb: download_patch start

<6>[   30.054677] rtk_btusb: check_fw_version : read_ver_rsp->lmp_subver = 0x1200

<6>[   30.054693] rtk_btusb: load_firmware

<6>[   31.041027] rtk_btusb: check_fw_version : read_ver_rsp->lmp_subver = 0x963e

<6>[   31.041049] rtk_btusb: Rtk patch end 0

<6>[   31.041406] rtk_btusb: btusb_open end  pm_usage_cnt(0x0)

<6>[   31.604346] rtk_btusb: btfcd close

<6>[   31.604356] 

<6>[   31.604376] rtk_btusb: btusb_flush add delay 

<6>[   31.616324] rtk_btusb: btusb_close

<4>[   31.639293] [rfkill]: rfkill set power 1

<4>[   31.639332] [rtl8723au]: rtl8723au is powered down by bt

<4>[   31.639356] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_disable_ehci

<4>[   31.639386] [sw_hci_sun6i]: [sw-ehci1]: remove, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<6>[   31.639440] sw-ehci sw-ehci.1: remove, state 1

<6>[   31.639487] usb usb3: USB disconnect, device number 1

<6>[   31.639508] usb 3-1: USB disconnect, device number 2

<6>[   31.639914] rtk_btusb: btusb_disconnect

<6>[   31.639931] rtk_btusb: patch_remove

<6>[   31.639952] rtk_btusb: hci_unregister_dev hdeveca4b000 name hci0 bus 1

<6>[   31.639968] rtk_btusb: btusb_flush add delay 

<6>[   31.688673] sw-ehci sw-ehci.1: USB bus 3 deregistered

<4>[   31.688716] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power OFF

<4>[   31.688733] [sw_hci_sun6i]: [sw-ehci1]: close clock

<4>[   31.688764] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[   31.688779] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<6>[   32.316293] init: waitpid returned pid 3116, status = 00000000

<3>[   32.316328] init: untracked pid 3116 exited

<5>[   36.083550] CPU2: shutdown

<6>[   36.083572] [hotplug]: cpu(3) try to kill cpu(2)

<6>[   36.103106] [hotplug]: cpu2 is killed! .

<5>[   36.105691] CPU3: shutdown

<6>[   36.105716] [hotplug]: cpu(0) try to kill cpu(3)

<6>[   36.123091] [hotplug]: cpu3 is killed! .

<4>[   36.712910] CPU2: Booted secondary processor

<6>[   36.712971] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[   36.743157] Calibrating delay loop (skipped) already calibrated this CPU

<5>[   46.079854] CPU1: shutdown

<6>[   46.079974] [hotplug]: cpu(2) try to kill cpu(1)

<6>[   46.093484] [hotplug]: cpu1 is killed! .

<5>[   46.107881] CPU2: shutdown

<6>[   46.108009] [hotplug]: cpu(0) try to kill cpu(2)

<6>[   46.123491] [hotplug]: cpu2 is killed! .

<4>[   46.662281] [sun6i_usb]: 

<4>[   46.662337] 

<4>[   46.662366] insmod_device_driver

<4>[   46.662402] 

<4>[   46.662497] [sw_udc]: sw_usb_device_enable start

<4>[   46.662599] [sw_udc]: usb_vbase  = 0xf1c19000

<4>[   46.662692] [sw_udc]: sram_vbase = 0xf1c00000

<4>[   46.662978] [sw_udc]: open_usb_clock

<4>[   46.663363] [sw_udc]: usbd_stop_work

<4>[   46.663510] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_1 dma_hdle[1] = 0xc0831108

<4>[   46.663664] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_2 dma_hdle[2] = 0xc083118c

<4>[   46.663817] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_3 dma_hdle[3] = 0xc0831210

<4>[   46.663970] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_4 dma_hdle[4] = 0xc0831294

<4>[   46.664124] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_5 dma_hdle[5] = 0xc0831318

<4>[   46.664450] [sw_udc]: CONFIG_USB_GADGET_DUALSPEED: USBC_TS_MODE_HS

<4>[   46.664560] [sw_udc]: usbd_start_work

<4>[   46.664642] [sw_udc]: usbd_start_work

<4>[   46.664723] [sw_udc]: sw_usb_device_enable end

<4>[   46.720109] [sw_udc]: IRQ: suspend

<4>[   46.720189] [sw_udc]: ERR: usb speed is unkown

<4>[   47.028182] CPU1: Booted secondary processor

<6>[   47.028243] Calibrating delay loop (skipped) already calibrated this CPUCPU2: Booted secondary processor

<6>[   47.043996] Calibrating delay loop (skipped) already calibrated this CPU[sw_udc]: IRQ: reset

<4>[   47.140290] (1:star,2:end): vfs_read:0, vfs_write:0,dma_working:0,amount:0,file_offset:0

<4>[   47.140313] [sw_udc]: irq: reset happen, throw away all urb

<4>[   47.197304] [sw_udc]: 

<4>[   47.197320] +++++++++++++++++++++++++++++++++++++

<4>[   47.197337] [sw_udc]:  usb enter high speed.

<4>[   47.197346] [sw_udc]: 

<4>[   47.197350] +++++++++++++++++++++++++++++++++++++

<6>[   47.197996] android_work: sent uevent USB_STATE=CONNECTED

<4>[   47.202433] [sw_udc]: IRQ: reset

<4>[   47.202462] (1:star,2:end): vfs_read:0, vfs_write:0,dma_working:0,amount:0,file_offset:0

<4>[   47.202479] [sw_udc]: irq: reset happen, throw away all urb

<4>[   47.239311] [sw_udc]: Set address 2

<6>[   47.311900] android_usb gadget: high-speed config #1: android

<4>[   47.312106] [sw_udc]: ep enable: ep3(0xc07fdffc, ep3-bulk, 128, 512)

<4>[   47.312157] [sw_udc]: ep enable: ep4(0xc07fe048, ep4-bulk, 0, 512)

<4>[   47.312267] [sw_udc]: ep enable: ep1(0xc07fdf64, ep1-bulk, 128, 512)

<4>[   47.312298] [sw_udc]: ep enable: ep2(0xc07fdfb0, ep2-bulk, 0, 512)

<4>[   47.312331] [sw_udc]: alloc request: ep(0xc07fdf64, ep1-bulk, 512), req(0xec843940)

<4>[   47.312357] [sw_udc]: alloc request: ep(0xc07fdfb0, ep2-bulk, 512), req(0xec31adc0)

<4>[   47.312390] [sw_udc]: alloc request: ep(0xc07fdf64, ep1-bulk, 512), req(0xec1001c0)

<4>[   47.312425] [sw_udc]: alloc request: ep(0xc07fdfb0, ep2-bulk, 512), req(0xedc64ec0)

<6>[   47.315007] android_work: sent uevent USB_STATE=CONFIGURED

<4>[   47.383078] [sun6i_usb]: nuke: ep num is 0

<4>[   47.525454] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<5>[   48.753520] CPU1: shutdown

<6>[   48.753543] [hotplug]: cpu(2) try to kill cpu(1)

<6>[   48.773088] [hotplug]: cpu1 is killed! .

<5>[   48.775425] CPU2: shutdown

<6>[   48.775448] [hotplug]: cpu(3) try to kill cpu(2)

<6>[   48.793091] [hotplug]: cpu2 is killed! .

<6>[   94.375651] EXT4-fs (nandd): re-mounted. Opts: (null)

