#######

<4>[35345.765630] [IIS]Entered sun6i_i2s_resume

<4>[35345.765833] [PCM]Entered sun6i_pcm_resume

<7>[35345.765875] gpu:open gpu power!

<6>[35345.785424] PM: resume of devices complete after 188.286 msecs

<6>[35345.785674] PM: resume devices took 0.190 seconds

<4>[35345.785757] [pm]aw_pm_end!

<7>[35345.785770] PM: Finishing wakeup.

<4>[35345.785783] Restarting tasks ... 

<6>[35345.789555] usb 1-1: USB disconnect, device number 69

<6>[35345.791265] init: waitpid returned pid 26675, status = 00000000

<3>[35345.791298] init: untracked pid 26675 exited

<6>[35345.799144] request_suspend_state: wakeup (3->0) at 35345783997855 (2014-01-13 09:34:35.053762541 UTC)

<4>[35345.800442] done.

<4>[35345.800484] sunxi cpufreq resume ok

<6>[35345.800541] suspend: exit suspend, ret = 0 (2014-01-13 09:34:35.055171416 UTC)

<6>[35345.800597] [HDMI]Hdmi_late_resume

<6>[35345.800677] [DISP]>>display late resume done<<

<4>[35345.800694] ts->is_suspended:1

<5>[35345.800708] [VFE]vfe_resume

<5>[35345.800773] [VFE]vfe resume work start!

<5>[35345.802086] [VFE]mclk on

<4>[35345.802583] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35345.814152] [VFE_WARN]invalid gpio

<4>[35345.842970] CPU2: Booted secondary processor

<6>[35345.843029] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35345.868111] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35345.892498] [VFE]sensor full initial success when resume from suspend!

<4>[35345.892801] [OV5647]disalbe oe!

<5>[35345.908820] [VFE]mclk on

<4>[35345.920920] [VFE_WARN]invalid gpio

<4>[35345.965779] [CSI][GC2035]V4L2_IDENT_SENSOR=2035

<5>[35346.159577] [VFE]sensor full initial success when resume from suspend!

<4>[35346.159651] [CSI][GC2035]disalbe oe!

<5>[35346.171975] [VFE]mclk off

<5>[35346.172084] [VFE]vfe resume work end!

<4>[35348.775218] do_wake

<4>[35348.775248] [sw_module]: usi6276 modem wakeup

<4>[35349.332723] ehci_irq: highspeed device connect

<6>[35349.605599] usb 1-1: new high-speed USB device number 70 using sw-ehci

<6>[35349.775720] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<5>[35351.303194] CPU2: shutdown

<6>[35351.303319] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35351.316551] [hotplug]: cpu2 is killed! .

<5>[35351.331054] CPU3: shutdown

<6>[35351.331175] [hotplug]: cpu(1) try to kill cpu(3)

<6>[35351.346566] [hotplug]: cpu3 is killed! .

<6>[35351.843265] init: waitpid returned pid 26924, status = 00000000

<3>[35351.843466] init: untracked pid 26924 exited

<4>[35390.735905] CPU2: Booted secondary processor

<6>[35390.735959] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35390.756831] Calibrating delay loop (skipped) already calibrated this CPU

<4>[35391.847800] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<4>[35391.898301] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<4>[35394.176188] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<5>[35396.193669] CPU1: shutdown

<6>[35396.193790] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35396.206594] [hotplug]: cpu1 is killed! .

<5>[35396.219951] CPU3: shutdown

<6>[35396.220071] [hotplug]: cpu(2) try to kill cpu(3)

<6>[35396.236598] [hotplug]: cpu3 is killed! .

<4>[35417.663866] CPU1: Booted secondary processor

<6>[35417.663964] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35417.690517] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35418.902282] CPU1: shutdown

<6>[35418.902403] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35418.916551] [hotplug]: cpu1 is killed! .

<5>[35418.928716] CPU3: shutdown

<6>[35418.928840] [hotplug]: cpu(2) try to kill cpu(3)

<6>[35418.946693] [hotplug]: cpu3 is killed! .

<4>[35432.529248] CPU1: Booted secondary processor

<6>[35432.529305] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35432.540100] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35433.792338] CPU1: shutdown

<6>[35433.792460] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35433.806562] [hotplug]: cpu1 is killed! .

<5>[35433.818194] CPU3: shutdown

<6>[35433.818314] [hotplug]: cpu(2) try to kill cpu(3)

<6>[35433.836602] [hotplug]: cpu3 is killed! .

<4>[35441.949116] CPU1: Booted secondary processor

<6>[35441.949177] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35441.973253] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35443.293134] CPU1: shutdown

<6>[35443.293253] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35443.306586] [hotplug]: cpu1 is killed! .

<5>[35443.319112] CPU3: shutdown

<6>[35443.319231] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35443.336649] [hotplug]: cpu3 is killed! .

<4>[35446.240111] CPU1: Booted secondary processor

<6>[35446.240170] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35446.263517] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35447.632891] CPU1: shutdown

<6>[35447.633013] [hotplug]: cpu(3) try to kill cpu(1)

<6>[35447.646678] [hotplug]: cpu1 is killed! .

<5>[35447.658745] CPU3: shutdown

<6>[35447.658869] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35447.676660] [hotplug]: cpu3 is killed! .

<4>[35452.119463] CPU1: Booted secondary processor

<6>[35452.119525] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35452.143743] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35453.442919] CPU1: shutdown

<6>[35453.443039] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35453.456542] [hotplug]: cpu1 is killed! .

<5>[35453.469417] CPU3: shutdown

<6>[35453.469537] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35453.486649] [hotplug]: cpu3 is killed! .

<4>[35466.118468] CPU1: Booted secondary processor

<6>[35466.118524] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35466.140845] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35467.442821] CPU1: shutdown

<6>[35467.442943] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35467.456538] [hotplug]: cpu1 is killed! .

<5>[35467.468754] CPU3: shutdown

<6>[35467.468874] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35467.486814] [hotplug]: cpu3 is killed! .

<4>[35470.810564] CPU1: Booted secondary processor

<6>[35470.810624] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35470.834982] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35472.142935] CPU1: shutdown

<6>[35472.143058] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35472.156566] [hotplug]: cpu1 is killed! .

<5>[35472.168669] CPU3: shutdown

<6>[35472.168912] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35472.186648] [hotplug]: cpu3 is killed! .

<4>[35474.938442] CPU1: Booted secondary processor

<6>[35474.938496] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35474.961068] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35476.263010] CPU1: shutdown

<6>[35476.263129] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35476.276513] [hotplug]: cpu1 is killed! .

<5>[35476.288975] CPU3: shutdown

<6>[35476.289098] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35476.306662] [hotplug]: cpu3 is killed! .

<4>[35587.828615] CPU1: Booted secondary processor

<6>[35587.828674] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35587.839753] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35590.363013] CPU1: shutdown

<6>[35590.363134] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35590.376552] [hotplug]: cpu1 is killed! .

<5>[35590.388222] CPU3: shutdown

<6>[35590.388340] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35590.406762] [hotplug]: cpu3 is killed! .

<4>[35594.803582] CPU1: Booted secondary processor

<6>[35594.803765] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35594.839412] Calibrating delay loop (skipped) already calibrated this CPU

<4>[35595.017871] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35595.019091] [pm]valid

<6>[35595.019264] request_suspend_state: sleep (0->3) at 35595004067890 (2014-01-13 09:38:44.273814451 UTC)

<5>[35595.021477] [VFE]vfe_suspend

<5>[35595.021576] [VFE]set camera to power off!

<5>[35595.021693] [VFE]mclk off

<4>[35595.021783] [VFE_WARN]invalid gpio

<4>[35595.033671] [VFE_WARN]invalid gpio

<4>[35595.045458] [VFE_WARN]invalid gpio

<5>[35595.058373] [VFE]mclk off

<5>[35595.058503] [VFE]vfe_suspend done!

<6>[35595.815202] [HDMI]Hdmi_early_suspend

<6>[35595.815253] [DISP]>>display early suspend done<<

<6>[35595.815490] active wake lock sync_system

<4>[35595.834961] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[35595.883280] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[35595.907898] [pm]valid

<6>[35595.907936] PM: Syncing filesystems ... done.

<7>[35595.912528] PM: Preparing system for mem sleep

<4>[35595.912592] sunxi cpufreq suspend ok

<4>[35595.912648] Freezing user space processes ... (elapsed 0.02 seconds) done.

<4>[35595.935792] Freezing remaining freezable tasks ... (elapsed 0.01 seconds) done.

<7>[35595.955750] PM: Entering mem sleep

<4>[35595.955780] [pm]3 state begin

<4>[35595.957961] Suspending console(s) (use no_console_suspend to debug)

<7>[35595.959036] gpu:close gpu power!

<4>[35595.959259] [PCM]Entered sun6i_pcm_suspend

<4>[35595.959709] [IIS]Entered sun6i_i2s_suspend

<6>[35595.960215] [DISP]>>disp super standby enter<<

<4>[35595.960381] [sw_module]: usi6276 modem sleep

<6>[35595.960593] [HDMI]Hdmi_suspend

<4>[35595.960776] [audio codec]:suspend

<4>[35596.185197] [audio codec]:suspend end

<4>[35596.423705] ehci_irq: highspeed device disconnect

<4>[35596.705307] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35596.706382] [mmc]: smc 1 suspend

<4>[35596.706422] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35596.707500] [mmc]: smc 0 suspend

<6>[35596.707730] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35596.707749] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:45

<6>[35596.707779] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35596.707798] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:45

<6>[35596.707814] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35596.707831] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:45

<6>[35596.707851] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35596.707868] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:45

<6>[35596.707896] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35596.707914] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:45

<4>[35596.708984] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_suspend

<4>[35596.709004] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power OFF

<4>[35596.709019] [sw_hci_sun6i]: [sw-ehci2]: close clock

<4>[35596.709052] [sw_hci_sun6i]: ERR: hcd is null

<4>[35596.709307] [uart]: uart3 suspend

<4>[35596.709363] [uart]: uart2 suspend

<4>[35596.709389] [uart]: uart0 suspend

<4>[35596.709793] [sw_hcd0]: sw_hcd_suspend start

<4>[35596.709806] [sun6i_usb]: wrn: hcd is disable, need not enter to suspend

<4>[35596.709834] [sw_udc]: sw_udc_suspend start

<4>[35596.709845] [sw_udc]: udc is disable, need not enter to suspend

<4>[35596.711545] [i2c2] suspend okay.. 

<4>[35596.711574] [i2c1] suspend okay.. 

<4>[35596.711602] [i2c0] suspend okay.. 

<4>[35596.711787] [NAND] nand_suspend super

<6>[35596.712098] PM: suspend of devices complete after 753.492 msecs

<6>[35596.712116] PM: suspend devices took 0.750 seconds

<4>[35596.712128] [pm]prepare

<6>[35596.712649] PM: late suspend of devices complete after 0.505 msecs

<4>[35596.712662] [pm]prepare_late

<4>[35596.712673] Disabling non-boot CPUs ...

<5>[35596.714285] CPU1: shutdown

<6>[35596.714303] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35596.726231] [hotplug]: cpu1 is killed! .

<5>[35596.728772] CPU2: shutdown

<6>[35596.728789] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35596.746226] [hotplug]: cpu2 is killed! .

<5>[35596.748841] CPU3: shutdown

<6>[35596.748860] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35596.766223] [hotplug]: cpu3 is killed! .

<4>[35596.767517] [pm]enter state 3

<6>[35596.767517] resume_pointer = 0xc0052918. 

<4>[35596.767517] scence_lock: 

<4>[35596.767517] wakeup_src 0x2000

<4>[35596.767517] wakeup_gpio_map 0x1020

<4>[35596.767517] wakeup_gpio_group 0x0

<6>[35596.767517] resume1_bin_start = 0xc0056220, resume1_bin_end = 0xc0058a20. 

<6>[35596.767517] resume_code_src = 0x40056220, resume_code_length = 10240. resume_code_length = 2800 

<4>[35596.767517] arch/arm/mach-sun6i/pm/./pm.c, aw_super_standby, 635. 

<6>[35596.767517] suspend_status_flag = 0. 

<4>[35596.767517] [pm]platform wakeup, super standby wakesource is:0x400

<6>[35596.767528] Suspended for 0.000 seconds

<6>[35596.767616] Enabling non-boot CPUs ...

<4>[35596.800516] CPU1: Booted secondary processor

<6>[35596.800577] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35596.801472] CPU1 is up

<4>[35596.834135] CPU2: Booted secondary processor

<6>[35596.834197] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35596.835075] CPU2 is up

<4>[35596.847707] CPU3: Booted secondary processor

<6>[35596.847764] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35596.848503] CPU3 is up

<4>[35596.848516] [pm]platform wakeup.

<6>[35596.849036] PM: early resume of devices complete after 0.500 msecs

<4>[35596.849269] [pm]platform wakeup finish

<4>[35596.849493] [NAND] nand_resume super

<4>[35596.852467] [i2c0] resume okay.. 

<4>[35596.852491] [i2c1] resume okay.. 

<4>[35596.852515] [i2c2] resume okay.. 

<6>[35596.854182] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35596.854221] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:49

<6>[35596.854244] wakeup wake lock: alarm_rtc

<6>[35596.854333] [DISP]>>disp super standby exit<<

<4>[35596.854349] battery vol change: 16->17 

<6>[35596.854467] [HDMI]Hdmi_resume

<4>[35596.857387] [sw_udc]: sw_udc_resume start

<4>[35596.857400] [sw_udc]: udc is disable, need not enter to resume

<4>[35596.857416] [sw_hcd0]: sw_hcd_resume start

<4>[35596.857426] [sun6i_usb]: wrn: hcd is disable, need not resume

<4>[35596.857663] [uart]: uart0 resume

<4>[35596.857682] [uart]: uart2 resume

<4>[35596.857727] [uart]: uart3 resume

<4>[35596.857834] [sw_hci_sun6i]: ERR: hcd is null

<4>[35596.857850] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_resume

<4>[35596.857862] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[35596.858089] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<4>[35596.858101] [sw_hci_sun6i]: [sw-ehci2]: lost power, restarting

<4>[35596.858116] usb usb1: root hub lost power or was reset

<6>[35596.865205] [DISP]>>disp_resume call<<

<4>[35596.947685] [LCD] ANX9804 Chip found

<4>[35596.950473] [LCD] ANX9804 clock is stable.

<6>[35597.005408] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35597.005425] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:49

<4>[35597.010526] [mmc]: smc 0 resume

<4>[35597.010542] [mmc]: smc 1 resume

<4>[35597.010695] [audio codec]:resume start

<4>[35597.010714] [audio codec]:resume end

<4>[35597.010937] [rfkill]: rfkill set power 1

<4>[35597.010952] [rtl8723au]: rtl8723au is powered down by bt

<4>[35597.010964] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[35597.025729] [IIS]Entered sun6i_i2s_resume

<4>[35597.025986] [PCM]Entered sun6i_pcm_resume

<7>[35597.026020] gpu:open gpu power!

<6>[35597.045484] PM: resume of devices complete after 196.196 msecs

<6>[35597.045740] PM: resume devices took 0.200 seconds

<4>[35597.046037] [pm]aw_pm_end!

<7>[35597.046051] PM: Finishing wakeup.

<4>[35597.046063] Restarting tasks ... 

<6>[35597.046229] usb 1-1: USB disconnect, device number 70

<4>[35597.057847] done.

<4>[35597.057899] sunxi cpufreq resume ok

<6>[35597.057966] suspend: exit suspend, ret = 0 (2014-01-13 09:38:49.052550957 UTC)

<6>[35597.057999] active wake lock alarm_rtc, time left 79

<6>[35597.058013] active wake lock unknown_wakeups, time left 500

<5>[35599.262726] CPU1: shutdown

<6>[35599.262848] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35599.276556] [hotplug]: cpu1 is killed! .

<5>[35599.288606] CPU3: shutdown

<6>[35599.288724] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35599.306663] [hotplug]: cpu3 is killed! .

<4>[35600.036173] do_wake

<4>[35600.036276] [sw_module]: usi6276 modem wakeup

<4>[35600.593683] ehci_irq: highspeed device connect

<6>[35600.865595] usb 1-1: new high-speed USB device number 71 using sw-ehci

<6>[35601.040163] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<4>[35602.081699] [pm]valid

<6>[35602.081917] PM: Syncing filesystems ... done.

<7>[35602.097287] PM: Preparing system for mem sleep

<4>[35602.097473] sunxi cpufreq suspend ok

<4>[35602.097645] Freezing user space processes ... (elapsed 0.04 seconds) done.

<4>[35602.147229] Freezing remaining freezable tasks ... (elapsed 0.01 seconds) done.

<7>[35602.167214] PM: Entering mem sleep

<4>[35602.167311] [pm]3 state begin

<4>[35602.169601] Suspending console(s) (use no_console_suspend to debug)

<7>[35602.170768] gpu:close gpu power!

<4>[35602.170986] [PCM]Entered sun6i_pcm_suspend

<4>[35602.171417] [IIS]Entered sun6i_i2s_suspend

<4>[35602.172022] [sw_module]: usi6276 modem sleep

<4>[35602.172418] [audio codec]:suspend

<4>[35602.395223] [audio codec]:suspend end

<4>[35602.637231] ehci_irq: highspeed device disconnect

<6>[35602.905238] [DISP]>>disp super standby enter<<

<6>[35602.905547] [HDMI]Hdmi_suspend

<4>[35602.915334] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35602.916406] [mmc]: smc 1 suspend

<4>[35602.916447] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35602.917525] [mmc]: smc 0 suspend

<6>[35602.917762] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35602.917780] sun6i-rtc sun6i-rtc: read time 2014-1-13 9:38:55

<4>[35602.919257] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_suspend

<4>[35602.919276] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power OFF

<4>[35602.919292] [sw_hci_sun6i]: [sw-ehci2]: close clock

<4>[35602.919326] [sw_hci_sun6i]: ERR: hcd is null

<4>[35602.919578] [uart]: uart3 suspend

<4>[35602.919633] [uart]: uart2 suspend

<4>[35602.919659] [uart]: uart0 suspend

<4>[35602.920055] [sw_hcd0]: sw_hcd_suspend start

<4>[35602.920067] [sun6i_usb]: wrn: hcd is disable, need not enter to suspend

<4>[35602.920095] [sw_udc]: sw_udc_suspend start

<4>[35602.920106] [sw_udc]: udc is disable, need not enter to suspend

<4>[35602.921790] [i2c2] suspend okay.. 

<4>[35602.921819] [i2c1] suspend okay.. 

<4>[35602.921847] [i2c0] suspend okay.. 

<4>[35602.922034] [NAND] nand_suspend super

<6>[35602.922310] PM: suspend of devices complete after 752.065 msecs

<6>[35602.922327] PM: suspend devices took 0.750 seconds

<4>[35602.922339] [pm]prepare

<6>[35602.922845] PM: late suspend of devices complete after 0.489 msecs

<4>[35602.922858] [pm]prepare_late

<4>[35602.922869] Disabling non-boot CPUs ...

<5>[35602.924503] CPU2: shutdown

<6>[35602.924521] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35602.936270] [hotplug]: cpu2 is killed! .

<4>[35602.937514] [pm]enter state 3

<6>[35602.937514] resume_pointer = 0xc0052918. 

<4>[35602.937514] scence_lock: 

<4>[35602.937514] wakeup_src 0x2000

<4>[35602.937514] wakeup_gpio_map 0x1020

<4>[35602.937514] wakeup_gpio_group 0x0

<6>[35602.937514] resume1_bin_start = 0xc0056220, resume1_bin_end = 0xc0058a20. 

<6>[35602.937514] resume_code_src = 0x40056220, resume_code_length = 10240. resume_code_length = 2800 

<4>[35602.937514] arch/arm/mach-sun6i/pm/./pm.c, aw_super_standby, 635. 

<6>[35602.937514] suspend_status_flag = 0. 

<4>[35602.937514] [pm]platform wakeup, super standby wakesource is:0x40

<6>[35602.937526] Suspended for 0.000 seconds

<6>[35602.937611] Enabling non-boot CPUs ...

<4>[35602.970212] CPU2: Booted secondary processor

<6>[35602.970273] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35602.971013] CPU2 is up

<4>[35602.971027] [pm]platform wakeup.

<6>[35602.971545] PM: early resume of devices complete after 0.499 msecs

<4>[35602.976797] [pm]platform wakeup finish

<6>[35602.977206] [DISP]>>disp super standby exit<<

<4>[35602.977241] [NAND] nand_resume super

<6>[35602.977342] [HDMI]Hdmi_resume

<4>[35602.980222] [i2c0] resume okay.. 

<4>[35602.980246] [i2c1] resume okay.. 

<4>[35602.980269] [i2c2] resume okay.. 

<4>[35602.981652] battery vol change: 17->41 

<6>[35602.981697] wakeup wake lock: event0-2018

<4>[35602.984440] [sw_udc]: sw_udc_resume start

<4>[35602.984452] [sw_udc]: udc is disable, need not enter to resume

<4>[35602.984469] [sw_hcd0]: sw_hcd_resume start

<4>[35602.984479] [sun6i_usb]: wrn: hcd is disable, need not resume

<4>[35602.984712] [uart]: uart0 resume

<4>[35602.984731] [uart]: uart2 resume

<4>[35602.984777] [uart]: uart3 resume

<4>[35602.984883] [sw_hci_sun6i]: ERR: hcd is null

<4>[35602.984899] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_resume

<4>[35602.984911] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[35602.985138] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<4>[35602.985150] [sw_hci_sun6i]: [sw-ehci2]: lost power, restarting

<4>[35602.985167] usb usb1: root hub lost power or was reset

<6>[35602.995293] [DISP]>>disp_resume call<<

<4>[35603.077876] [LCD] ANX9804 Chip found

<4>[35603.080660] [LCD] ANX9804 clock is stable.

<6>[35603.125424] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35603.125441] sun6i-rtc sun6i-rtc: read time 2014-1-13 10:12:3

<4>[35603.130571] [mmc]: smc 0 resume

<4>[35603.130587] [mmc]: smc 1 resume

<4>[35603.130721] [audio codec]:resume start

<4>[35603.130741] [audio codec]:resume end

<4>[35603.130827] [rfkill]: rfkill set power 1

<4>[35603.130842] [rtl8723au]: rtl8723au is powered down by bt

<4>[35603.130854] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[35603.145717] [IIS]Entered sun6i_i2s_resume

<4>[35603.145929] [PCM]Entered sun6i_pcm_resume

<7>[35603.145968] gpu:open gpu power!

<6>[35603.165513] PM: resume of devices complete after 188.696 msecs

<6>[35603.165765] PM: resume devices took 0.190 seconds

<4>[35603.165847] [pm]aw_pm_end!

<7>[35603.165860] PM: Finishing wakeup.

<4>[35603.165873] Restarting tasks ... 

<6>[35603.169595] usb 1-1: USB disconnect, device number 71

<6>[35603.174949] init: waitpid returned pid 27488, status = 00000000

<3>[35603.174985] init: untracked pid 27488 exited

<4>[35603.185318] done.

<4>[35603.185364] sunxi cpufreq resume ok

<6>[35603.185427] suspend: exit suspend, ret = 0 (2014-01-13 10:12:03.059999625 UTC)

<6>[35603.193663] request_suspend_state: wakeup (3->0) at 35603178420675 (2014-01-13 10:12:03.068216708 UTC)

<6>[35603.193751] [HDMI]Hdmi_late_resume

<6>[35603.193835] [DISP]>>display late resume done<<

<4>[35603.193852] ts->is_suspended:1

<5>[35603.193867] [VFE]vfe_resume

<5>[35603.193940] [VFE]vfe resume work start!

<4>[35603.194965] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<5>[35603.195327] [VFE]mclk on

<4>[35603.207417] [VFE_WARN]invalid gpio

<4>[35603.216298] CPU1: Booted secondary processor

<6>[35603.216354] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[35603.235915] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35603.281561] [VFE]sensor full initial success when resume from suspend!

<4>[35603.281591] [OV5647]disalbe oe!

<5>[35603.297390] [VFE]mclk on

<4>[35603.309537] [VFE_WARN]invalid gpio

<4>[35603.354096] [CSI][GC2035]V4L2_IDENT_SENSOR=2035

<5>[35603.534201] [VFE]sensor full initial success when resume from suspend!

<4>[35603.534299] [CSI][GC2035]disalbe oe!

<5>[35603.545299] [VFE]mclk off

<5>[35603.545326] [VFE]vfe resume work end!

<4>[35606.155292] do_wake

<4>[35606.155324] [sw_module]: usi6276 modem wakeup

<4>[35606.712695] ehci_irq: highspeed device connect

<6>[35606.985794] usb 1-1: new high-speed USB device number 72 using sw-ehci

<6>[35607.156951] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<6>[35609.223229] init: waitpid returned pid 27738, status = 00000000

<3>[35609.223436] init: untracked pid 27738 exited

<4>[35613.778088] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[35619.550465] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35619.551763] [pm]valid

<6>[35619.551919] request_suspend_state: sleep (0->3) at 35619536641598 (2014-01-13 10:12:19.426427257 UTC)

<5>[35619.553909] [VFE]vfe_suspend

<5>[35619.553998] [VFE]set camera to power off!

<5>[35619.554093] [VFE]mclk off

<4>[35619.554173] [VFE_WARN]invalid gpio

<4>[35619.565563] [VFE_WARN]invalid gpio

<4>[35619.578035] [VFE_WARN]invalid gpio

<5>[35619.590800] [VFE]mclk off

<5>[35619.590940] [VFE]vfe_suspend done!

<6>[35620.345720] [HDMI]Hdmi_early_suspend

<6>[35620.345948] [DISP]>>display early suspend done<<

<4>[35620.363216] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<5>[35622.852788] CPU1: shutdown

<6>[35622.852908] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35622.866617] [hotplug]: cpu1 is killed! .

<5>[35622.879707] CPU2: shutdown

<6>[35622.879825] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35622.896664] [hotplug]: cpu2 is killed! .

<4>[35623.193056] [pm]valid

<6>[35623.193170] PM: Syncing filesystems ... done.

<7>[35623.208610] PM: Preparing system for mem sleep

<4>[35623.208794] sunxi cpufreq suspend ok

<4>[35623.208963] Freezing user space processes ... (elapsed 0.05 seconds) done.

<4>[35623.267241] Freezing remaining freezable tasks ... (elapsed 0.01 seconds) done.

<7>[35623.287104] PM: Entering mem sleep

<4>[35623.287202] [pm]3 state begin

<4>[35623.289496] Suspending console(s) (use no_console_suspend to debug)

<7>[35623.290534] gpu:close gpu power!

<4>[35623.290755] [PCM]Entered sun6i_pcm_suspend

<4>[35623.291167] [IIS]Entered sun6i_i2s_suspend

<6>[35623.291635] [DISP]>>disp super standby enter<<

<4>[35623.291798] [sw_module]: usi6276 modem sleep

<6>[35623.292008] [HDMI]Hdmi_suspend

<4>[35623.292347] [audio codec]:suspend

<4>[35623.515274] [audio codec]:suspend end

<4>[35623.757030] ehci_irq: highspeed device disconnect

<4>[35624.035394] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35624.036469] [mmc]: smc 1 suspend

<4>[35624.036509] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35624.037586] [mmc]: smc 0 suspend

<6>[35624.037821] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35624.037840] sun6i-rtc sun6i-rtc: read time 2014-1-13 10:12:24

<4>[35624.039310] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_suspend

<4>[35624.039329] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power OFF

<4>[35624.039345] [sw_hci_sun6i]: [sw-ehci2]: close clock

<4>[35624.039378] [sw_hci_sun6i]: ERR: hcd is null

<4>[35624.039629] [uart]: uart3 suspend

<4>[35624.039684] [uart]: uart2 suspend

<4>[35624.039710] [uart]: uart0 suspend

<4>[35624.040112] [sw_hcd0]: sw_hcd_suspend start

<4>[35624.040124] [sun6i_usb]: wrn: hcd is disable, need not enter to suspend

<4>[35624.040151] [sw_udc]: sw_udc_suspend start

<4>[35624.040163] [sw_udc]: udc is disable, need not enter to suspend

<4>[35624.041851] [i2c2] suspend okay.. 

<4>[35624.041880] [i2c1] suspend okay.. 

<4>[35624.041907] [i2c0] suspend okay.. 

<4>[35624.042092] [NAND] nand_suspend super

<6>[35624.042401] PM: suspend of devices complete after 752.262 msecs

<6>[35624.042418] PM: suspend devices took 0.750 seconds

<4>[35624.042430] [pm]prepare

<6>[35624.042938] PM: late suspend of devices complete after 0.492 msecs

<4>[35624.042952] [pm]prepare_late

<4>[35624.042963] Disabling non-boot CPUs ...

<5>[35624.044584] CPU3: shutdown

<6>[35624.044602] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35624.056311] [hotplug]: cpu3 is killed! .

<4>[35624.057841] [pm]enter state 3

<6>[35624.057841] resume_pointer = 0xc0052918. 

<4>[35624.057841] scence_lock: 

<4>[35624.057841] wakeup_src 0x2000

<4>[35624.057841] wakeup_gpio_map 0x1020

<4>[35624.057841] wakeup_gpio_group 0x0

<6>[35624.057841] resume1_bin_start = 0xc0056220, resume1_bin_end = 0xc0058a20. 

<6>[35624.057841] resume_code_src = 0x40056220, resume_code_length = 10240. resume_code_length = 2800 

<4>[35624.057841] arch/arm/mach-sun6i/pm/./pm.c, aw_super_standby, 635. 

<6>[35624.057841] suspend_status_flag = 0. 

<4>[35624.057841] [pm]platform wakeup, super standby wakesource is:0x40

<6>[35624.057853] Suspended for 0.000 seconds

<6>[35624.058016] Enabling non-boot CPUs ...

<4>[35624.090470] CPU3: Booted secondary processor

<6>[35624.090533] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35624.091396] CPU3 is up

<4>[35624.091409] [pm]platform wakeup.

<6>[35624.091931] PM: early resume of devices complete after 0.502 msecs

<4>[35624.097230] [pm]platform wakeup finish

<6>[35624.097761] [DISP]>>disp super standby exit<<

<6>[35624.097895] [HDMI]Hdmi_resume

<4>[35624.097988] [NAND] nand_resume super

<4>[35624.100952] [i2c0] resume okay.. 

<4>[35624.100977] [i2c1] resume okay.. 

<4>[35624.101001] [i2c2] resume okay.. 

<4>[35624.102389] battery vol change: 40->58 

<6>[35624.102433] wakeup wake lock: event0-2018

<4>[35624.105189] [sw_udc]: sw_udc_resume start

<4>[35624.105201] [sw_udc]: udc is disable, need not enter to resume

<4>[35624.105218] [sw_hcd0]: sw_hcd_resume start

<4>[35624.105228] [sun6i_usb]: wrn: hcd is disable, need not resume

<4>[35624.105496] [uart]: uart0 resume

<4>[35624.105516] [uart]: uart2 resume

<4>[35624.105566] [uart]: uart3 resume

<4>[35624.105673] [sw_hci_sun6i]: ERR: hcd is null

<4>[35624.105689] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_resume

<4>[35624.105701] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[35624.105927] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<4>[35624.105940] [sw_hci_sun6i]: [sw-ehci2]: lost power, restarting

<4>[35624.105957] usb usb1: root hub lost power or was reset

<6>[35624.115330] [DISP]>>disp_resume call<<

<4>[35624.197811] [LCD] ANX9804 Chip found

<4>[35624.200595] [LCD] ANX9804 clock is stable.

<6>[35624.255485] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35624.255504] sun6i-rtc sun6i-rtc: read time 2014-1-13 11:13:45

<4>[35624.260606] [mmc]: smc 0 resume

<4>[35624.260623] [mmc]: smc 1 resume

<4>[35624.260777] [audio codec]:resume start

<4>[35624.260798] [audio codec]:resume end

<4>[35624.261023] [rfkill]: rfkill set power 1

<4>[35624.261038] [rtl8723au]: rtl8723au is powered down by bt

<4>[35624.261051] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[35624.275751] [IIS]Entered sun6i_i2s_resume

<4>[35624.275983] [PCM]Entered sun6i_pcm_resume

<7>[35624.276020] gpu:open gpu power!

<6>[35624.295572] PM: resume of devices complete after 198.322 msecs

<6>[35624.295824] PM: resume devices took 0.200 seconds

<4>[35624.296107] [pm]aw_pm_end!

<7>[35624.296120] PM: Finishing wakeup.

<4>[35624.296133] Restarting tasks ... 

<6>[35624.300695] usb 1-1: USB disconnect, device number 72

<4>[35624.303227] done.

<4>[35624.303266] sunxi cpufreq resume ok

<6>[35624.303346] suspend: exit suspend, ret = 0 (2014-01-13 11:13:45.047858082 UTC)

<6>[35624.313222] request_suspend_state: wakeup (3->0) at 35624297947001 (2014-01-13 11:13:45.057726707 UTC)

<6>[35624.313292] [HDMI]Hdmi_late_resume

<6>[35624.313365] [DISP]>>display late resume done<<

<4>[35624.313379] ts->is_suspended:1

<5>[35624.313391] [VFE]vfe_resume

<5>[35624.313454] [VFE]vfe resume work start!

<4>[35624.314649] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<5>[35624.314735] [VFE]mclk on

<4>[35624.329165] [VFE_WARN]invalid gpio

<4>[35624.330621] CPU1: Booted secondary processor

<6>[35624.330677] Calibrating delay loop (skipped) already calibrated this CPUCPU2: Booted secondary processor

<6>[35624.353589] Calibrating delay loop (skipped) already calibrated this CPU

<4>[35624.404128] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<5>[35624.413041] [VFE]sensor full initial success when resume from suspend!

<4>[35624.413066] [OV5647]disalbe oe!

<5>[35624.426754] [VFE]mclk on

<4>[35624.438917] [VFE_WARN]invalid gpio

<4>[35624.452304] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<4>[35624.483015] [CSI][GC2035]V4L2_IDENT_SENSOR=2035

<5>[35624.658933] [VFE]sensor full initial success when resume from suspend!

<4>[35624.659023] [CSI][GC2035]disalbe oe!

<5>[35624.671298] [VFE]mclk off

<5>[35624.671387] [VFE]vfe resume work end!

<4>[35627.070764] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35627.072056] [pm]valid

<6>[35627.072214] request_suspend_state: sleep (0->3) at 35627056889920 (2014-01-13 11:13:47.816657793 UTC)

<5>[35627.074381] [VFE]vfe_suspend

<5>[35627.074465] [VFE]set camera to power off!

<5>[35627.074560] [VFE]mclk off

<4>[35627.074639] [VFE_WARN]invalid gpio

<4>[35627.085508] [VFE_WARN]invalid gpio

<4>[35627.097933] [VFE_WARN]invalid gpio

<5>[35627.110710] [VFE]mclk off

<5>[35627.110771] [VFE]vfe_suspend done!

<4>[35627.285329] do_wake

<4>[35627.285357] [sw_module]: usi6276 modem wakeup

<4>[35627.839382] ehci_irq: highspeed device connect

<6>[35627.865616] [HDMI]Hdmi_early_suspend

<6>[35627.865829] [DISP]>>display early suspend done<<

<6>[35628.115735] usb 1-1: new high-speed USB device number 73 using sw-ehci

<6>[35628.289469] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<4>[35629.313031] [pm]valid

<6>[35629.313149] PM: Syncing filesystems ... done.

<7>[35629.329042] PM: Preparing system for mem sleep

<4>[35629.329231] sunxi cpufreq suspend ok

<4>[35629.329405] Freezing user space processes ... (elapsed 0.04 seconds) done.

<4>[35629.377312] Freezing remaining freezable tasks ... (elapsed 0.01 seconds) done.

<7>[35629.397243] PM: Entering mem sleep

<4>[35629.397340] [pm]3 state begin

<4>[35629.399660] Suspending console(s) (use no_console_suspend to debug)

<7>[35629.400768] gpu:close gpu power!

<4>[35629.400989] [PCM]Entered sun6i_pcm_suspend

<4>[35629.401407] [IIS]Entered sun6i_i2s_suspend

<6>[35629.401905] [DISP]>>disp super standby enter<<

<4>[35629.402071] [sw_module]: usi6276 modem sleep

<6>[35629.402287] [HDMI]Hdmi_suspend

<4>[35629.402440] [audio codec]:suspend

<4>[35629.625320] [audio codec]:suspend end

<4>[35629.867320] ehci_irq: highspeed device disconnect

<4>[35630.145436] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35630.146511] [mmc]: smc 1 suspend

<4>[35630.146551] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35630.147629] [mmc]: smc 0 suspend

<6>[35630.147867] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35630.147885] sun6i-rtc sun6i-rtc: read time 2014-1-13 11:13:51

<4>[35630.149098] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_suspend

<4>[35630.149117] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power OFF

<4>[35630.149133] [sw_hci_sun6i]: [sw-ehci2]: close clock

<4>[35630.149166] [sw_hci_sun6i]: ERR: hcd is null

<4>[35630.149420] [uart]: uart3 suspend

<4>[35630.149474] [uart]: uart2 suspend

<4>[35630.149499] [uart]: uart0 suspend

<4>[35630.149895] [sw_hcd0]: sw_hcd_suspend start

<4>[35630.149907] [sun6i_usb]: wrn: hcd is disable, need not enter to suspend

<4>[35630.149934] [sw_udc]: sw_udc_suspend start

<4>[35630.149946] [sw_udc]: udc is disable, need not enter to suspend

<4>[35630.151632] [i2c2] suspend okay.. 

<4>[35630.151661] [i2c1] suspend okay.. 

<4>[35630.151689] [i2c0] suspend okay.. 

<4>[35630.151874] [NAND] nand_suspend super

<6>[35630.152182] PM: suspend of devices complete after 751.879 msecs

<6>[35630.152199] PM: suspend devices took 0.750 seconds

<4>[35630.152211] [pm]prepare

<6>[35630.152712] active wake lock alarm, time left 448

<3>[35630.152746] dpm_run_callback(): power_suspend_late+0x0/0x68 returns -11

<3>[35630.152763] PM: Device power.0 failed to suspend late: error -11

<6>[35630.152987] PM: early resume of devices complete after 0.203 msecs

<3>[35630.153166] PM: Some devices failed to power down

<4>[35630.153178] [pm]platform wakeup finish

<4>[35630.153420] [NAND] nand_resume super

<6>[35630.153476] [DISP]>>disp super standby exit<<

<6>[35630.153609] [HDMI]Hdmi_resume

<6>[35630.153921] [DISP]>>disp_resume call<<

<4>[35630.154129] [i2c0] resume okay.. 

<4>[35630.154171] [i2c1] resume okay.. 

<4>[35630.154195] [i2c2] resume okay.. 

<4>[35630.157412] [sw_udc]: sw_udc_resume start

<4>[35630.157424] [sw_udc]: udc is disable, need not enter to resume

<4>[35630.157441] [sw_hcd0]: sw_hcd_resume start

<4>[35630.157451] [sun6i_usb]: wrn: hcd is disable, need not resume

<4>[35630.157697] [uart]: uart0 resume

<4>[35630.157716] [uart]: uart2 resume

<4>[35630.157766] [uart]: uart3 resume

<4>[35630.157873] [sw_hci_sun6i]: ERR: hcd is null

<4>[35630.157888] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_resume

<4>[35630.157900] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[35630.158124] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<4>[35630.158136] [sw_hci_sun6i]: [sw-ehci2]: lost power, restarting

<4>[35630.158153] usb usb1: root hub lost power or was reset

<4>[35630.227775] [LCD] ANX9804 Chip found

<4>[35630.230563] [LCD] ANX9804 clock is stable.

<6>[35630.305511] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35630.305529] sun6i-rtc sun6i-rtc: read time 2014-1-13 11:13:51

<4>[35630.310611] [mmc]: smc 0 resume

<4>[35630.310627] [mmc]: smc 1 resume

<4>[35630.310784] [audio codec]:resume start

<4>[35630.310804] [audio codec]:resume end

<4>[35630.311028] [rfkill]: rfkill set power 1

<4>[35630.311043] [rtl8723au]: rtl8723au is powered down by bt

<4>[35630.311056] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[35630.325850] [IIS]Entered sun6i_i2s_resume

<4>[35630.326087] [PCM]Entered sun6i_pcm_resume

<7>[35630.326113] gpu:open gpu power!

<6>[35630.345566] PM: resume of devices complete after 192.369 msecs

<6>[35630.345851] PM: resume devices took 0.200 seconds

<4>[35630.365203] [pm]aw_pm_end!

<7>[35630.365216] PM: Finishing wakeup.

<4>[35630.365229] Restarting tasks ... 

<6>[35630.365415] usb 1-1: USB disconnect, device number 73

<4>[35630.372305] done.

<4>[35630.372361] sunxi cpufreq resume ok

<6>[35630.372433] suspend: exit suspend, ret = -11 (2014-01-13 11:13:51.116941920 UTC)

<6>[35630.372547] init: waitpid returned pid 28181, status = 00000000

<3>[35630.372579] init: untracked pid 28181 exited

<4>[35633.335685] do_wake

<4>[35633.335799] [sw_module]: usi6276 modem wakeup

<4>[35633.893221] ehci_irq: highspeed device connect

<6>[35634.165705] usb 1-1: new high-speed USB device number 74 using sw-ehci

<6>[35634.336145] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<4>[35635.404865] [pm]valid

<6>[35635.404927] PM: Syncing filesystems ... done.

<7>[35635.414430] PM: Preparing system for mem sleep

<4>[35635.414542] sunxi cpufreq suspend ok

<4>[35635.414641] Freezing user space processes ... (elapsed 0.03 seconds) done.

<4>[35635.446462] Freezing remaining freezable tasks ... (elapsed 0.01 seconds) done.

<7>[35635.466386] PM: Entering mem sleep

<4>[35635.466441] [pm]3 state begin

<4>[35635.468675] Suspending console(s) (use no_console_suspend to debug)

<7>[35635.469782] gpu:close gpu power!

<4>[35635.469997] [PCM]Entered sun6i_pcm_suspend

<4>[35635.470437] [IIS]Entered sun6i_i2s_suspend

<4>[35635.471073] [sw_module]: usi6276 modem sleep

<4>[35635.471449] [audio codec]:suspend

<4>[35635.695313] [audio codec]:suspend end

<4>[35635.936392] ehci_irq: highspeed device disconnect

<6>[35636.205332] [DISP]>>disp super standby enter<<

<6>[35636.205616] [HDMI]Hdmi_suspend

<4>[35636.215431] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35636.216503] [mmc]: smc 1 suspend

<4>[35636.216543] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35636.217620] [mmc]: smc 0 suspend

<6>[35636.217857] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35636.217875] sun6i-rtc sun6i-rtc: read time 2014-1-13 11:13:57

<4>[35636.219298] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_suspend

<4>[35636.219317] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power OFF

<4>[35636.219334] [sw_hci_sun6i]: [sw-ehci2]: close clock

<4>[35636.219367] [sw_hci_sun6i]: ERR: hcd is null

<4>[35636.219623] [uart]: uart3 suspend

<4>[35636.219678] [uart]: uart2 suspend

<4>[35636.219704] [uart]: uart0 suspend

<4>[35636.220106] [sw_hcd0]: sw_hcd_suspend start

<4>[35636.220119] [sun6i_usb]: wrn: hcd is disable, need not enter to suspend

<4>[35636.220146] [sw_udc]: sw_udc_suspend start

<4>[35636.220157] [sw_udc]: udc is disable, need not enter to suspend

<4>[35636.221852] [i2c2] suspend okay.. 

<4>[35636.221882] [i2c1] suspend okay.. 

<4>[35636.221909] [i2c0] suspend okay.. 

<4>[35636.222094] [NAND] nand_suspend super

<6>[35636.222404] PM: suspend of devices complete after 753.084 msecs

<6>[35636.222422] PM: suspend devices took 0.750 seconds

<4>[35636.222434] [pm]prepare

<6>[35636.222953] PM: late suspend of devices complete after 0.503 msecs

<4>[35636.222966] [pm]prepare_late

<4>[35636.222977] Disabling non-boot CPUs ...

<5>[35636.224605] CPU1: shutdown

<6>[35636.224624] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35636.236362] [hotplug]: cpu1 is killed! .

<5>[35636.239084] CPU2: shutdown

<6>[35636.239103] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35636.256358] [hotplug]: cpu2 is killed! .

<5>[35636.258952] CPU3: shutdown

<6>[35636.258971] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35636.276355] [hotplug]: cpu3 is killed! .

<4>[35636.277809] [pm]enter state 3

<6>[35636.277809] resume_pointer = 0xc0052918. 

<4>[35636.277809] scence_lock: 

<4>[35636.277809] wakeup_src 0x2000

<4>[35636.277809] wakeup_gpio_map 0x1020

<4>[35636.277809] wakeup_gpio_group 0x0

<6>[35636.277809] resume1_bin_start = 0xc0056220, resume1_bin_end = 0xc0058a20. 

<6>[35636.277809] resume_code_src = 0x40056220, resume_code_length = 10240. resume_code_length = 2800 

<4>[35636.277809] arch/arm/mach-sun6i/pm/./pm.c, aw_super_standby, 635. 

<6>[35636.277809] suspend_status_flag = 0. 

<4>[35636.277809] [pm]platform wakeup, super standby wakesource is:0x18

<6>[35636.277821] Suspended for 0.000 seconds

<6>[35636.277907] Enabling non-boot CPUs ...

<4>[35636.310849] CPU1: Booted secondary processor

<6>[35636.310913] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35636.311805] CPU1 is up

<4>[35636.334456] CPU2: Booted secondary processor

<6>[35636.334517] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35636.335535] CPU2 is up

<4>[35636.348162] CPU3: Booted secondary processor

<6>[35636.348219] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35636.349105] CPU3 is up

<4>[35636.349119] [pm]platform wakeup.

<6>[35636.349638] PM: early resume of devices complete after 0.499 msecs

<4>[35636.349871] [pm]platform wakeup finish

<4>[35636.350092] [NAND] nand_resume super

<4>[35636.353074] [i2c0] resume okay.. 

<4>[35636.353098] [i2c1] resume okay.. 

<4>[35636.353122] [i2c2] resume okay.. 

<6>[35636.354931] [DISP]>>disp super standby exit<<

<4>[35636.354950] battery vol change: 58->100 

<6>[35636.355049] wakeup wake lock: power-supply

<6>[35636.355069] [HDMI]Hdmi_resume

<4>[35636.358133] [sw_udc]: sw_udc_resume start

<4>[35636.358144] [sw_udc]: udc is disable, need not enter to resume

<4>[35636.358161] [sw_hcd0]: sw_hcd_resume start

<4>[35636.358171] [sun6i_usb]: wrn: hcd is disable, need not resume

<4>[35636.358402] [uart]: uart0 resume

<4>[35636.358421] [uart]: uart2 resume

<4>[35636.358466] [uart]: uart3 resume

<4>[35636.358573] [sw_hci_sun6i]: ERR: hcd is null

<4>[35636.358588] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_resume

<4>[35636.358601] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[35636.358827] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<4>[35636.358839] [sw_hci_sun6i]: [sw-ehci2]: lost power, restarting

<4>[35636.358857] usb usb1: root hub lost power or was reset

<6>[35636.365334] [DISP]>>disp_resume call<<

<4>[35636.457818] [LCD] ANX9804 Chip found

<4>[35636.460606] [LCD] ANX9804 clock is stable.

<6>[35636.505524] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35636.505543] sun6i-rtc sun6i-rtc: read time 2014-1-14 3:36:12

<4>[35636.510644] [mmc]: smc 0 resume

<4>[35636.510660] [mmc]: smc 1 resume

<4>[35636.510816] [audio codec]:resume start

<4>[35636.510837] [audio codec]:resume end

<4>[35636.511058] [rfkill]: rfkill set power 1

<4>[35636.511073] [rtl8723au]: rtl8723au is powered down by bt

<4>[35636.511086] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[35636.525862] [IIS]Entered sun6i_i2s_resume

<7>[35636.526075] gpu:open gpu power!

<4>[35636.526151] [PCM]Entered sun6i_pcm_resume

<6>[35636.545615] PM: resume of devices complete after 195.725 msecs

<6>[35636.545873] PM: resume devices took 0.200 seconds

<4>[35636.546162] [pm]aw_pm_end!

<7>[35636.546176] PM: Finishing wakeup.

<4>[35636.546188] Restarting tasks ... 

<6>[35636.546368] usb 1-1: USB disconnect, device number 74

<4>[35636.552700] done.

<4>[35636.552745] sunxi cpufreq resume ok

<6>[35636.552855] suspend: exit suspend, ret = 0 (2014-01-14 03:36:12.047325958 UTC)

<6>[35636.553515] init: waitpid returned pid 28192, status = 00000000

<3>[35636.553549] init: untracked pid 28192 exited

<6>[35636.803528] request_suspend_state: wakeup (3->0) at 35636788191295 (2014-01-14 03:36:12.297974208 UTC)

<6>[35636.803634] [HDMI]Hdmi_late_resume

<6>[35636.803725] [DISP]>>display late resume done<<

<4>[35636.803747] ts->is_suspended:1

<5>[35636.803763] [VFE]vfe_resume

<5>[35636.803846] [VFE]vfe resume work start!

<5>[35636.805161] [VFE]mclk on

<4>[35636.805577] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35636.815390] [VFE_WARN]invalid gpio

<5>[35636.892470] [VFE]sensor full initial success when resume from suspend!

<4>[35636.892601] [OV5647]disalbe oe!

<5>[35636.906712] [VFE]mclk on

<4>[35636.918814] [VFE_WARN]invalid gpio

<4>[35636.962842] [CSI][GC2035]V4L2_IDENT_SENSOR=2035

<5>[35637.140125] [VFE]sensor full initial success when resume from suspend!

<4>[35637.140222] [CSI][GC2035]disalbe oe!

<5>[35637.152374] [VFE]mclk off

<5>[35637.152409] [VFE]vfe resume work end!

<4>[35637.360033] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[35637.982972] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[35639.535363] do_wake

<4>[35639.535387] [sw_module]: usi6276 modem wakeup

<5>[35639.863831] CPU1: shutdown

<6>[35639.863951] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35639.876741] [hotplug]: cpu1 is killed! .

<5>[35639.889747] CPU2: shutdown

<6>[35639.889866] [hotplug]: cpu(3) try to kill cpu(2)

<6>[35639.906736] [hotplug]: cpu2 is killed! .

<4>[35640.092692] ehci_irq: highspeed device connect

<6>[35640.365655] usb 1-1: new high-speed USB device number 75 using sw-ehci

<6>[35640.548466] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<6>[35642.601819] init: waitpid returned pid 28409, status = 00000000

<3>[35642.602026] init: untracked pid 28409 exited

<4>[35644.027295] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[35653.278308] CPU1: Booted secondary processor

<6>[35653.278367] Calibrating delay loop (skipped) already calibrated this CPUCPU2: Booted secondary processor

<6>[35653.292955] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35654.632720] CPU1: shutdown

<6>[35654.632842] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35654.646794] [hotplug]: cpu1 is killed! .

<5>[35654.658525] CPU2: shutdown

<6>[35654.658650] [hotplug]: cpu(3) try to kill cpu(2)

<6>[35654.676855] [hotplug]: cpu2 is killed! .

<4>[35657.187066] CPU1: Booted secondary processor

<6>[35657.187119] Calibrating delay loop (skipped) already calibrated this CPUCPU2: Booted secondary processor

<6>[35657.198173] Calibrating delay loop (skipped) already calibrated this CPU

<4>[35657.253330] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35657.253915] [pm]valid

<6>[35657.253990] request_suspend_state: sleep (0->3) at 35657238658347 (2014-01-14 03:36:32.748438009 UTC)

<5>[35657.255847] [VFE]vfe_suspend

<5>[35657.255901] [VFE]set camera to power off!

<5>[35657.255969] [VFE]mclk off

<4>[35657.256019] [VFE_WARN]invalid gpio

<4>[35657.268241] [VFE_WARN]invalid gpio

<4>[35657.280569] [VFE_WARN]invalid gpio

<5>[35657.293193] [VFE]mclk off

<5>[35657.293292] [VFE]vfe_suspend done!

<6>[35658.045740] [HDMI]Hdmi_early_suspend

<6>[35658.045965] [DISP]>>display early suspend done<<

<6>[35658.047051] active wake lock sync_system

<4>[35658.079662] [pm]valid

<6>[35658.079768] PM: Syncing filesystems ... done.

<7>[35658.094637] PM: Preparing system for mem sleep

<4>[35658.094825] sunxi cpufreq suspend ok

<4>[35658.094993] Freezing user space processes ... (elapsed 0.05 seconds) done.

<4>[35658.147505] Freezing remaining freezable tasks ... (elapsed 0.01 seconds) done.

<7>[35658.167432] PM: Entering mem sleep

<4>[35658.167530] [pm]3 state begin

<4>[35658.169851] Suspending console(s) (use no_console_suspend to debug)

<7>[35658.170937] gpu:close gpu power!

<4>[35658.171161] [PCM]Entered sun6i_pcm_suspend

<4>[35658.171562] [IIS]Entered sun6i_i2s_suspend

<6>[35658.172027] [DISP]>>disp super standby enter<<

<4>[35658.172191] [sw_module]: usi6276 modem sleep

<6>[35658.172420] [HDMI]Hdmi_suspend

<4>[35658.172571] [audio codec]:suspend

<4>[35658.395358] [audio codec]:suspend end

<4>[35658.631593] ehci_irq: highspeed device disconnect

<4>[35658.915481] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35658.916555] [mmc]: smc 1 suspend

<4>[35658.916596] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[35658.917674] [mmc]: smc 0 suspend

<6>[35658.917912] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35658.917931] sun6i-rtc sun6i-rtc: read time 2014-1-14 3:36:34

<4>[35658.918998] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_suspend

<4>[35658.919017] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power OFF

<4>[35658.919033] [sw_hci_sun6i]: [sw-ehci2]: close clock

<4>[35658.919065] [sw_hci_sun6i]: ERR: hcd is null

<4>[35658.919320] [uart]: uart3 suspend

<4>[35658.919376] [uart]: uart2 suspend

<4>[35658.919401] [uart]: uart0 suspend

<4>[35658.919801] [sw_hcd0]: sw_hcd_suspend start

<4>[35658.919814] [sun6i_usb]: wrn: hcd is disable, need not enter to suspend

<4>[35658.919841] [sw_udc]: sw_udc_suspend start

<4>[35658.919852] [sw_udc]: udc is disable, need not enter to suspend

<4>[35658.921541] [i2c2] suspend okay.. 

<4>[35658.921570] [i2c1] suspend okay.. 

<4>[35658.921598] [i2c0] suspend okay.. 

<4>[35658.921781] [NAND] nand_suspend super

<6>[35658.933407] PM: suspend of devices complete after 762.909 msecs

<6>[35658.933425] PM: suspend devices took 0.760 seconds

<4>[35658.933438] [pm]prepare

<6>[35658.933961] PM: late suspend of devices complete after 0.506 msecs

<4>[35658.933974] [pm]prepare_late

<4>[35658.933985] Disabling non-boot CPUs ...

<5>[35658.935663] CPU1: shutdown

<6>[35658.935683] [hotplug]: cpu(0) try to kill cpu(1)

<6>[35658.956379] [hotplug]: cpu1 is killed! .

<5>[35658.958663] CPU2: shutdown

<6>[35658.958681] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35658.976431] [hotplug]: cpu2 is killed! .

<5>[35658.978742] CPU3: shutdown

<6>[35658.978761] [hotplug]: cpu(0) try to kill cpu(3)

<6>[35658.996394] [hotplug]: cpu3 is killed! .

<4>[35658.997768] [pm]enter state 3

<6>[35658.997768] resume_pointer = 0xc0052918. 

<4>[35658.997768] scence_lock: 

<4>[35658.997768] wakeup_src 0x2000

<4>[35658.997768] wakeup_gpio_map 0x1020

<4>[35658.997768] wakeup_gpio_group 0x0

<6>[35658.997768] resume1_bin_start = 0xc0056220, resume1_bin_end = 0xc0058a20. 

<6>[35658.997768] resume_code_src = 0x40056220, resume_code_length = 10240. resume_code_length = 2800 

<4>[35658.997768] arch/arm/mach-sun6i/pm/./pm.c, aw_super_standby, 635. 

<6>[35658.997768] suspend_status_flag = 0. 

<4>[35658.997768] [pm]platform wakeup, super standby wakesource is:0x18

<6>[35658.997779] Suspended for 0.000 seconds

<6>[35658.997866] Enabling non-boot CPUs ...

<4>[35659.030826] CPU1: Booted secondary processor

<6>[35659.030888] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35659.031625] CPU1 is up

<4>[35659.054330] CPU2: Booted secondary processor

<6>[35659.054389] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35659.055163] CPU2 is up

<4>[35659.067889] CPU3: Booted secondary processor

<6>[35659.067945] Calibrating delay loop (skipped) already calibrated this CPU

<6>[35659.068832] CPU3 is up

<4>[35659.068845] [pm]platform wakeup.

<6>[35659.069364] PM: early resume of devices complete after 0.499 msecs

<4>[35659.069597] [pm]platform wakeup finish

<4>[35659.069818] [NAND] nand_resume super

<4>[35659.072796] [i2c0] resume okay.. 

<4>[35659.072820] [i2c1] resume okay.. 

<4>[35659.072843] [i2c2] resume okay.. 

<6>[35659.074659] [DISP]>>disp super standby exit<<

<6>[35659.074795] [HDMI]Hdmi_resume

<6>[35659.075070] wakeup wake lock: power-supply

<4>[35659.077702] [sw_udc]: sw_udc_resume start

<4>[35659.077713] [sw_udc]: udc is disable, need not enter to resume

<4>[35659.077730] [sw_hcd0]: sw_hcd_resume start

<4>[35659.077740] [sun6i_usb]: wrn: hcd is disable, need not resume

<4>[35659.077969] [uart]: uart0 resume

<4>[35659.077988] [uart]: uart2 resume

<4>[35659.078033] [uart]: uart3 resume

<4>[35659.078139] [sw_hci_sun6i]: ERR: hcd is null

<4>[35659.078154] [sw_hci_sun6i]: [sw-ehci2]: sw_ehci_hcd_resume

<4>[35659.078166] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[35659.078393] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<4>[35659.078405] [sw_hci_sun6i]: [sw-ehci2]: lost power, restarting

<4>[35659.078423] usb usb1: root hub lost power or was reset

<6>[35659.085404] [DISP]>>disp_resume call<<

<4>[35659.167863] [LCD] ANX9804 Chip found

<4>[35659.170650] [LCD] ANX9804 clock is stable.

<6>[35659.225608] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[35659.225626] sun6i-rtc sun6i-rtc: read time 2014-1-14 3:37:15

<4>[35659.230726] [mmc]: smc 0 resume

<4>[35659.230742] [mmc]: smc 1 resume

<4>[35659.230902] [audio codec]:resume start

<4>[35659.230969] [audio codec]:resume end

<4>[35659.231198] [rfkill]: rfkill set power 1

<4>[35659.231213] [rtl8723au]: rtl8723au is powered down by bt

<4>[35659.231226] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<4>[35659.245913] [IIS]Entered sun6i_i2s_resume

<4>[35659.246179] [PCM]Entered sun6i_pcm_resume

<7>[35659.246221] gpu:open gpu power!

<6>[35659.265695] PM: resume of devices complete after 196.078 msecs

<6>[35659.265951] PM: resume devices took 0.200 seconds

<4>[35659.266041] [pm]aw_pm_end!

<7>[35659.266054] PM: Finishing wakeup.

<4>[35659.266067] Restarting tasks ... 

<6>[35659.266236] usb 1-1: USB disconnect, device number 75

<4>[35659.276710] done.

<4>[35659.276758] sunxi cpufreq resume ok

<6>[35659.276817] suspend: exit suspend, ret = 0 (2014-01-14 03:37:15.051204791 UTC)

<6>[35659.308277] request_suspend_state: wakeup (3->0) at 35659292899596 (2014-01-14 03:37:15.082641959 UTC)

<6>[35659.308371] [HDMI]Hdmi_late_resume

<6>[35659.308462] [DISP]>>display late resume done<<

<4>[35659.308481] ts->is_suspended:1

<5>[35659.308495] [VFE]vfe_resume

<5>[35659.308576] [VFE]vfe resume work start!

<4>[35659.309033] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<5>[35659.309881] [VFE]mclk on

<4>[35659.322020] [VFE_WARN]invalid gpio

<5>[35659.402785] [VFE]sensor full initial success when resume from suspend!

<4>[35659.402867] [OV5647]disalbe oe!

<5>[35659.417168] [VFE]mclk on

<4>[35659.429302] [VFE_WARN]invalid gpio

<4>[35659.473844] [CSI][GC2035]V4L2_IDENT_SENSOR=2035

<5>[35659.664157] [VFE]sensor full initial success when resume from suspend!

<4>[35659.664191] [CSI][GC2035]disalbe oe!

<5>[35659.675521] [VFE]mclk off

<5>[35659.675567] [VFE]vfe resume work end!

<4>[35661.585658] [sun6i_usb]: 

<4>[35661.585705] 

<4>[35661.585733] insmod_device_driver

<4>[35661.585769] 

<4>[35661.585865] [sw_udc]: sw_usb_device_enable start

<4>[35661.585970] [sw_udc]: usb_vbase  = 0xf1c19000

<4>[35661.586066] [sw_udc]: sram_vbase = 0xf1c00000

<4>[35661.586351] [sw_udc]: open_usb_clock

<4>[35661.586734] [sw_udc]: usbd_stop_work

<4>[35661.586879] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_1 dma_hdle[1] = 0xc0831108

<4>[35661.587036] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_2 dma_hdle[2] = 0xc083118c

<4>[35661.587192] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_3 dma_hdle[3] = 0xc0831210

<4>[35661.587349] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_4 dma_hdle[4] = 0xc0831294

<4>[35661.587506] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_5 dma_hdle[5] = 0xc0831318

<4>[35661.587835] [sw_udc]: CONFIG_USB_GADGET_DUALSPEED: USBC_TS_MODE_HS

<4>[35661.587947] [sw_udc]: usbd_start_work

<4>[35661.588031] [sw_udc]: usbd_start_work

<4>[35661.588113] [sw_udc]: sw_usb_device_enable end

<4>[35661.643500] [sw_udc]: IRQ: suspend

<4>[35661.643584] [sw_udc]: ERR: usb speed is unkown

<4>[35662.060165] [sw_udc]: IRQ: reset

<4>[35662.060273] (1:star,2:end): vfs_read:0, vfs_write:0,dma_working:0,amount:0,file_offset:0

<4>[35662.060381] [sw_udc]: irq: reset happen, throw away all urb

<4>[35662.133707] [sw_udc]: 

<4>[35662.133751] +++++++++++++++++++++++++++++++++++++

<4>[35662.133835] [sw_udc]:  usb enter high speed.

<4>[35662.133906] [sw_udc]: 

<4>[35662.133938] +++++++++++++++++++++++++++++++++++++

<6>[35662.136495] android_work: sent uevent USB_STATE=CONNECTED

<4>[35662.139343] [sw_udc]: IRQ: reset

<4>[35662.139451] (1:star,2:end): vfs_read:0, vfs_write:0,dma_working:0,amount:0,file_offset:0

<4>[35662.139559] [sw_udc]: irq: reset happen, throw away all urb

<4>[35662.174723] [sw_udc]: Set address 2

<4>[35662.255389] do_wake

<4>[35662.255408] [sw_module]: usi6276 modem wakeup

<6>[35662.306581] android_usb gadget: high-speed config #1: android

<4>[35662.306627] [sw_udc]: ep enable: ep3(0xc07fdffc, ep3-bulk, 128, 512)

<4>[35662.306647] [sw_udc]: ep enable: ep1(0xc07fdf64, ep1-bulk, 128, 512)

<4>[35662.306659] [sw_udc]: ep enable: ep4(0xc07fe048, ep4-bulk, 0, 512)

<4>[35662.306680] [sw_udc]: ep enable: ep2(0xc07fdfb0, ep2-bulk, 0, 512)

<4>[35662.306708] [sw_udc]: alloc request: ep(0xc07fdf64, ep1-bulk, 512), req(0xebc36440)

<4>[35662.306725] [sw_udc]: alloc request: ep(0xc07fdfb0, ep2-bulk, 512), req(0xedd91940)

<4>[35662.306743] [sw_udc]: alloc request: ep(0xc07fdf64, ep1-bulk, 512), req(0xecd8cac0)

<4>[35662.306760] [sw_udc]: alloc request: ep(0xc07fdfb0, ep2-bulk, 512), req(0xecd8c940)

<6>[35662.307088] android_work: sent uevent USB_STATE=CONFIGURED

<4>[35662.812622] ehci_irq: highspeed device connect

<6>[35663.085402] usb 1-1: new high-speed USB device number 76 using sw-ehci

<6>[35663.238877] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<6>[35665.248776] init: waitpid returned pid 28655, status = 00000000

<3>[35665.248806] init: untracked pid 28655 exited

<4>[35667.394715] [sun6i_usb]: handle_ep0: ep0 setup end

<4>[35678.662513] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<5>[35688.196714] CPU1: shutdown

<6>[35688.196736] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35688.216404] [hotplug]: cpu1 is killed! .

<5>[35688.218481] CPU2: shutdown

<6>[35688.218502] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35688.236397] [hotplug]: cpu2 is killed! .

<4>[35791.856076] CPU1: Booted secondary processor

<6>[35791.856131] Calibrating delay loop (skipped) already calibrated this CPUCPU2: Booted secondary processor

<6>[35791.872980] Calibrating delay loop (skipped) already calibrated this CPU

<5>[35793.186623] CPU1: shutdown

<6>[35793.186644] [hotplug]: cpu(2) try to kill cpu(1)

<6>[35793.206401] [hotplug]: cpu1 is killed! .

<5>[35793.208255] CPU2: shutdown

<6>[35793.208278] [hotplug]: cpu(0) try to kill cpu(2)

<6>[35793.226406] [hotplug]: cpu2 is killed! .

<4>[35798.997642] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[35798.997881] [pm]valid

<6>[35798.997919] request_suspend_state: sleep (0->3) at 35798982562078 (2014-01-14 03:39:34.772302899 UTC)

<5>[35798.998924] [VFE]vfe_suspend

<5>[35798.998942] [VFE]set camera to power off!

<5>[35798.998981] [VFE]mclk off

<4>[35798.999003] [VFE_WARN]invalid gpio

<4>[35799.011159] [VFE_WARN]invalid gpio

<4>[35799.022262] [VFE_WARN]invalid gpio

<5>[35799.034510] [VFE]mclk off

<5>[35799.034539] [VFE]vfe_suspend done!

<6>[35799.785407] [HDMI]Hdmi_early_suspend

<6>[35799.785449] [DISP]>>display early suspend done<<

<4>[35799.810736] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<6>[36367.328998] request_suspend_state: wakeup (3->0) at 36367313632683 (2014-01-14 03:49:03.103375380 UTC)

<6>[36367.329128] [HDMI]Hdmi_late_resume

<4>[36367.330586] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[36367.407636] [LCD] ANX9804 Chip found

<4>[36367.410167] [LCD] ANX9804 clock is stable.

<6>[36367.515547] [DISP]>>display late resume done<<

<4>[36367.515623] ts->is_suspended:0

<5>[36367.515641] [VFE]vfe_resume

<5>[36367.515766] [VFE]vfe resume work start!

<5>[36367.517137] [VFE]mclk on

<4>[36367.529206] [VFE_WARN]invalid gpio

<4>[36367.537814] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<4>[36367.570314] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<4>[36367.596256] CPU1: Booted secondary processor

<6>[36367.596313] Calibrating delay loop (skipped) already calibrated this CPU

<5>[36367.601405] [VFE]sensor full initial success when resume from suspend!

<4>[36367.601426] [OV5647]disalbe oe!

<5>[36367.616668] [VFE]mclk on

<4>[36367.618031] CPU2: Booted secondary processor

<6>[36367.618090] Calibrating delay loop (skipped) already calibrated this CPU

<4>[36367.628763] [VFE_WARN]invalid gpio

<4>[36367.672773] [CSI][GC2035]V4L2_IDENT_SENSOR=2035

<5>[36367.845047] [VFE]sensor full initial success when resume from suspend!

<4>[36367.845075] [CSI][GC2035]disalbe oe!

<5>[36367.855461] [VFE]mclk off

<5>[36367.855494] [VFE]vfe resume work end!

<5>[36371.896661] CPU1: shutdown

<6>[36371.896682] [hotplug]: cpu(2) try to kill cpu(1)

<6>[36371.916397] [hotplug]: cpu1 is killed! .

<5>[36371.918766] CPU3: shutdown

<6>[36371.918788] [hotplug]: cpu(0) try to kill cpu(3)

<6>[36371.936397] [hotplug]: cpu3 is killed! .

<4>[36482.646007] CPU1: Booted secondary processor

<6>[36482.646061] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[36482.666957] Calibrating delay loop (skipped) already calibrated this CPU

<5>[36485.226661] CPU1: shutdown

<6>[36485.226684] [hotplug]: cpu(2) try to kill cpu(1)

<6>[36485.246403] [hotplug]: cpu1 is killed! .

<5>[36485.248449] CPU3: shutdown

<6>[36485.248471] [hotplug]: cpu(0) try to kill cpu(3)

<6>[36485.266397] [hotplug]: cpu3 is killed! .

<4>[36489.529502] CPU1: Booted secondary processor

<6>[36489.529576] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[36489.546050] Calibrating delay loop (skipped) already calibrated this CPU

<4>[36489.595942] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[36489.596159] [pm]valid

<6>[36489.596188] request_suspend_state: sleep (0->3) at 36489580833324 (2014-01-14 03:51:05.370574104 UTC)

<5>[36489.597122] [VFE]vfe_suspend

<5>[36489.597153] [VFE]set camera to power off!

<5>[36489.597186] [VFE]mclk off

<4>[36489.597215] [VFE_WARN]invalid gpio

<4>[36489.609388] [VFE_WARN]invalid gpio

<4>[36489.621471] [VFE_WARN]invalid gpio

<5>[36489.633716] [VFE]mclk off

<5>[36489.633739] [VFE]vfe_suspend done!

<6>[36490.385411] [HDMI]Hdmi_early_suspend

<6>[36490.385455] [DISP]>>display early suspend done<<

<5>[36494.416698] CPU1: shutdown

<6>[36494.416719] [hotplug]: cpu(0) try to kill cpu(1)

<6>[36494.436423] [hotplug]: cpu1 is killed! .

<5>[36494.438547] CPU3: shutdown

<6>[36494.438568] [hotplug]: cpu(0) try to kill cpu(3)

<6>[36494.456430] [hotplug]: cpu3 is killed! .

<4>[36519.708993] CPU1: Booted secondary processor

<6>[36519.709048] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[36519.722533] Calibrating delay loop (skipped) already calibrated this CPU

<5>[36524.476456] CPU1: shutdown

<6>[36524.476478] [hotplug]: cpu(0) try to kill cpu(1)

<6>[36524.496437] [hotplug]: cpu1 is killed! .

<5>[36524.498407] CPU3: shutdown

<6>[36524.498428] [hotplug]: cpu(0) try to kill cpu(3)

<6>[36524.516418] [hotplug]: cpu3 is killed! .

<4>[36525.887508] CPU1: Booted secondary processor

<6>[36525.887561] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[36525.908808] Calibrating delay loop (skipped) already calibrated this CPUPHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<5>[36530.476760] CPU2: shutdown

<6>[36530.476782] [hotplug]: cpu(0) try to kill cpu(2)

<6>[36530.496413] [hotplug]: cpu2 is killed! .

<5>[36530.498619] CPU3: shutdown

<6>[36530.498641] [hotplug]: cpu(1) try to kill cpu(3)

<6>[36530.516423] [hotplug]: cpu3 is killed! .

<4>[37444.266282] CPU2: Booted secondary processor

<6>[37444.266341] Calibrating delay loop (skipped) already calibrated this CPUCPU3: Booted secondary processor

<6>[37444.280748] Calibrating delay loop (skipped) already calibrated this CPU

<5>[37456.276668] CPU2: shutdown

<6>[37456.276689] [hotplug]: cpu(0) try to kill cpu(2)

<6>[37456.296426] [hotplug]: cpu2 is killed! .

<5>[37456.298697] CPU3: shutdown

<6>[37456.298717] [hotplug]: cpu(1) try to kill cpu(3)

<6>[37456.316407] [hotplug]: cpu3 is killed! .

<6>[37621.769259] EXT4-fs (nandd): re-mounted. Opts: (null)

<4>[37624.112744] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

