 PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache

<4>[    0.000000] Machine: sun6i

<4>[    0.000000] Memory policy: ECC disabled, Data cache writealloc

<7>[    0.000000] On node 0 totalpages: 415744

<7>[    0.000000] free_area_init_node: node 0, pgdat c0814e00, node_mem_map dd900000

<7>[    0.000000]   DMA zone: 144 pages used for memmap

<7>[    0.000000]   DMA zone: 0 pages reserved

<7>[    0.000000]   DMA zone: 16240 pages, LIFO batch:3

<7>[    0.000000]   Normal zone: 1566 pages used for memmap

<7>[    0.000000]   Normal zone: 68066 pages, LIFO batch:15

<7>[    0.000000]   HighMem zone: 2898 pages used for memmap

<7>[    0.000000]   HighMem zone: 326830 pages, LIFO batch:31

<6>[    0.000000] PERCPU: Embedded 8 pages/cpu @deb0f000 s10176 r8192 d14400 u32768

<7>[    0.000000] pcpu-alloc: s10176 r8192 d14400 u32768 alloc=8*4096

<7>[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 

<4>[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 411136

<5>[    0.000000] Kernel command line: console=ttyS0,115200 rw init=/init loglevel=4 ion_reserve=256M boot_type=0 partitions=bootloader@nanda:env@nandb:boot@nandc:system@nandd:data@nande:misc@nandf:recovery@nandg:cache@nandh:databk@nandi:UDISK@nandj

<6>[    0.000000] PID hash table entries: 2048 (order: 1, 8192 bytes)

<6>[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)

<6>[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)

<6>[    0.000000] Memory: 49MB 1575MB = 1624MB total

<5>[    0.000000] Memory: 1633448k/1633448k available, 463704k reserved, 1318912K highmem

<5>[    0.000000] Virtual kernel memory layout:

<5>[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)

<5>[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)

<5>[    0.000000]     vmalloc : 0xf0000000 - 0xff000000   ( 240 MB)

<5>[    0.000000]     lowmem  : 0xc0000000 - 0xef800000   ( 760 MB)

<5>[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)

<5>[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)

<5>[    0.000000]       .text : 0xc0008000 - 0xc0784000   (7664 kB)

<5>[    0.000000]       .init : 0xc0784000 - 0xc07cb7c0   ( 286 kB)

<5>[    0.000000]       .data : 0xc07cc000 - 0xc0821f70   ( 344 kB)

<5>[    0.000000]        .bss : 0xc0821f94 - 0xc099dbd0   (1520 kB)

<6>[    0.000000] Preemptible hierarchical RCU implementation.

<6>[    0.000000] NR_IRQS:160

<4>[    0.000000] [aw_delay]: It is use use_time_delay function!

<6>[    0.000000] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 178956ms

<6>[    0.000000] Architected local timer running at 24.00MHz.

<6>[    0.000000] Console: colour dummy device 80x30

<6>[    0.000436] Calibrating delay loop... 2013.59 BogoMIPS (lpj=10067968)

<6>[    0.059952] pid_max: default: 32768 minimum: 301

<6>[    0.060307] Mount-cache hash table entries: 512

<6>[    0.061030] CPU: Testing write buffer coherency: ok

<6>[    0.061078] ftrace: allocating 20628 entries in 61 pages

<6>[    0.097490] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000

<6>[    0.097573] Setting up static identity map for 0x4058cb18 - 0x4058cb70

<4>[    0.224687] CPU1: Booted secondary processor

<6>[    0.277838] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001

<4>[    0.344865] CPU2: Booted secondary processor

<6>[    0.398007] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002

<4>[    0.465045] CPU3: Booted secondary processor

<6>[    0.518175] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003

<6>[    0.518265] Brought up 4 CPUs

<6>[    0.518280] SMP: Total of 4 processors activated (8054.37 BogoMIPS).

<6>[    0.519339] devtmpfs: initialized

<4>[    0.524759] script_init enter!

<4>[    0.525484] script_init exit!

<6>[    0.527131] print_constraints: dummy: 

<6>[    0.527615] NET: Registered protocol family 16

<7>[    0.527825] sunxi_dump_init success

<6>[    0.528100] script_sysfs_init success

<6>[    0.532820] gpiochip_add: registered GPIOs 0 to 27 on device: GPA

<6>[    0.533034] gpiochip_add: registered GPIOs 30 to 37 on device: GPB

<6>[    0.533232] gpiochip_add: registered GPIOs 40 to 67 on device: GPC

<6>[    0.533440] gpiochip_add: registered GPIOs 70 to 97 on device: GPD

<6>[    0.533655] gpiochip_add: registered GPIOs 100 to 116 on device: GPE

<6>[    0.533857] gpiochip_add: registered GPIOs 119 to 124 on device: GPF

<6>[    0.534063] gpiochip_add: registered GPIOs 127 to 145 on device: GPG

<6>[    0.534259] gpiochip_add: registered GPIOs 148 to 178 on device: GPH

<6>[    0.534456] gpiochip_add: registered GPIOs 181 to 189 on device: GPL

<6>[    0.534673] gpiochip_add: registered GPIOs 192 to 199 on device: GPM

<4>[    0.535117] sun6i ar100 driver v1.00

<4>[    0.543864] move ar100 binary data [addr = c00359d8, len = 13000] to sram_a2 finished

<3>[    0.954376] AR100 ERROR :ar100 ir power key code config type err!

<3>[    0.954387] AR100 WARING :parse ir power key code fail

<6>[    0.993317] bio: create slab <bio-0> at 0

<5>[    0.995154] SCSI subsystem initialized

<6>[    0.995943] usbcore: registered new interface driver usbfs

<6>[    0.996240] usbcore: registered new interface driver hub

<6>[    0.996445] usbcore: registered new device driver usb

<6>[    0.999543] axp_mfd 1-0034: AXP (CHIP ID: 0x17) detected

<4>[    1.004057] pmu fake power off config type err!

<6>[    1.004546] print_constraints: axp22_ldo1: 3000 mV 

<4>[    1.004953] suspend_set_state: axp22_ldo2: No configuration

<6>[    1.005013] print_constraints: axp22_ldo2: 700 <--> 3300 mV at 3300 mV 

<6>[    1.005527] print_constraints: axp22_ldo3: 700 <--> 3300 mV at 1800 mV 

<6>[    1.006047] print_constraints: axp22_ldo4: 700 <--> 3300 mV at 3000 mV 

<4>[    1.006463] suspend_set_state: axp22_ldo5: No configuration

<6>[    1.006520] print_constraints: axp22_ldo5: 700 <--> 3300 mV at 700 mV 

<4>[    1.006904] suspend_set_state: axp22_ldo6: No configuration

<6>[    1.006962] print_constraints: axp22_ldo6: 700 <--> 3300 mV at 700 mV 

<4>[    1.007337] suspend_set_state: axp22_ldo7: No configuration

<6>[    1.007395] print_constraints: axp22_ldo7: 700 <--> 3300 mV at 2800 mV 

<4>[    1.007796] suspend_set_state: axp22_ldo8: No configuration

<6>[    1.007853] print_constraints: axp22_ldo8: 700 <--> 3300 mV at 700 mV 

<4>[    1.008233] suspend_set_state: axp22_ldo9: No configuration

<6>[    1.008291] print_constraints: axp22_ldo9: 700 <--> 3300 mV at 1500 mV 

<4>[    1.008705] suspend_set_state: axp22_ldo10: No configuration

<6>[    1.008764] print_constraints: axp22_ldo10: 700 <--> 3300 mV at 1800 mV 

<4>[    1.009153] suspend_set_state: axp22_ldo11: No configuration

<6>[    1.009211] print_constraints: axp22_ldo11: 700 <--> 3300 mV at 1800 mV 

<6>[    1.009753] print_constraints: axp22_ldo12: 700 <--> 1400 mV at 1100 mV 

<6>[    1.010263] print_constraints: axp22_DCDC1: 1600 <--> 3400 mV at 3000 mV 

<6>[    1.010801] print_constraints: axp22_DCDC2: 600 <--> 1540 mV at 1200 mV 

<6>[    1.011356] print_constraints: axp22_DCDC3: 600 <--> 1860 mV at 1260 mV 

<6>[    1.011868] print_constraints: axp22_DCDC4: 600 <--> 1540 mV at 1200 mV 

<6>[    1.012377] print_constraints: axp22_DCDC5: 1000 <--> 2550 mV at 1500 mV 

<6>[    1.012796] print_constraints: axp22_ldoio0: 700 <--> 3300 mV at 2800 mV 

<6>[    1.013230] print_constraints: axp22_ldoio1: 700 <--> 3300 mV at 3800 mV 

<6>[    1.013908] input: axp22-supplyer as /devices/platform/sun6i-i2c.1/i2c-1/1-0034/axp22-supplyer.19/input/input0

<4>[    1.013922] axp charger not limit now

<4>[    1.017520] now_rest_vol = 92

<6>[    1.018283] gpiochip_add: registered GPIOs 202 to 206 on device: axp_pin

<6>[    1.020362] Advanced Linux Sound Architecture Driver Version 1.0.24.

<6>[    1.021455] Bluetooth: Core ver 2.16

<6>[    1.021614] NET: Registered protocol family 31

<6>[    1.021625] Bluetooth: HCI device and connection manager initialized

<6>[    1.021642] Bluetooth: HCI socket layer initialized

<6>[    1.021653] Bluetooth: L2CAP socket layer initialized

<6>[    1.021688] Bluetooth: SCO socket layer initialized

<6>[    1.022158] cfg80211: Calling CRDA to update world regulatory domain

<6>[    1.022792] Switching to clocksource arch_sys_counter

<5>[    1.040594] FS-Cache: Loaded

<6>[    1.041111] CacheFiles: Loaded

<6>[    1.061718] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.061939] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver

<4>[    1.062131] [usb_manager]: CONFIG_USB_SW_SUN6I_USB0_OTG

<4>[    1.062716] [sw_udc]: udc_init: version 20080411

<6>[    1.063726] NET: Registered protocol family 2

<6>[    1.064003] IP route cache hash table entries: 16384 (order: 4, 65536 bytes)

<6>[    1.064763] TCP established hash table entries: 65536 (order: 7, 524288 bytes)

<6>[    1.065758] TCP bind hash table entries: 65536 (order: 7, 786432 bytes)

<6>[    1.066684] TCP: Hash tables configured (established 65536 bind 65536)

<6>[    1.066697] TCP reno registered

<6>[    1.066711] UDP hash table entries: 256 (order: 1, 8192 bytes)

<6>[    1.066737] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)

<6>[    1.067104] NET: Registered protocol family 1

<6>[    1.067681] RPC: Registered named UNIX socket transport module.

<6>[    1.067693] RPC: Registered udp transport module.

<6>[    1.067702] RPC: Registered tcp transport module.

<6>[    1.067711] RPC: Registered tcp NFSv4.1 backchannel transport module.

<6>[    1.067973] Unpacking initramfs...

<6>[    1.215335] Freeing initrd memory: 564K

<6>[    1.215353] sunxi_reg_init enter

<4>[    1.216188] [pm]aw_pm_init!

<6>[    1.216201] standby_mode = 1. 

<6>[    1.216211] cpu0_en = 0.

<6>[    1.216219] dram_selfresh_en = 1.

<6>[    1.216229] wakeup src cnt is : 2. 

<4>[    1.216243] [exstandby]leave extended_standby_enable_wakeup_src : event 0x2000

<4>[    1.216254] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_map 0x20

<4>[    1.216266] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_group 0x0

<4>[    1.216278] [exstandby]leave extended_standby_enable_wakeup_src : event 0x2000

<4>[    1.216289] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_map 0x1020

<4>[    1.216301] [exstandby]leave extended_standby_enable_wakeup_src : wakeup_gpio_group 0x0

<6>[    1.216312] cpus need care gpio: mem_para_info.cpus_gpio_wakeup = 0x0. 

<4>[    1.216331] [wifi]: select wifi: rtl8723au !!

<4>[    1.216707] [rtl8723au]: exec rtl8723au_wifi_gpio_init

<4>[    1.216723] [sw_hci_sun6i]: ERR: sw_ehci is null

<4>[    1.216733] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[    1.217735] [rtl8723au]: rtl8723au module power set by axp.

<4>[    1.217828] [rtl8723au]: first time

<4>[    1.218156] [wifi_pm]: wifi gpio init is OK !!

<4>[    1.220004] highmem bounce pool size: 64 pages

<6>[    1.223681] NTFS driver 2.1.30 [Flags: R/W].

<6>[    1.224146] fuse init (API version 7.18)

<6>[    1.225244] msgmni has been set to 615

<6>[    1.226325] io scheduler noop registered

<6>[    1.226337] io scheduler deadline registered (default)

<4>[    1.235153] [uart]: driver initializied

<6>[    1.236098] sw_serial.0: ttyS0 at MMIO 0x1c28000 (irq = 32) is a SW

<4>[    1.236124] [uart]: console setup baud 115200 parity n bits 8, flow n

<6>[    1.248783] console [ttyS0] enabled

<6>[    1.249266] sw_serial.2: ttyS2 at MMIO 0x1c28800 (irq = 34) is a SW

<6>[    1.249702] sw_serial.3: ttyS3 at MMIO 0x1c28c00 (irq = 35) is a SW

<6>[    1.258103] loop: module loaded

<3>[    1.258141] sun6i_vibrator_init motor is not used in config

<6>[    1.264364] sunxi_hw_init: sunxi debug register driver init

<6>[    1.265295] tun: Universal TUN/TAP device driver, 1.6

<6>[    1.265308] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>

<6>[    1.265621] PPP generic driver version 2.4.2

<6>[    1.266042] PPP BSD Compression module registered

<6>[    1.266057] PPP Deflate Compression module registered

<6>[    1.266678] PPP MPPE Compression module registered

<6>[    1.266698] NET: Registered protocol family 24

<6>[    1.266747] PPTP driver version 0.8.5

<6>[    1.267345] usbcore: registered new interface driver cdc_ether

<6>[    1.267519] usbcore: registered new interface driver cdc_eem

<6>[    1.267689] usbcore: registered new interface driver cdc_subset

<4>[    1.267776] [sw_hci_sun6i]: ERR: sw-ehci1(restrict_gpio) is invalid

<4>[    1.267791] [sw_hci_sun6i]: ERR: sw-ehci1(drv vbus) is invalid

<4>[    1.267807] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.267864] [sw_hci_sun6i]: ERR: sw-ohci1(restrict_gpio) is invalid

<4>[    1.267878] [sw_hci_sun6i]: ERR: sw-ohci1(drv vbus) is invalid

<4>[    1.267893] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.267936] [sw_hci_sun6i]: ERR: sw-ehci2(restrict_gpio) is invalid

<4>[    1.267951] [sw_hci_sun6i]: ERR: sw-ehci2(drv vbus) is invalid

<4>[    1.267967] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.268006] [sw_hci_sun6i]: ERR: sw-ohci2(restrict_gpio) is invalid

<4>[    1.268021] [sw_hci_sun6i]: ERR: sw-ohci2(drv vbus) is invalid

<4>[    1.268036] [sw_hci_sun6i]: ERR: get usb_restrict_flag failed

<4>[    1.268333] [sw_hci_sun6i]: [sw-ehci1]: probe, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<4>[    1.268356] [sw_hci_sun6i]: [sw-ehci1]: open clock

<4>[    1.268587] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power ON

<6>[    1.268606] sw-ehci sw-ehci.1: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.268643] sw-ehci sw-ehci.1: new USB bus registered, assigned bus number 1

<6>[    1.268773] sw-ehci sw-ehci.1: irq 104, io mem 0xf1c1a000

<6>[    1.282878] sw-ehci sw-ehci.1: USB 0.0 started, EHCI 1.00

<4>[    1.282899] ehci_irq: highspeed device connect

<6>[    1.283848] hub 1-0:1.0: USB hub found

<6>[    1.283881] hub 1-0:1.0: 1 port detected

<4>[    1.284456] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_disable_ehci

<4>[    1.284474] [sw_hci_sun6i]: [sw-ehci1]: remove, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<6>[    1.284500] sw-ehci sw-ehci.1: remove, state 1

<6>[    1.284522] usb usb1: USB disconnect, device number 1

<6>[    1.285854] sw-ehci sw-ehci.1: USB bus 1 deregistered

<4>[    1.285877] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power OFF

<4>[    1.285892] [sw_hci_sun6i]: [sw-ehci1]: close clock

<4>[    1.285921] [sw_hci_sun6i]: ERR: usb1 sw-ohci1 is not enable

<4>[    1.286164] [sw_hci_sun6i]: [sw-ehci2]: probe, pdev->name: sw-ehci, pdev->id: 2, sw_ehci: 0xc08926bc

<4>[    1.286183] [sw_hci_sun6i]: [sw-ehci2]: open clock

<4>[    1.286407] [sw_hci_sun6i]: [sw-ehci2]: Set USB Power ON

<6>[    1.286422] sw-ehci sw-ehci.2: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.286451] sw-ehci sw-ehci.2: new USB bus registered, assigned bus number 1

<6>[    1.286530] sw-ehci sw-ehci.2: irq 106, io mem 0xf1c1b000

<6>[    1.302871] sw-ehci sw-ehci.2: USB 0.0 started, EHCI 1.00

<6>[    1.303783] hub 1-0:1.0: USB hub found

<6>[    1.303813] hub 1-0:1.0: 1 port detected

<4>[    1.304368] [sw_hci_sun6i]: ERR: usb2 sw-ohci2 is not enable

<4>[    1.304382] [sw_hci_sun6i]: ERR: usb0  is not enable

<6>[    1.304599] usbcore: registered new interface driver cdc_acm

<6>[    1.304613] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters

<6>[    1.304628] Initializing USB Mass Storage driver...

<6>[    1.304839] usbcore: registered new interface driver usb-storage

<6>[    1.304852] USB Mass Storage support registered.

<6>[    1.305021] usbcore: registered new interface driver ums-alauda

<6>[    1.305193] usbcore: registered new interface driver ums-cypress

<6>[    1.305373] usbcore: registered new interface driver ums-datafab

<6>[    1.305540] usbcore: registered new interface driver ums_eneub6250

<6>[    1.305716] usbcore: registered new interface driver ums-freecom

<6>[    1.305885] usbcore: registered new interface driver ums-isd200

<6>[    1.306055] usbcore: registered new interface driver ums-jumpshot

<6>[    1.306224] usbcore: registered new interface driver ums-karma

<6>[    1.306394] usbcore: registered new interface driver ums-onetouch

<6>[    1.306580] usbcore: registered new interface driver ums-realtek

<6>[    1.306749] usbcore: registered new interface driver ums-sddr09

<6>[    1.306919] usbcore: registered new interface driver ums-sddr55

<6>[    1.307097] usbcore: registered new interface driver ums-usbat

<6>[    1.307476] usbcore: registered new interface driver usbserial

<6>[    1.307491] usbserial: USB Serial Driver core

<6>[    1.307647] USB Serial support registered for GSM modem (1-port)

<6>[    1.307883] usbcore: registered new interface driver option

<6>[    1.307897] option: v0.7.2:USB Driver for GSM modems

<4>[    1.308391] [sw_udc]: [sw_usb_udc]: binding gadget driver 'android_usb'

<4>[    1.308413] [sw_udc]: alloc request: ep(0xc07fdf18, ep0, 64), req(0xeeae8cc0)

<4>[    1.308428] [sun6i_usb]: ERR: usb device is not active

<4>[    1.308444] [sw_udc]: sw_udc_pullup, is_on = 0

<4>[    1.308455] [sun6i_usb]: usb device is not active

<6>[    1.311626] android_usb gadget: Mass Storage Function, version: 2009/09/11

<6>[    1.311643] android_usb gadget: Number of LUNs=2

<6>[    1.311658]  lun0: LUN: removable file: (no medium)

<6>[    1.311672]  lun1: LUN: removable file: (no medium)

<4>[    1.312218] [sun6i_usb]: ERR: usb device is not active

<6>[    1.312242] android_usb gadget: android_usb ready

<4>[    1.312374] [sw_hcd0]: usb host driver initialize........

<4>[    1.312502] [sw_hcd0]: open_usb_clock

<4>[    1.312748] [sun6i_usb]: [sw_hcd0]: host_init_state = 0

<4>[    1.312762] [sw_hcd0]: platform is usb host

<4>[    1.312830] [sw_hcd0]: sw_hcd_init_controller: sw_hcd_host0: USB Host mode controller at f1c19000 using PIO, IRQ 103

<6>[    1.312903] sw_hcd_host0 sw_hcd_host0: sw_hcd host driver

<6>[    1.312924] sw_hcd_host0 sw_hcd_host0: new USB bus registered, assigned bus number 2

<6>[    1.313787] hub 2-0:1.0: USB hub found

<6>[    1.313824] hub 2-0:1.0: 1 port detected

<4>[    1.314346] [sw_hcd0]: sw_usb_host0_disable start

<4>[    1.314360] [sw_hcd0]: sw_hcd_wait_for_disconnect cnt=0

<4>[    1.314375] [sun6i_usb]: [sw_hcd_host0]: Set USB Power OFF

<4>[    1.314392] [sun6i_usb]: -------sw_hcd0_soft_disconnect---------

<4>[    1.314406] [sun6i_usb]: wrn: hcd is not enable, need not stop hcd

<4>[    1.314440] [sw_hcd0]: close_usb_clock

<4>[    1.314458] [sw_hcd0]: sw_usb_host0_disable end

<6>[    1.315154] mousedev: PS/2 mouse device common for all mice

<6>[    1.315887] =====ctp_fetch_sysconfig_para=====. 

<6>[    1.316663] sun6i-rtc sun6i-rtc: sun6i_rtc_probe tmp_data = 380239881

<6>[    1.316747] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[    1.316764] sun6i-rtc sun6i-rtc: read time 2014-1-14 5:37:37

<6>[    1.317320] using rtc device, rtc, for alarms

<6>[    1.317365] sun6i-rtc sun6i-rtc: rtc core: registered rtc as rtc0

<6>[    1.317534] Linux video capture interface: v2.00

<4>[    1.317678] [cedar]: install start!!!

<4>[    1.318606] [cedar]: install end!!!

<6>[    1.328731] device-mapper: ioctl: 4.22.0-ioctl (2011-10-19) initialised: dm-devel@redhat.com

<6>[    1.329289] Bluetooth: HCI UART driver ver 2.2

<6>[    1.329305] Bluetooth: HCI H4 protocol initialized

<6>[    1.329318] Bluetooth: HCI BCSP protocol initialized

<4>[    1.329802] [mmc]: sw_mci_init

<4>[    1.329855] [mmc]: MMC host used card: 0x3, boot card: 0x0, io_card 2

<4>[    1.336004] [mmc]: sdc0 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[    1.337095] [mmc]: sdc0 Probe: base:0xf0038000 irq:92 sg_cpu:ffdfc000(42c00000) ret 0.

<4>[    1.337626] [mmc]: sdc1 set ios: clk 0Hz bm OD pm OFF vdd 3.3V width 1 timing LEGACY(SDR12) dt B

<4>[    1.338691] [mmc]: sdc1 Probe: base:0xf003a000 irq:93 sg_cpu:ffdfb000(42c01000) ret 0.

<6>[    1.341489] usbcore: registered new interface driver usbhid

<6>[    1.341503] usbhid: USB HID core driver

<6>[    1.342454] ashmem: initialized

<6>[    1.342722] logger: created 256K log 'log_main'

<6>[    1.343014] logger: created 256K log 'log_events'

<6>[    1.343274] logger: created 256K log 'log_radio'

<6>[    1.343536] logger: created 256K log 'log_system'

<6>[    1.344697] input: headset as /devices/virtual/input/input1

<4>[    1.347004] enter sun6i Audio codec!!!

<6>[    1.348482] sun6i audio support initialized

<4>[    1.348589] sun6i Audio codec init end

<6>[    1.350893] asoc: sndhdmi <-> sun6i-hdmiaudio.0 mapping ok

<6>[    1.351971] ALSA device list:

<6>[    1.351985]   #0: sun6i-CODEC  Audio Codec

<6>[    1.351997]   #1: sndhdmi

<6>[    1.352224] Netfilter messages via NETLINK v0.30.

<6>[    1.352328] nf_conntrack version 0.5.0 (16384 buckets, 65536 max)

<6>[    1.352868] ctnetlink v0.93: registering with nfnetlink.

<6>[    1.352892] NF_TPROXY: Transparent proxy support initialized, version 4.1.0

<6>[    1.352905] NF_TPROXY: Copyright (c) 2006-2007 BalaBit IT Ltd.

<6>[    1.353803] xt_time: kernel timezone is -0000

<6>[    1.353849] IPv4 over IPv4 tunneling driver

<6>[    1.354737] GRE over IPv4 demultiplexor driver

<6>[    1.354752] GRE over IPv4 tunneling driver

<6>[    1.355744] ip_tables: (C) 2000-2006 Netfilter Core Team

<6>[    1.355950] TCP cubic registered

<6>[    1.355961] Initializing XFRM netlink socket

<6>[    1.356638] NET: Registered protocol family 10

<6>[    1.357885] ip6_tables: (C) 2000-2006 Netfilter Core Team

<6>[    1.358073] IPv6 over IPv4 tunneling driver

<6>[    1.359988] NET: Registered protocol family 17

<6>[    1.360038] NET: Registered protocol family 15

<6>[    1.360183] Bluetooth: RFCOMM TTY layer initialized

<6>[    1.360214] Bluetooth: RFCOMM socket layer initialized

<6>[    1.360227] Bluetooth: RFCOMM ver 1.11

<6>[    1.360242] Bluetooth: BNEP (Ethernet Emulation) ver 1.3

<6>[    1.360255] Bluetooth: BNEP filters: protocol multicast

<6>[    1.360271] Bluetooth: HIDP (Human Interface Emulation) ver 1.2

<6>[    1.360497] L2TP core driver, V2.0

<6>[    1.360526] PPPoL2TP kernel driver, V2.0

<6>[    1.360538] L2TP IP encapsulation support (L2TPv3)

<6>[    1.360689] L2TP netlink interface

<6>[    1.360729] L2TP ethernet pseudowire support (L2TPv3)

<6>[    1.360744] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 3

<6>[    1.360778] ThumbEE CPU extension supported.

<5>[    1.360803] Registering SWP/SWPB emulation handler

<4>[    1.361552] [rfkill]: rfkill set power 0

<4>[    1.361571] [rtl8723au]: rtl8723au is powered up by bt

<4>[    1.361585] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_enable_ehci

<4>[    1.361604] [sw_hci_sun6i]: [sw-ehci1]: probe, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<4>[    1.361626] [sw_hci_sun6i]: [sw-ehci1]: open clock

<4>[    1.361855] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power ON

<6>[    1.361873] sw-ehci sw-ehci.1: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[    1.361914] sw-ehci sw-ehci.1: new USB bus registered, assigned bus number 3

<6>[    1.362025] sw-ehci sw-ehci.1: irq 104, io mem 0xf1c1a000

<4>[    1.363293] regulator_init_complete: axp22_ldoio0: incomplete constraints, leaving on

<4>[    1.363353] regulator_init_complete: axp22_DCDC5: incomplete constraints, leaving on

<4>[    1.363410] regulator_init_complete: axp22_DCDC4: incomplete constraints, leaving on

<4>[    1.363468] regulator_init_complete: axp22_DCDC3: incomplete constraints, leaving on

<4>[    1.363525] regulator_init_complete: axp22_DCDC2: incomplete constraints, leaving on

<4>[    1.363582] regulator_init_complete: axp22_DCDC1: incomplete constraints, leaving on

<4>[    1.363640] regulator_init_complete: axp22_ldo12: incomplete constraints, leaving on

<4>[    1.363697] regulator_init_complete: axp22_ldo11: incomplete constraints, leaving on

<4>[    1.363996] regulator_init_complete: axp22_ldo4: incomplete constraints, leaving on

<4>[    1.364053] regulator_init_complete: axp22_ldo3: incomplete constraints, leaving on

<4>[    1.364184] [sw_module]: sw_module_init 1.0

<4>[    1.364599] [sw_module]: usimt6276ma modem support

<4>[    1.364622] [sw_module]: ERR: get dldo_name failed

<4>[    1.364679] [sw_module]: gpio_request bb_wake failed

<4>[    1.364701] [sw_module]: usi6276 modem init

<4>[    1.365006] [sw_module]: usi6276 modem probe

<4>[    1.365314] [sw_module]: usi6276_start: start ======

<3>[    1.365328] otg_wakelock_init: No OTG transceiver found

<4>[    1.365410] [sw_module]: before power on ======

<4>[    1.365420] [sw_module]: set usi6276 modem power on

<4>[    1.365435] [sw_module]: err: dldo parameter is invalid. dldo_name=, dldo_min_uV=2800000, dldo_max_uV=2800000.

<6>[    1.371180] sun6i-rtc sun6i-rtc: sun6i_rtc_gettime

<6>[    1.371197] sun6i-rtc sun6i-rtc: read time 2014-1-14 5:37:37

<6>[    1.371241] sun6i-rtc sun6i-rtc: setting system clock to 2014-01-14 05:37:37 UTC (1389677857)

<6>[    1.372008] Freeing init memory: 284K

<6>[    1.372024] Write protecting the kernel text section c0008000 - c0784000

<6>[    1.372208] rodata_test: attempting to write to read-only section:

<6>[    1.372227] write to read-only section trapped, success

<6>[    1.372902] sw-ehci sw-ehci.1: USB 0.0 started, EHCI 1.00

<4>[    1.372923] ehci_irq: highspeed device connect

<6>[    1.374037] hub 3-0:1.0: USB hub found

<6>[    1.374073] hub 3-0:1.0: 1 port detected

<4>[    1.374696] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[    1.374712] [rtl8723au]: rtl8723au power state change: wifi 0, bt 1 !!

<3>[    1.378638] init: /init.sun6i.rc: 150: invalid service name 'ttyusb-compatible'

<4>[    1.387356] init (1): /proc/1/oom_adj is deprecated, please use /proc/1/oom_score_adj instead.

<6>[    1.509191] init: command 'loglevel' r=0

<6>[    1.509290] init: command 'export' r=0

<6>[    1.509314] init: command 'export' r=0

<6>[    1.509335] init: command 'export' r=0

<6>[    1.509354] init: command 'export' r=0

<6>[    1.509374] init: command 'export' r=0

<6>[    1.509393] init: command 'export' r=0

<6>[    1.509413] init: command 'export' r=0

<6>[    1.509432] init: command 'export' r=0

<6>[    1.509452] init: command 'export' r=0

<6>[    1.509473] init: command 'export' r=0

<4>[    1.518838] hello:init_nand_libmodule,21

<4>[    1.518856] hello:init_nand_libmodule,22

<4>[    1.518875] [NAND]nand init start, nand0_used_flag is 1

<4>[    1.518890] [NAND] nand IO Merge: 0x2 

<4>[    1.518900] [NAND] turn off log release thread

<4>[    1.518915] [NAND] nand driver version: 0x2, 0x12 0x20130607 14:00

<4>[    1.521298] [NAND]nand get good block ratio  896

<4>[    1.521310] nand good block ratio value is valid 

<4>[    1.521347] Request memory for lsb page table 

<4>[    1.521361] page type: 0

<4>[    1.528929] PHY_PageReadSpare: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[    1.534229] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[    1.542904] [NAND]nandlogrelease_thread init 

<6>[    1.544761]  nanda:

<6>[    1.546777]  nandb: unknown partition table

<6>[    1.548615]  nandc: unknown partition table

<6>[    1.556518]  nandd: unknown partition table

<6>[    1.565309]  nande: unknown partition table

<6>[    1.568082]  nandf: unknown partition table

<6>[    1.569919]  nandg: unknown partition table

<6>[    1.572615]  nandh: unknown partition table

<6>[    1.575343]  nandi: unknown partition table

<6>[    1.578060]  nandj:

<4>[    1.578796] [NAND]nand init end.

<6>[    1.579122] init: command 'insmod' r=0

<6>[    1.579220] init: command 'symlink' r=0

<6>[    1.579271] init: command 'symlink' r=0

<6>[    1.579325] init: command 'symlink' r=0

<6>[    1.579366] init: command 'mkdir' r=0

<6>[    1.579520] init: command 'mount' r=-1

<6>[    1.579561] init: command 'mkdir' r=0

<6>[    1.579639] init: command 'mkdir' r=0

<6>[    1.579725] init: command 'mkdir' r=0

<6>[    1.579791] init: command 'mkdir' r=0

<6>[    1.579871] init: command 'mkdir' r=0

<6>[    1.579941] init: command 'mkdir' r=0

<6>[    1.580006] init: command 'mkdir' r=0

<6>[    1.580073] init: command 'mkdir' r=0

<6>[    1.580137] init: command 'mkdir' r=0

<6>[    1.580296] init: command 'mount' r=0

<6>[    1.580369] init: command 'mkdir' r=0

<6>[    1.580447] init: command 'mkdir' r=0

<6>[    1.580513] init: command 'mkdir' r=0

<6>[    1.580644] init: command 'mount' r=0

<6>[    1.580713] init: command 'mkdir' r=0

<6>[    1.580841] init: command 'mount' r=0

<6>[    1.580996] init: command 'write' r=0

<6>[    1.581128] init: command 'write' r=-2

<6>[    1.581235] init: command 'write' r=0

<6>[    1.581342] init: command 'write' r=-2

<6>[    1.581444] init: command 'write' r=-2

<6>[    1.581546] init: command 'write' r=-2

<6>[    1.581615] init: command 'write' r=0

<6>[    1.581688] init: command 'write' r=0

<6>[    1.581763] init: command 'write' r=0

<6>[    1.581835] init: command 'write' r=0

<6>[    1.581934] init: command 'write' r=0

<6>[    1.582012] init: command 'write' r=0

<6>[    1.582093] init: command 'write' r=0

<6>[    1.582165] init: command 'write' r=0

<6>[    1.582205] init: command 'mkdir' r=0

<6>[    1.623031] init: command 'mount' r=0

<6>[    1.623105] init: command 'chown' r=0

<6>[    1.623276] init: command 'chown' r=0

<6>[    1.623353] init: command 'chmod' r=0

<6>[    1.623406] init: command 'write' r=-22

<6>[    1.623459] init: command 'write' r=0

<6>[    1.623509] init: command 'write' r=0

<6>[    1.623683] init: command 'mkdir' r=0

<6>[    1.623740] init: command 'chown' r=0

<6>[    1.623790] init: command 'chmod' r=0

<6>[    1.623837] init: command 'write' r=0

<6>[    1.623887] init: command 'write' r=0

<6>[    1.623938] init: command 'write' r=0

<6>[    1.624102] init: command 'mkdir' r=0

<6>[    1.624159] init: command 'chown' r=0

<6>[    1.624209] init: command 'chmod' r=0

<6>[    1.624264] init: command 'write' r=0

<6>[    1.624317] init: command 'write' r=0

<6>[    1.624372] init: command 'write' r=0

<6>[    1.624441] init: command 'chmod' r=0

<6>[    1.624463] init: processing action 0x348f8 (init)

<6>[    1.624489] init: command 'export' r=0

<6>[    1.624557] init: command 'mkdir' r=0

<6>[    1.624619] init: command 'symlink' r=0

<6>[    1.624673] init: command 'symlink' r=0

<6>[    1.624740] init: command 'mkdir' r=0

<6>[    1.624804] init: command 'mkdir' r=0

<6>[    1.624926] init: command 'mount' r=0

<6>[    1.624993] init: command 'mkdir' r=0

<6>[    1.625014] init: processing action 0x34a88 (early-fs)

<6>[    1.634444] EXT4-fs (nandd): mounted filesystem with ordered data mode. Opts: (null)

<6>[    1.660712] EXT4-fs (nandh): recovery complete

<6>[    1.664065] EXT4-fs (nandh): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,errors=remount-ro

<6>[    1.692906] usb 3-1: new high-speed USB device number 2 using sw-ehci

<6>[    1.742904] fs_mgr: Running /system/bin/e2fsck on /dev/block/nandh

<6>[    1.842587] EXT4-fs (nandh): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,barrier=1

<6>[    1.848262] EXT4-fs (nandi): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,errors=remount-ro

<6>[    1.902908] fs_mgr: Running /system/bin/e2fsck on /dev/block/nandi

<6>[    1.918136] EXT4-fs (nandi): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,barrier=1

<6>[    1.941952] EXT4-fs (nande): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,errors=remount-ro

<6>[    1.992902] fs_mgr: Running /system/bin/e2fsck on /dev/block/nande

<4>[    2.012880] ====codec_resume_events===

<6>[    2.037002] EXT4-fs (nande): mounted filesystem with ordered data mode. Opts: nomblk_io_submit,barrier=1

<6>[    2.037430] init: command 'mount_all' r=0

<6>[    2.037491] init: command 'setprop' r=0

<6>[    2.214386] [DISP]==disp_module_init==

<6>[    2.215523] [DISP]==disp_probe call==

<6>[    2.215539] [DISP]==disp_probe finish==

<6>[    2.215937] [DISP]capture_module_init

<6>[    2.216788] [DISP]capture_probe

<6>[    2.216969] [DISP]==capture finish==

<6>[    2.216981] [DISP]==disp_module_init finish==

<6>[    2.218633] init: command 'insmod' r=0

<6>[    2.239091] [LCD]==lcd_module_init==

<4>[    2.241026] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/iep/deu/iep_deu.c,line:458:    deu_mode1 not exist.

<4>[    2.241165] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/iep/drc/iep_drc.c,line:565:    lcdgamma4iep for lcd1 not exist.

<6>[    2.252868] [DISP]==Fb_Init==

<6>[    2.270125] [LCD]==lcd_module_init finish==

<6>[    2.270442] init: command 'insmod' r=0

<6>[    2.288978] [HDMI]==hdmi_module_init==

<6>[    2.290099] [HDMI]==hdmi_probe call==

<6>[    2.293192] [DISP]==Fb_Init==

<6>[    2.293206] [HDMI]==hdmi_probe finish==

<6>[    2.293417] [HDMI]==hdmi_module_init finish==

<6>[    2.293632] init: command 'insmod' r=0

<6>[    2.301344] init: command 'insmod' r=0

<6>[    2.308644] init: command 'insmod' r=0

<6>[    2.315836] init: command 'insmod' r=0

<6>[    2.323096] asoc: sndi2s <-> sun6i-i2s.0 mapping ok

<6>[    2.324739] init: command 'insmod' r=0

<6>[    2.331768] init: command 'insmod' r=0

<4>[    2.335164] [LCD] ANX9804 Chip found

<4>[    2.337721] [LCD] ANX9804 clock is stable.

<6>[    2.338938] init: command 'insmod' r=0

<6>[    2.346321] init: command 'insmod' r=0

<6>[    2.353661] asoc: sndpcm <-> sun6i-pcm.0 mapping ok

<6>[    2.355292] init: command 'insmod' r=0

<6>[    2.355347] init: processing action 0x37e30 (console_init)

<3>[    2.356293] init: width = 2048

<3>[    2.359703] init: height = 1536

<3>[    2.363233] init: s.st_size = 12582912

<6>[    2.419991] init: command 'console_init' r=0

<6>[    2.420064] init: processing action 0x2dbc0 (fs)

<6>[    2.420176] init: command 'mount' r=-1

<6>[    2.420201] init: command 'mount' r=-1

<6>[    2.420222] init: command 'mount' r=-1

<6>[    2.420242] init: command 'mount' r=-1

<6>[    2.420260] init: processing action 0x34c90 (fs)

<3>[    2.421666] init: dont need format /dev/block/by-name/UDISK

<6>[    2.427762] init: command 'format_userdata' r=1

<6>[    2.441802] init: command 'mkdir' r=0

<6>[    2.442903] init: command 'chmod' r=-30

<6>[    2.442966] init: command 'chmod' r=-2

<6>[    2.443993] init: command 'chmod' r=-30

<6>[    2.444078] init: command 'chmod' r=-30

<6>[    2.444122] init: command 'chown' r=-30

<6>[    2.444161] init: command 'chown' r=-2

<6>[    2.444203] init: command 'chown' r=-30

<6>[    2.444243] init: command 'chown' r=-30

<4>[    2.549006] create_regulator: axp22_DCDC2: Failed to create debugfs directory

<7>[    2.549616] gpu:open gpu power!

<6>[    2.565157] init: command 'insmod' r=0

<4>[    2.573096] #####: Device 0: Framebuffer physical address: 0x43100000

<6>[    2.573176] init: command 'insmod' r=0

<6>[    2.573393] init: command 'chmod' r=0

<6>[    2.573403] PVR_K:(Error): ############ !psDevInfo->psKernelSGXHostCtlMemInfo [0, ]

<6>[    2.573489] init: command 'chmod' r=0

<6>[    2.581125] init: command 'insmod' r=0

<6>[    2.586574] init: command 'insmod' r=0

<4>[    2.598077] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    2.598108] create_regulator: axp22_ldoio0: Failed to create debugfs directory

<4>[    2.598152] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    2.598179] create_regulator: axp22_ldo10: Failed to create debugfs directory

<4>[    2.773068] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x3c)

<4>[    2.933053] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x21)

<4>[    3.293062] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x21)

<4>[    3.453048] [i2c0] incomplete xfer (status: 0x20, dev addr: 0x3c)

<4>[    3.764509] ehci_irq: highspeed device connect

<6>[    3.794643] init: command 'insmod' r=0

<6>[    3.798892] init: command 'insmod' r=0

<6>[    3.803013] init: command 'insmod' r=0

<6>[    3.810520] init: command 'insmod' r=0

<6>[    3.816780] init: command 'insmod' r=0

<6>[    3.823293] init: command 'insmod' r=0

<6>[    3.831197] init: command 'insmod' r=0

<6>[    3.838776] init: command 'insmod' r=0

<5>[    3.877578] [VFE]Welcome to Video Front End driver

<5>[    3.878238] [VFE]pdev->id = 1

<5>[    3.878251] [VFE]dev->mipi_sel = 1

<5>[    3.878262] [VFE]dev->vip_sel = 1

<5>[    3.878274] [VFE]dev->isp_sel = 0

<4>[    3.894523] [VFE_WARN]fetch front_camera from camera.ini failed,apply default value!

<4>[    3.894565] [VFE_WARN]fetch flicker_type from camera.ini failed,apply default value!

<4>[    3.894581] [VFE_WARN]fetch adaptive_frame_rate from camera.ini failed,apply default value!

<4>[    3.894599] [VFE_WARN]fetch color_denoise_level from camera.ini failed,apply default value!

<4>[    3.894617] [VFE_WARN]fetch defog_value from camera.ini failed,apply default value!

<4>[    3.894632] [VFE_WARN]fetch brightness_tune from camera.ini failed,apply default value!

<4>[    3.894648] [VFE_WARN]fetch gain_delay_frame from camera.ini failed,apply default value!

<4>[    3.895280] [VFE_WARN]fetch csc_coeff_0 from camera.ini failed,apply default value!

<4>[    3.895299] [VFE_WARN]fetch csc_coeff_1 from camera.ini failed,apply default value!

<4>[    3.895314] [VFE_WARN]fetch csc_coeff_2 from camera.ini failed,apply default value!

<4>[    3.895330] [VFE_WARN]fetch csc_coeff_3 from camera.ini failed,apply default value!

<4>[    3.895346] [VFE_WARN]fetch csc_coeff_4 from camera.ini failed,apply default value!

<4>[    3.895361] [VFE_WARN]fetch csc_coeff_5 from camera.ini failed,apply default value!

<5>[    3.905257] [VFE]vip_pin_list addr = 0 

<5>[    3.905275] [VFE]request gpio cnt=18, i=18

<5>[    3.905858] [VFE]vfe_init end

<6>[    3.906334] init: command 'insmod' r=0

<5>[    3.912903] [VFE]probe_work_handle start!

<5>[    3.913653] [VFE]registered sub device,input_num = 0

<5>[    3.914143] [VFE]registered act sub device,input_num = 0

<4>[    3.914204] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    3.914229] create_regulator: axp22_ldoio0: Failed to create debugfs directory

<4>[    3.914256] create_regulator: axp22_ldo9: Failed to create debugfs directory

<5>[    3.914820] [VFE]registered sub device,input_num = 1

<4>[    3.914859] create_regulator: axp22_ldo7: Failed to create debugfs directory

<4>[    3.914883] create_regulator: axp22_ldoio0: Failed to create debugfs directory

<4>[    3.914911] create_regulator: axp22_ldo10: Failed to create debugfs directory

<5>[    3.914929] [VFE]power on and standy on camera 0!

<5>[    3.916208] [VFE]mclk on

<7>[    3.921560] G2D: drv_g2d_init

<6>[    3.921768] G2D: Module initialized.major:245

<6>[    3.921977] init: command 'insmod' r=0

<4>[    3.928256] [VFE_WARN]invalid gpio

<6>[    3.931483] usbcore: registered new interface driver asix

<6>[    3.931541] init: command 'insmod' r=0

<6>[    3.940459] usbcore: registered new interface driver qf9700

<6>[    3.940513] init: command 'insmod' r=0

<6>[    3.948513] usbcore: registered new interface driver MOSCHIP usb-ethernet driver

<6>[    3.948564] init: command 'insmod' r=0

<6>[    3.957624] usbcore: registered new interface driver rtl8150

<6>[    3.957681] init: command 'insmod' r=0

<6>[    3.964268] init: command 'insmod' r=0

<6>[    3.969751] input: sw-keyboard as /devices/virtual/input/input2

<6>[    3.970172] init: command 'insmod' r=0

<6>[    3.970635] init: command 'chmod' r=0

<6>[    3.970925] init: command 'chown' r=0

<6>[    3.971076] init: command 'chmod' r=0

<6>[    3.971145] init: command 'chmod' r=-2

<6>[    3.971233] init: command 'chown' r=0

<6>[    3.971330] init: command 'chown' r=0

<4>[    3.971421] [rfkill]: rfkill set power 1

<4>[    3.971439] [rtl8723au]: rtl8723au is powered down by bt

<4>[    3.971456] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_disable_ehci

<4>[    3.971477] [sw_hci_sun6i]: [sw-ehci1]: remove, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<6>[    3.971509] sw-ehci sw-ehci.1: remove, state 1

<6>[    3.971540] usb usb3: USB disconnect, device number 1

<6>[    3.971556] usb 3-1: USB disconnect, device number 2

<4>[    3.971840] [OV5647]disalbe oe!

<6>[    3.975103] sw-ehci sw-ehci.1: USB bus 3 deregistered

<4>[    3.975132] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power OFF

<4>[    3.975147] [sw_hci_sun6i]: [sw-ehci1]: close clock

<4>[    3.975170] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[    3.975184] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<5>[    3.985572] [VFE]power on and standy on camera 1!

<5>[    3.986833] [VFE]mclk on

<6>[    3.993073] init: command 'write' r=0

<6>[    3.993139] init: command 'chown' r=-2

<6>[    3.993255] init: command 'chown' r=-30

<6>[    3.993329] init: command 'chown' r=-2

<6>[    3.993393] init: command 'setprop' r=0

<4>[    3.998889] [VFE_WARN]invalid gpio

<6>[    4.003630] rtk_btusb: Realtek Bluetooth USB driver ver 1.0.20130524

<4>[    4.003646] Registering file operations for btfcd driver

<4>[    4.004196] Class driver initialized successfully

<6>[    4.004450] usbcore: registered new interface driver rtk_btusb

<6>[    4.004508] init: command 'insmod' r=0

<6>[    4.004566] rtk_btusb: btfcd open

<6>[    4.004572] 

<3>[    4.004581] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.009563] rtk_btusb: btfcd open

<6>[    4.009568] 

<3>[    4.009577] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.014570] init: command 'chmod' r=-1

<6>[    4.014606] rtk_btusb: btfcd open

<6>[    4.014612] 

<3>[    4.014621] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.019578] rtk_btusb: btfcd open

<6>[    4.019583] 

<3>[    4.019593] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[    4.024812] init: command 'chown' r=-1

<6>[    4.024839] init: processing action 0x2dca8 (post-fs)

<6>[    4.024943] init: command 'mount' r=0

<6>[    4.024985] init: command 'mount' r=0

<6>[    4.025126] init: command 'chown' r=0

<6>[    4.025185] init: command 'chmod' r=0

<6>[    4.025206] init: command 'restorecon' r=0

<6>[    4.026291] init: command 'chown' r=0

<6>[    4.026352] init: command 'chmod' r=0

<6>[    4.026372] init: command 'restorecon' r=0

<6>[    4.026484] init: command 'chown' r=0

<6>[    4.026557] init: command 'chmod' r=0

<6>[    4.026631] init: command 'chown' r=0

<6>[    4.026702] init: command 'chmod' r=0

<6>[    4.026779] init: command 'chown' r=0

<6>[    4.026848] init: command 'chmod' r=0

<6>[    4.026920] init: command 'chown' r=0

<6>[    4.026989] init: command 'chmod' r=0

<6>[    4.027062] init: command 'chown' r=-2

<6>[    4.027119] init: command 'chmod' r=-2

<6>[    4.027250] init: command 'mkdir' r=0

<6>[    4.027293] init: processing action 0x2dfd8 (post-fs-data)

<6>[    4.027370] init: command 'chown' r=0

<6>[    4.027426] init: command 'chmod' r=0

<6>[    4.027445] init: command 'restorecon' r=0

<6>[    4.027577] init: command 'mkdir' r=0

<6>[    4.027617] init: command 'copy' r=-1

<6>[    4.028627] init: command 'chown' r=-2

<6>[    4.028667] init: command 'chmod' r=-2

<6>[    4.028705] init: command 'copy' r=-1

<6>[    4.028761] init: command 'chown' r=-2

<6>[    4.028798] init: command 'chmod' r=-2

<6>[    4.028837] init: command 'write' r=-2

<6>[    4.028944] init: command 'mkdir' r=0

<6>[    4.029101] init: command 'mkdir' r=0

<6>[    4.029223] init: command 'mkdir' r=0

<6>[    4.029367] init: command 'mkdir' r=0

<6>[    4.029487] init: command 'mkdir' r=0

<6>[    4.029615] init: command 'mkdir' r=0

<6>[    4.029746] init: command 'mkdir' r=0

<6>[    4.029865] init: command 'mkdir' r=0

<6>[    4.029985] init: command 'mkdir' r=0

<6>[    4.030956] init: command 'chmod' r=0

<6>[    4.031020] init: command 'chown' r=0

<6>[    4.031149] init: command 'mkdir' r=0

<6>[    4.031269] init: command 'mkdir' r=0

<6>[    4.031326] init: command 'chown' r=0

<6>[    4.032335] init: command 'mkdir' r=0

<6>[    4.032456] init: command 'mkdir' r=0

<6>[    4.033445] init: command 'mkdir' r=0

<6>[    4.034448] init: command 'mkdir' r=0

<6>[    4.034566] init: command 'mkdir' r=0

<6>[    4.036413] init: command 'mkdir' r=0

<6>[    4.036534] init: command 'mkdir' r=0

<4>[    4.042258] [CSI][GC2035]disalbe oe!

<6>[    4.042910] usb 1-1: new high-speed USB device number 2 using sw-ehci

<6>[    4.043679] init: command 'mkdir' r=0

<6>[    4.043798] init: command 'mkdir' r=0

<6>[    4.044829] init: command 'mkdir' r=0

<6>[    4.045833] init: command 'mkdir' r=0

<6>[    4.045952] init: command 'mkdir' r=0

<6>[    4.046968] init: command 'mkdir' r=0

<6>[    4.047025] init: command 'chown' r=0

<6>[    4.047079] init: command 'chmod' r=0

<6>[    4.047199] init: command 'mkdir' r=0

<6>[    4.047320] init: command 'mkdir' r=0

<6>[    4.047341] init: processing action 0x32288 (post-fs-data)

<6>[    4.047546] init: command 'chown' r=0

<6>[    4.047662] init: command 'chmod' r=0

<6>[    4.047767] init: command 'chown' r=0

<6>[    4.047854] init: command 'chmod' r=0

<6>[    4.047874] init: processing action 0x34c60 (post-fs-data)

<6>[    4.047895] init: processing action 0x37e78 (property_service_init)

<5>[    4.052870] [VFE]mclk off

<5>[    4.053349] [VFE]V4L2 device registered as video1

<5>[    4.053385] [VFE]register_early_suspend @ probe handle!

<5>[    4.053398] [VFE]probe_work_handle end!

<6>[    4.063099] init: Created socket '/dev/socket/property_service' with mode '666', user '0', group '0'

<6>[    4.063140] init: command 'property_service_init' r=0

<6>[    4.063174] init: processing action 0x37ec0 (signal_init)

<6>[    4.063254] init: command 'signal_init' r=0

<6>[    4.063292] init: processing action 0x37f08 (check_startup)

<6>[    4.063355] init: command 'check_startup' r=0

<6>[    4.063377] init: processing action 0x2e768 (boot)

<6>[    4.064300] init: command 'ifup' r=0

<6>[    4.064432] init: command 'hostname' r=0

<6>[    4.064515] init: command 'domainname' r=0

<6>[    4.064544] init: command 'setrlimit' r=0

<6>[    4.064629] init: command 'write' r=0

<6>[    4.064705] init: command 'write' r=0

<6>[    4.064846] init: command 'chown' r=0

<6>[    4.064908] init: command 'chmod' r=0

<6>[    4.064980] init: command 'chown' r=0

<6>[    4.065042] init: command 'chmod' r=0

<6>[    4.065125] init: command 'write' r=0

<6>[    4.065197] init: command 'write' r=0

<6>[    4.065256] init: command 'chown' r=-2

<6>[    4.065310] init: command 'chown' r=-2

<6>[    4.065364] init: command 'chown' r=-2

<6>[    4.065418] init: command 'chown' r=-2

<6>[    4.065472] init: command 'chown' r=-2

<6>[    4.065546] init: command 'chown' r=-2

<6>[    4.065613] init: command 'chown' r=0

<6>[    4.065677] init: command 'chown' r=0

<6>[    4.065750] init: command 'chown' r=0

<6>[    4.065816] init: command 'chown' r=0

<6>[    4.065872] init: command 'chmod' r=0

<6>[    4.065926] init: command 'chmod' r=0

<6>[    4.065980] init: command 'chmod' r=0

<6>[    4.066065] init: command 'chown' r=-2

<6>[    4.066139] init: command 'chmod' r=-2

<6>[    4.066212] init: command 'chown' r=-2

<6>[    4.066284] init: command 'chmod' r=-2

<6>[    4.066358] init: command 'chown' r=-2

<6>[    4.066430] init: command 'chmod' r=-2

<6>[    4.066503] init: command 'chown' r=-2

<6>[    4.066577] init: command 'chmod' r=-2

<6>[    4.066649] init: command 'chown' r=-2

<6>[    4.066721] init: command 'chmod' r=-2

<6>[    4.066793] init: command 'chown' r=-2

<6>[    4.066864] init: command 'chmod' r=-2

<6>[    4.066938] init: command 'chown' r=-2

<6>[    4.067011] init: command 'chown' r=-2

<6>[    4.067084] init: command 'chmod' r=-2

<6>[    4.067160] init: command 'chown' r=-2

<6>[    4.067234] init: command 'chmod' r=-2

<6>[    4.067318] init: command 'chown' r=0

<6>[    4.067383] init: command 'chmod' r=0

<6>[    4.067459] init: command 'chown' r=0

<6>[    4.067524] init: command 'chmod' r=0

<6>[    4.067619] init: command 'chown' r=0

<6>[    4.067685] init: command 'chmod' r=0

<6>[    4.067764] init: command 'chown' r=0

<6>[    4.067830] init: command 'chmod' r=0

<6>[    4.067906] init: command 'chown' r=0

<6>[    4.067972] init: command 'chmod' r=0

<6>[    4.068043] init: command 'chown' r=-2

<6>[    4.068106] init: command 'chown' r=-2

<6>[    4.068165] init: command 'chown' r=-2

<6>[    4.068224] init: command 'chown' r=-2

<6>[    4.068284] init: command 'chown' r=-2

<6>[    4.068343] init: command 'chown' r=-2

<6>[    4.068402] init: command 'chown' r=-2

<6>[    4.068462] init: command 'chown' r=-2

<6>[    4.068521] init: command 'chown' r=-2

<6>[    4.068579] init: command 'chown' r=-2

<6>[    4.068639] init: command 'chown' r=-2

<6>[    4.068698] init: command 'chown' r=-2

<6>[    4.068759] init: command 'chown' r=-2

<6>[    4.068820] init: command 'chown' r=-2

<6>[    4.068880] init: command 'chown' r=-2

<6>[    4.068940] init: command 'chown' r=-2

<6>[    4.068999] init: command 'chown' r=-2

<6>[    4.069064] init: command 'chown' r=-2

<6>[    4.069127] init: command 'chown' r=-2

<6>[    4.069207] init: command 'chown' r=0

<6>[    4.069275] init: command 'chown' r=0

<6>[    4.069344] init: command 'chown' r=0

<6>[    4.069412] init: command 'chown' r=0

<6>[    4.069479] init: command 'chown' r=0

<6>[    4.069546] init: command 'chown' r=0

<6>[    4.069640] init: command 'chown' r=0

<6>[    4.069747] init: command 'chmod' r=-30

<6>[    4.069828] init: command 'setprop' r=0

<6>[    4.069898] init: command 'setprop' r=0

<6>[    4.069967] init: command 'setprop' r=0

<6>[    4.070035] init: command 'setprop' r=0

<6>[    4.070103] init: command 'setprop' r=0

<6>[    4.070171] init: command 'setprop' r=0

<6>[    4.070240] init: command 'setprop' r=0

<6>[    4.070309] init: command 'setprop' r=0

<6>[    4.070377] init: command 'setprop' r=0

<6>[    4.070455] init: command 'setprop' r=0

<6>[    4.070524] init: command 'setprop' r=0

<6>[    4.070563] init: command 'setprop' r=0

<5>[    4.070637] init: starting 'servicemanager'

<5>[    4.071086] init: starting 'vold'

<6>[    4.071779] init: Created socket '/dev/socket/vold' with mode '660', user '0', group '1009'

<5>[    4.072552] init: starting 'pvrsrvctl'

<6>[    4.072984] init: command 'class_start' r=0

<5>[    4.073099] init: starting 'netd'

<5>[    4.073480] init: starting 'debuggerd'

<6>[    4.073767] init: Created socket '/dev/socket/mdns' with mode '660', user '0', group '1000'

<5>[    4.073799] init: starting 'updatesoftwinner'

<6>[    4.073928] init: Created socket '/dev/socket/dnsproxyd' with mode '660', user '0', group '3003'

<6>[    4.074058] init: Created socket '/dev/socket/netd' with mode '660', user '0', group '1000'

<5>[    4.074174] init: starting 'surfaceflinger'

<5>[    4.074587] init: starting 'zygote'

<5>[    4.075011] init: starting 'drm'

<6>[    4.075346] init: Created socket '/dev/socket/zygote' with mode '660', user '0', group '1000'

<5>[    4.075424] init: starting 'media'

<5>[    4.075819] init: starting 'installd'

<3>[    4.076190] init: cannot find '/system/etc/install-recovery.sh', disabling 'flash_recovery'

<6>[    4.076977] init: Created socket '/dev/socket/installd' with mode '600', user '1000', group '1000'

<5>[    4.085619] init: starting 'keystore'

<5>[    4.086079] init: starting 'ril-daemon'

<6>[    4.086371] init: Created socket '/dev/socket/keystore' with mode '666', user '0', group '0'

<5>[    4.086485] init: starting 'u3gmonitor'

<6>[    4.086784] init: Created socket '/dev/socket/rild-debug' with mode '660', user '1001', group '1000'

<5>[    4.086873] init: starting 'ttyusb-scan'

<6>[    4.086924] init: Created socket '/dev/socket/rild' with mode '660', user '0', group '1001'

<6>[    4.087202] init: command 'class_start' r=0

<6>[    4.087270] init: processing action 0x379d8 (boot)

<6>[    4.087368] init: command 'chmod' r=0

<6>[    4.087464] init: command 'chown' r=0

<6>[    4.087535] init: command 'chown' r=0

<6>[    4.087611] init: command 'chown' r=0

<6>[    4.087688] init: command 'chown' r=0

<6>[    4.087756] init: command 'chown' r=0

<6>[    4.087826] init: command 'chown' r=0

<6>[    4.087894] init: command 'chown' r=0

<6>[    4.087965] init: command 'chown' r=0

<6>[    4.088053] init: command 'chown' r=-2

<6>[    4.088116] init: command 'chown' r=0

<6>[    4.088173] init: command 'chmod' r=0

<6>[    4.088230] init: command 'chmod' r=0

<6>[    4.088287] init: command 'chmod' r=0

<6>[    4.088357] init: command 'chmod' r=0

<6>[    4.088442] init: command 'chmod' r=0

<6>[    4.088528] init: command 'chmod' r=0

<6>[    4.088603] init: command 'chmod' r=0

<6>[    4.088674] init: command 'chmod' r=0

<6>[    4.088764] init: command 'chmod' r=-2

<6>[    4.088836] init: command 'chmod' r=0

<4>[    4.123897] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6a)

<6>[    4.132996] init: command 'chown' r=0

<4>[    4.143089] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6a)

<4>[    4.163112] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6b)

<4>[    4.183110] [i2c2] incomplete xfer (status: 0x20, dev addr: 0x6b)

<6>[    4.183124] init: command 'chmod' r=0

<6>[    4.183179] init: processing action 0x37f50 (queue_property_triggers)

<6>[    4.183289] init: command 'queue_property_triggers' r=0

<6>[    4.183313] init: processing action 0x2f5f8 (nonencrypted)

<6>[    4.183339] init: command 'class_start' r=0

<6>[    4.183360] init: processing action 0x2fa98 (property:ro.debuggable=1)

<5>[    4.183487] init: starting 'console'

<6>[    4.183889] init: command 'start' r=0

<6>[    4.183919] init: processing action 0x32c80 (property:persist.sys.usb.config=*)

<6>[    4.184011] init: command 'setprop' r=0

<6>[    4.184116] init: command 'setprop' r=0

<6>[    4.184142] init: processing action 0x32358 (property:sys.usb.config=none)

<6>[    4.184199] init: command 'stop' r=0

<6>[    4.184369] init: command 'write' r=0

<6>[    4.184483] init: command 'write' r=0

<6>[    4.184547] init: command 'setprop' r=0

<6>[    4.184570] init: processing action 0x368f8 (property:sys.usb.config=mass_storage,adb)

<6>[    4.184672] init: command 'write' r=0

<6>[    4.184803] init: command 'write' r=0

<6>[    4.184935] init: command 'write' r=0

<6>[    4.185062] init: command 'write' r=0

<6>[    4.185167] init: command 'write' r=0

<5>[    4.185205] init: starting 'adbd'

<6>[    4.185585] init: command 'start' r=0

<6>[    4.185660] init: command 'setprop' r=0

<6>[    4.186127] init: Created socket '/dev/socket/adbd' with mode '660', user '1000', group '1000'

<6>[    4.187884] adb_open

<4>[    4.187918] ep_matches, wrn: endpoint already claimed, ep(0xc07fdf64, 0xeeaeac80, ep1-bulk)

<6>[    4.188000] adb_bind_config

<4>[    4.188019] ep_matches, wrn: endpoint already claimed, ep(0xc07fdf64, 0xeeaeac80, ep1-bulk)

<4>[    4.188037] ep_matches, wrn: endpoint already claimed, ep(0xc07fdfb0, 0xeeaeac80, ep2-bulk)

<4>[    4.188056] ep_matches, wrn: endpoint already claimed, ep(0xc07fdf64, 0xeeaeac80, ep1-bulk)

<4>[    4.188073] ep_matches, wrn: endpoint already claimed, ep(0xc07fdfb0, 0xeeaeac80, ep2-bulk)

<4>[    4.188090] ep_matches, wrn: endpoint already claimed, ep(0xc07fdffc, 0xeeaebe00, ep3-bulk)

<4>[    4.188112] [sw_udc]: alloc request: ep(0xc07fe048, ep4-bulk, 512), req(0xee331a40)

<4>[    4.188129] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xedc93c40)

<4>[    4.188148] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xef29dec0)

<4>[    4.188166] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xedc937c0)

<4>[    4.188192] [sw_udc]: alloc request: ep(0xc07fdffc, ep3-bulk, 512), req(0xedebacc0)

<4>[    4.188216] [sw_udc]: sw_udc_pullup, is_on = 1

<4>[    4.188228] [sun6i_usb]: usb device is not active

<6>[    4.196660] cdc_acm 1-1:1.1: ttyACM0: USB ACM device

<6>[    4.276367] init: waitpid returned pid 1294, status = 00000000

<5>[    4.276398] init: process 'pvrsrvctl', pid 1294 exited

<5>[    4.811236] init: starting 'bootanim'

<4>[    4.811287] [DISP WRN] file:drivers/video/sun6i/disp/de_bsp/de/disp_layer.c,line:363:    all layer resource used!

<4>[    5.073457] [sun6i_usb]: set ctrl gpio off

<6>[    6.358884] init: waitpid returned pid 1734, status = 00000000

<3>[    6.358920] init: untracked pid 1734 exited

<6>[    9.089451] warning: `zygote' uses 32-bit capabilities (legacy support in use)

<6>[    9.211004] gsensor_detect: addr= 1c

<4>[    9.211406] gsensor_detect: mma8452 equipment is detected!

<6>[    9.213066] mma8452 2-001d: build time Nov  4 2013 19:17:35

<6>[    9.213830] input: mma8452 as /devices/virtual/input/input3

<4>[    9.283201] i2c-core: driver [gslX680] using legacy suspend method

<4>[    9.283221] i2c-core: driver [gslX680] using legacy resume method

<6>[    9.284521] input: gslX680 as /devices/platform/sun6i-i2c.1/i2c-1/1-0040/input/input4

<6>[    9.285893] init: processing action 0x2fcd0 (property:sys.sensors=1)

<5>[    9.286029] init: starting 'sensors'

<6>[    9.286435] init: command 'start' r=0

<6>[    9.349036] init: waitpid returned pid 2053, status = 00000a00

<5>[    9.349067] init: process 'sensors', pid 2053 exited

<4>[   11.133284] [sun6i_usb]: set ctrl gpio on

<6>[   15.194345] request_suspend_state: wakeup (3->0) at 15181488593 (2014-01-14 05:37:51.315174966 UTC)

<6>[   17.442995] EXT4-fs (dm-0): mounted filesystem without journal. Opts: (null)

<6>[   17.537984] EXT4-fs (dm-0): re-mounted. Opts: (null)

<6>[   17.544306] EXT4-fs (dm-0): re-mounted. Opts: (null)

<6>[   17.971589] acc_open

<6>[   17.971622] acc_release

<4>[   18.737449] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<4>[   19.106730] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<4>[   19.116079] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<6>[   21.094156] EXT4-fs (dm-1): mounted filesystem without journal. Opts: (null)

<6>[   21.804819] EXT4-fs (dm-1): re-mounted. Opts: (null)

<4>[   21.832060] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

<6>[   21.837249] EXT4-fs (dm-1): re-mounted. Opts: (null)

<6>[   22.035528] EXT4-fs (dm-2): mounted filesystem without journal. Opts: (null)

<6>[   22.115359] EXT4-fs (dm-2): re-mounted. Opts: (null)

<6>[   22.129050] EXT4-fs (dm-2): re-mounted. Opts: (null)

<4>[   22.208927] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<4>[   22.290650] vmap allocation for size 23597056 failed: use vmalloc=<size> to increase size.

<4>[   25.425835] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<4>[   25.551148] vmap allocation for size 11800576 failed: use vmalloc=<size> to increase size.

<6>[   25.724311] init: processing action 0x312c0 (property:sys.boot_completed=1)

<5>[   25.724620] init: starting 'preinstall'

<6>[   25.726206] init: command 'start' r=0

<6>[   26.166852] init: waitpid returned pid 2992, status = 00000000

<5>[   26.166891] init: process 'preinstall', pid 2992 exited

<3>[   26.173742] init: sys_prop: permission denied uid:1003  name:service.bootanim.exit

<4>[   26.306989] [rfkill]: rfkill set power 1

<4>[   26.307018] [rtl8723au]: rtl8723au is powered down by bt

<4>[   26.307034] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<6>[   26.324516] init: waitpid returned pid 1836, status = 00000000

<5>[   26.324609] init: process 'bootanim', pid 1836 exited

<4>[   26.330137] [rfkill]: rfkill set power 0

<4>[   26.330239] [rtl8723au]: rtl8723au is powered up by bt

<4>[   26.330304] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_enable_ehci

<4>[   26.330364] [sw_hci_sun6i]: [sw-ehci1]: probe, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<4>[   26.330434] [sw_hci_sun6i]: [sw-ehci1]: open clock

<4>[   26.330740] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power ON

<6>[   26.330791] sw-ehci sw-ehci.1: SW USB2.0 'Enhanced' Host Controller (EHCI) Driver

<6>[   26.331025] sw-ehci sw-ehci.1: new USB bus registered, assigned bus number 3

<6>[   26.331791] sw-ehci sw-ehci.1: irq 104, io mem 0xf1c1a000

<6>[   26.343004] sw-ehci sw-ehci.1: USB 0.0 started, EHCI 1.00

<4>[   26.343034] ehci_irq: highspeed device connect

<6>[   26.357885] hub 3-0:1.0: USB hub found

<6>[   26.358085] hub 3-0:1.0: 1 port detected

<4>[   26.361300] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[   26.361324] [rtl8723au]: rtl8723au power state change: wifi 0, bt 1 !!

<6>[   26.574557] rtk_btusb: btfcd open

<6>[   26.574595] 

<3>[   26.574639] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[   26.673011] usb 3-1: new high-speed USB device number 2 using sw-ehci

<6>[   26.780084] rtk_btusb: btfcd open

<6>[   26.780098] 

<3>[   26.780114] rtk_btusb: hci_dev_get Ghdev==NULL

<6>[   26.829391] rtk_btusb: btusb_probe 1==========can_wakeup=1	 flag2=0

<6>[   26.829413] rtk_btusb: patch_add

<6>[   26.829453] rtk_btusb: hci_register_dev ec01f400 name  bus 1

<6>[   26.829467] rtk_btusb: id=0 

<6>[   26.829480] rtk_btusb: hdev->name=hci0 

<3>[   26.829490] rtk_btusb:  ===================hci_register_dev success

<6>[   26.985247] rtk_btusb: btfcd open

<6>[   26.985256] 

<6>[   26.985279] rtk_btusb: btusb_open start pm_usage_cnt(0x0)

<6>[   26.985293] rtk_btusb: download_patch start

<6>[   26.987419] rtk_btusb: check_fw_version : read_ver_rsp->lmp_subver = 0x1200

<6>[   26.987437] rtk_btusb: load_firmware

<6>[   27.725284] rtk_btusb: check_fw_version : read_ver_rsp->lmp_subver = 0x963e

<6>[   27.725406] rtk_btusb: Rtk patch end 0

<6>[   27.725777] rtk_btusb: btusb_open end  pm_usage_cnt(0x0)

<6>[   28.222396] rtk_btusb: btfcd close

<6>[   28.222413] 

<6>[   28.222453] rtk_btusb: btusb_flush add delay 

<6>[   28.257523] rtk_btusb: btusb_close

<4>[   28.289880] [rfkill]: rfkill set power 1

<4>[   28.289915] [rtl8723au]: rtl8723au is powered down by bt

<4>[   28.289938] [sw_hci_sun6i]: [sw-ehci1]: sw_usb_disable_ehci

<4>[   28.289967] [sw_hci_sun6i]: [sw-ehci1]: remove, pdev->name: sw-ehci, pdev->id: 1, sw_ehci: 0xc08924cc

<6>[   28.290014] sw-ehci sw-ehci.1: remove, state 1

<6>[   28.290059] usb usb3: USB disconnect, device number 1

<6>[   28.290080] usb 3-1: USB disconnect, device number 2

<6>[   28.290467] rtk_btusb: btusb_disconnect

<6>[   28.290482] rtk_btusb: patch_remove

<6>[   28.290503] rtk_btusb: hci_unregister_dev hdevec01f400 name hci0 bus 1

<6>[   28.290527] rtk_btusb: btusb_flush add delay 

<6>[   28.338963] sw-ehci sw-ehci.1: USB bus 3 deregistered

<4>[   28.339012] [sw_hci_sun6i]: [sw-ehci1]: Set USB Power OFF

<4>[   28.339030] [sw_hci_sun6i]: [sw-ehci1]: close clock

<4>[   28.339060] [sw_hci_sun6i]: ERR: sw_ohci is null

<4>[   28.339218] [rtl8723au]: rtl8723au power state change: wifi 0, bt 0 !!

<6>[   28.840551] init: waitpid returned pid 3098, status = 00000000

<3>[   28.840781] init: untracked pid 3098 exited

<4>[   32.241335] PHY_PageRead: ecc limit, 0x0, 0x0, 0xa, 0x0

<5>[   42.190878] CPU1: shutdown

<6>[   42.190997] [hotplug]: cpu(2) try to kill cpu(1)

<6>[   42.204225] [hotplug]: cpu1 is killed! .

<5>[   42.217895] CPU2: shutdown

<6>[   42.218017] [hotplug]: cpu(3) try to kill cpu(2)

<6>[   42.234277] [hotplug]: cpu2 is killed! .

<4>[   44.613966] CPU1: Booted secondary processor

<6>[   44.614030] Calibrating delay loop (skipped) already calibrated this CPUCPU2: Booted secondary processor

<6>[   44.636338] Calibrating delay loop (skipped) already calibrated this CPU

<5>[   45.810518] CPU2: shutdown

<6>[   45.810640] [hotplug]: cpu(3) try to kill cpu(2)

<6>[   45.824240] [hotplug]: cpu2 is killed! .

<5>[   45.836779] CPU3: shutdown

<6>[   45.836902] [hotplug]: cpu(0) try to kill cpu(3)

<6>[   45.854405] [hotplug]: cpu3 is killed! .

<4>[   46.663112] [sun6i_usb]: 

<4>[   46.663164] 

<4>[   46.663193] insmod_device_driver

<4>[   46.663229] 

<4>[   46.663318] [sw_udc]: sw_usb_device_enable start

<4>[   46.663419] [sw_udc]: usb_vbase  = 0xf1c19000

<4>[   46.663514] [sw_udc]: sram_vbase = 0xf1c00000

<4>[   46.663801] [sw_udc]: open_usb_clock

<4>[   46.664186] [sw_udc]: usbd_stop_work

<4>[   46.664332] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_1 dma_hdle[1] = 0xc0831108

<4>[   46.664488] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_2 dma_hdle[2] = 0xc083118c

<4>[   46.664641] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_3 dma_hdle[3] = 0xc0831210

<4>[   46.664796] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_4 dma_hdle[4] = 0xc0831294

<4>[   46.664951] [sun6i_usb]: line:539 sw_udc_dma_probe name:sw_usb_udc_dma_5 dma_hdle[5] = 0xc0831318

<4>[   46.665252] [sw_udc]: CONFIG_USB_GADGET_DUALSPEED: USBC_TS_MODE_HS

<4>[   46.665361] [sw_udc]: usbd_start_work

<4>[   46.665443] [sw_udc]: usbd_start_work

<4>[   46.665524] [sw_udc]: sw_usb_device_enable end

<4>[   46.720911] [sw_udc]: IRQ: suspend

<4>[   46.720992] [sw_udc]: ERR: usb speed is unkown

<4>[   47.537121] [sw_udc]: IRQ: reset

<4>[   47.537233] (1:star,2:end): vfs_read:0, vfs_write:0,dma_working:0,amount:0,file_offset:0

<4>[   47.537342] [sw_udc]: irq: reset happen, throw away all urb

<4>[   47.629306] [sw_udc]: 

<4>[   47.629349] +++++++++++++++++++++++++++++++++++++

<4>[   47.629437] [sw_udc]:  usb enter high speed.

<4>[   47.629507] [sw_udc]: 

<4>[   47.629538] +++++++++++++++++++++++++++++++++++++

<4>[   47.634757] [sw_udc]: IRQ: reset

<4>[   47.634790] (1:star,2:end): vfs_read:0, vfs_write:0,dma_working:0,amount:0,file_offset:0

<4>[   47.634824] [sw_udc]: irq: reset happen, throw away all urb

<6>[   47.638581] android_work: sent uevent USB_STATE=CONNECTED

<4>[   47.660557] [sw_udc]: Set address 2

<6>[   47.750618] android_usb gadget: high-speed config #1: android

<4>[   47.750664] [sw_udc]: ep enable: ep3(0xc07fdffc, ep3-bulk, 128, 512)

<4>[   47.750682] [sw_udc]: ep enable: ep1(0xc07fdf64, ep1-bulk, 128, 512)

<4>[   47.750695] [sw_udc]: ep enable: ep4(0xc07fe048, ep4-bulk, 0, 512)

<4>[   47.750716] [sw_udc]: ep enable: ep2(0xc07fdfb0, ep2-bulk, 0, 512)

<4>[   47.750741] [sw_udc]: alloc request: ep(0xc07fdf64, ep1-bulk, 512), req(0xecc487c0)

<4>[   47.750761] [sw_udc]: alloc request: ep(0xc07fdfb0, ep2-bulk, 512), req(0xec1ecd40)

<4>[   47.750783] [sw_udc]: alloc request: ep(0xc07fdf64, ep1-bulk, 512), req(0xec33a8c0)

<4>[   47.750802] [sw_udc]: alloc request: ep(0xc07fdfb0, ep2-bulk, 512), req(0xeda491c0)

<6>[   47.751503] android_work: sent uevent USB_STATE=CONFIGURED

<4>[   47.957684] [sun6i_usb]: nuke: ep num is 0

<6>[   77.468282] EXT4-fs (nandd): re-mounted. Opts: (null)

<4>[   80.533477] PHY_PageRead: ecc limit, 0xa, 0x0, 0x0, 0x0

